MODEL-SPECIFIC REGISTERS	Release 60		Last change 03jan99
Copyright (c) 1996,1997,1998,1999 Ralf Brown

--------!---Note-----------------------------
Note:	except where mentioned otherwise, Pentium information also applies to
	  the PentiumMMX, and Pentium Pro information also applies to the
	  Pentium II
----------S00000000--------------------------
MSR 00000000h - Pentium, Pentium Pro - MACHINE CHECK EXCEPTION ADDRESS
Size:	32-36 bits
Access:	Read
Desc:	on any Machine Check exception (INT 12), this MSR contains the physical
	  address at which the exception occurred
Notes:	also supported by AMD Am5k86, K5, and K6; however, the K6 does not
	  actually support the machine check -- this register may be written
	  on the K6 to emulate that functionality
	this register does not exist on the PentiumII, but will not cause an
	  exception when accessed
SeeAlso: MSR 00000001h,MSR 80000000h,INT 12"MACHINE CHECK"
----------S00000001--------------------------
MSR 00000001h - Pentium, Pentium Pro - MACHINE CHECK EXCEPTION TYPE
Size:	6 bits
Access:	Read
Desc:	when a Machine Check exception occurs, this register contains the
	  reason for the exception
Notes:	also supported by AMD Am5k86, K5, and K6; however, the K6 does not
	  actually support the machine check -- this register may be written
	  on the K6 to emulate that functionality
	this register does not exist on the PentiumII, but will not cause an
	  exception when accessed
SeeAlso: MSR 00000000h,MSR 80000001h,INT 12"MACHINE CHECK"

Bitfields for Machine Check Exception type (MSR 00000001h):
Bit(s)	Description	(Table R0001)
 63-6	reserved (0)
 5	"FERI" Fan Error Indicator (Pentium OverDrive only) -- CPU overheated
	(once set, this bit remains set even through CPU reset)
 4	bus cycle causing exception was locked
 3	state of M/IO# pin during bus cycle
 2	state of D/C# pin during bus cycle
 1	state of W/R# pin during bus cycle
 0	Machine Check pending (cleared by reading this MSR)
----------S00000002--------------------------
MSR 00000002h - Pentium - (TR1) PARITY REVERSAL TEST REGISTER
Size:	14 bits
Access:	Write
SeeAlso: MSR 00000004h,MSR 80000002h

Bitfields for Parity Reversal Test Register (TR1):
Bit(s)	Description	(Table R0002)
 63-14	reserved (0)
 13	microcode
 12	Data TLB data
 11	Data TLB tag
 10	Data Cache data
 9	Data Cache tag
 8	Code TLB data
 7	Code TLB tag
 6	"ID3" data cache odd bits 129-255
 5	"ID2" data cache even bits 128-254
 4	"ID1" data cache odd bits 1-127
 3	"ID0" data cache even bits 0-126
 2	instruction cache tag
 1	do not go into SHUTDOWN mode on parity error
 0	(read/write-clear) "Parity Error Summary" set on any parity error
Notes:	bits 2-13 indicate that the parity should be reversed for the given
	  subsystem, thus always forcing a parity error
	the Centaur (IDT) WinChip C6 supports bit 1 (no shutdown)
----------S00000003--------------------------
MSR 00000003h - Pentium - INVALID
Note:	attempted accesses to this MSR cause an exception
SeeAlso: MSR 80000003h,MSR 0000000Fh
----------S00000003--------------------------
MSR 00000003h - Cyrix M2 - TEST DATA
SeeAlso: MSR 00000004h"Cyrix"
----------S00000004--------------------------
MSR 00000004h - Pentium - (TR2) INSTRUCTION CACHE END BITS
Size:	4 bits
Access:	Read/Write
Note:	documented as reserved on Pentium MMX
SeeAlso: MSR 00000002h,MSR 00000005h,MSR 80000004h

Bitfields for Instruction Cache End Bits (TR2):
Bit(s)	Description	(Table R0003)
 63-4	reserved (0)
 3-0	end bits (each set bit indicates the last byte of an instruction in
	  TR3 during code cache access)
Note:	when a new line is written into the code cache, all end bits are set;
	  the instruction decoder then clears those bits corresponding to
	  bytes which are not the last byte of an instruction
SeeAlso: #R0004
----------S00000004--------------------------
MSR 00000004h - Cyrix M2 - TEST ADDRESS
SeeAlso: MSR 00000003h"Cyrix",MSR 00000005h"Cyrix"
----------S00000005--------------------------
MSR 00000005h - Pentium - (TR3) CACHE DATA TEST REGISTER
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000004h,MSR 00000006h,MSR 80000005h

Bitfields for Cache Data Test Register (TR3):
Bit(s)	Description	(Table R0004)
 63-32	reserved (0)
 31-0	data read/written from/to cache (code or data)
SeeAlso: #R0005
----------S00000005--------------------------
MSR 00000005h - Cyrix M2 - COMMAND/STATUS
SeeAlso: MSR 00000004h"Cyrix"
----------S00000006--------------------------
MSR 00000006h - Pentium - (TR4) CACHE TAG
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000005h,MSR 00000007h,MSR 80000006h

Bitfields for Cache Tag Test Register (TR4):
Bit(s)	Description	(Table R0005)
 63-32	reserved (0)
 31-8	cache tag (bits 35-12 of address)
 7-3	reserved (0)
 2	LRU (P54C)
	=0  Way 0
	=1  Way 1
 4-2	LRU (P55C [PentiumMMX])
	=X00  Way 0
	=X10  Way 1
	=0X1  Way 2
	=1X1  Way 3
 1-0	Valid
	---code cache (selected by TR5)---
	x0 cache line invalid
	x1 cache line valid
	---data cache (selected by TR5)---
	00 cache line invalid
	01 cache line shared
	10 cache line exclusive
	11 cache line modified
SeeAlso: #R0004,#R0006
----------S00000007--------------------------
MSR 00000007h - Pentium - (TR5) CACHE CONTROL
Size:	15 bits
Access:	Write
SeeAlso: MSR 00000006h,MSR 00000008h,MSR 80000007h

Bitfields for Cache Control Test Register (TR5):
Bit(s)	Description	(Table R0006)
 63-20	reserved (0)
 19	entry[1] (PentiumMMX only)
	combined with bit 12, selects Way within cache set
 18-15	reserved (0)
 14	cache write-back mode (instead of write-through) enabled
 13	select data cache instead of code cache
 12	select Way within cache set
 11-5	cache set number
 4-2	buffer select (specify which 32-bit portion of cache line to access)
 1-0	control
	00 normal operation
	01 test write
	10 test read
	11 flush (action controlled by TR7)
		TR7.CD/TR7.WD	Action
		 0	x	invalidate code cache line
		 1	0	invalidate data cache line, but don't writeback
		 1	1	invalidate data cache line, writeback if dirty
SeeAlso: #R0004,#R0005
----------S00000008--------------------------
MSR 00000008h - Pentium, PentiumMMX - (TR6) TLB COMMAND
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000007h,MSR 00000009h,MSR 80000008h

Bitfields for Pentium TLB Command Test Register:
Bit(s)	Description	(Table R0007)
 63-32	reserved (0)
 31-12	linear address
 11	TLB entry is valid
 10	page is dirty (has been written to)
 9	page may only be accessed from Ring 0
 8	page may be written
 7-3	reserved (0)
 2	page is 4M instead of 4K
 1	data TLB instead of code TLB
 0	operation (0=write, 1=read)
SeeAlso: #R0008
----------S00000009--------------------------
MSR 00000009h - Pentium, PentiumMMX - (TR7) TLB DATA
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000008h,MSR 0000000Bh,MSR 80000009h

Bitfields for Pentium TLB Data Test Register (TR7):
Bit(s)	Description	(Table R0008)
 63-32	reserved (0)
 31-12	physical address
 11	"CD" Page Cache Disable
 10	"WB" Page Write-Through
 9-7	TLB Least-Recently Used value (non-MMX Pentium only)
 6-5	reserved (0) (P54C)
 6-5	bits 5-4 of TLB entry number (PentiumMMX only)
 4	Hit Indicator
 3-0	bits 3-0 of TLB entry number (PentiumMMX only)
 3-2	TLB entry number (non-MMX Pentium)
 1-0	reserved (0) (non-MMX Pentium)
Note:	if a write with bit 4 (Hit Indicator) set is followed by a read, the
	  value returned in bit 4 indicates whether the selected address was
	  found in the TLB; if found, bits 3-2 indicate which entry contained
	  the hit
SeeAlso: #R0007,#R0009
----------S0000000A--------------------------
MSR 0000000Ah O - Pentium A-step - (TR8) 36-BIT TLB DATA TEST REGISTER
Size:	4 bits
Note:	attempted accesses to this MSR cause an exception on any Pentium except
	  A-step chips, since the 36-bit physical addressing feature was
	  removed from the Pentium prior to general release
SeeAlso: MSR 8000000Ah

Bitfields for Pentium A-step 36-bit addressing Test Register (TR8):
Bit(s)	Description	(Table R0009)
 63-4	reserved (0)
 3-0	high bits of physical address (A35-A32)
SeeAlso: #R0008
----------S0000000B--------------------------
MSR 0000000Bh - Pentium, PentiumMMX - (TR9) BRANCH TARGET BUFFER TAG
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000009h,MSR 0000000Ch,MSR 8000000Bh

Bitfields for non-MMX Pentium Branch Target Buffer Tag (TR9):
Bit(s)	Description	(Table R0010)
 63-32	reserved (0)
 31-6	tag address (bits 31-6 of last byte of branch)
 5-2	reserved (0)
 1-0	history (state of current branch)
SeeAlso: #R0012,#R0013,#R0011

Bitfields for PentiumMMX Branch Target Buffer Tag (TR9):
Bit(s)	Description	(Table R0011)
 63-32	reserved
 31-8	tag address (bits 31-8 of last byte of branch)
 7-6	offset (bits 1-0 of last byte of branch)
 5	valid BTB entry
 4	branch is predicted as taken
 3-0	history (state of current branch)
SeeAlso: #R0010
----------S0000000C--------------------------
MSR 0000000Ch - Pentium, PentiumMMX - (TR10) BRANCH TARGET BUFFER TARGET
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 0000000Bh,MSR 0000000Dh,MSR 8000000Ch

Bitfields for Pentium Branch Target Buffer Target (TR10):
Bit(s)	Description	(Table R0012)
 63-32	reserved (0)
 31-0	target address
SeeAlso: #R0010,#R0013
----------S0000000D--------------------------
MSR 0000000Dh - Pentium, PentiumMMX - (TR11) BRANCH TARGET BUFFER CONTROL
Size:	12 bits
Access:	Write
SeeAlso: MSR 0000000Ch,MSR 0000000Eh,MSR 8000000Dh

Bitfields for Pentium Branch Target Buffer Control (TR11):
Bit(s)	Description	(Table R0013)
 63-26	reserved (0)
 25-24	branch type (PentiumMMX only)
	00 conditional branch
	01 unconditional jump
	10 call
	11 return
 23-13	reserved (0)
 12	bit 2 of test command (PentiumMMX only)
 11-8	BTB set number to access (non-MMX)
 11-8	BTB set number to access (PentiumMMX only)
 7-6	BTB bank (PentiumMMX only)
 5-4	reserved (0)
 3-2	BTB entry (way) within set
 1-0	test command
	00 normal operation
	01 test write
	10 test read
	11 flush
	101 test read tag (PentiumMMX only)
SeeAlso: #R0010,#R0012
----------S0000000E--------------------------
MSR 0000000Eh - Pentium, K6, C6 - (TR12) NEW FEATURE CONTROL
Size:	10 bits
Access:	Write
SeeAlso: MSR 0000000Dh,MSR 8000000Eh

Bitfields for Pentium New Feature Control (TR12):
Bit(s)	Description	(Table R0014)
 63-22	reserved (0)
 21	low-power mode enable
 20	(PentiumMMX only) Data Cache Inhibit (disable internal data cache)
 19	(PentiumMMX only) Code Cache Inhibit (disable internal code cache)
 18-15	reserved (0)
 14	(CPUID=052Bh/052Ch) ignore interrupt immediately after CLI and before
	  STI
 13-10	reserved (0)
 9	enable I/O instruction restart for SMM and use different interrupt
	  priority
 8	generate fast branch-trace message bus cycles
 7	"FTR" ??? (documented as reserved) (0)
 6	disable auto-halt feature (P54C only)
 5	??? (documented as reserved) (0)
 4	disable internal APIC (non-MMX Pentium only)
 3	Cache Inhibit (disable internal L1 cache)
 2	Single-Pipe Execution (disable V pipeline)
 1	enable special branch trace message cycle on BTB hit (default = 0)
 0	disable branch prediction (no BTB)
Notes:	the AMD K6 only supports bit 3 (cache inhibit) of this register;
	  all other bits should be set to zero
	the Centaur (IDT) WinChip C6 supports bits 9, 6, and 3 of this register
----------S0000000F--------------------------
MSR 0000000Fh - Pentium - INVALID
Note:	attempted accesses to this MSR cause an exception
SeeAlso: MSR 8000000Fh,MSR 00000003h
----------S00000010--------------------------
MSR 00000010h - Pentium, Pentium Pro - TIME STAMP COUNTER REGISTER
Size:	64 bits
Access:	Read/Write
Desc:	starting at 00000000h:00000000h on reset, this counter increments on
	  every CPU-core clock cycle
Notes:	on a Pentium Pro, only the low 32 bits may be written; on writes, the
	  high 32 bits are cleared to 00000000h
	also supported by Pentium II; AMD Am5k86,K5,K6; Cyrix 6x86MX; Centaur
	  (IDT) WinChip C6
SeeAlso: MSR 80000010h
----------S00000011--------------------------
MSR 00000011h - Pentium, Cyrix 6x86MX - EVENT COUNTER SELECTION AND CONTROL
Size:	26 bits
Access:	Read/Write
Note:	also supported by Cyrix 6x86MX and Centaur (IDT) WinChip C6
SeeAlso: MSR 00000012h,MSR 00000013h,MSR 00000186h,MSR 80000011h

Bitfields for Pentium Event Counter Control:
Bit(s)	Description	(Table R0015)
 63-27	reserved (0)
 26	(Cyrix 6x86MX only) "ES1" bit 6 of event type for counter 1
 25	external pin PM1 shows counter overflows instead of counter increments
 24	counter 1 counts clock cycles instead of events
 23	enable counter 1 counting in CPL3
 22	enable counter 1 counting in CPL2-0
 21-16	event type for counter 1 (see #R0017)
 15-11	reserved
 10	(Cyrix 6x86MX only) "ES0" bit 6 of event type for counter 0
 9	external pin PM0 shows counter overflows instead of counter increments
 8	counter 0 counts clock cycles instead of events
 7	enable counter 0 counting in CPL3
 6	enable counter 0 counting in CPL2-0
 5-0	event type for counter 0 (see #R0017)
SeeAlso: #R0016

Bitfields for IDT WinChip C6 Event Counter Control:
Bit(s)	Description	(Table R0016)
 63-24	reserved
 23-16	counter 1 control (see #R0018)
 15-8	reserved
 7-0	counter 0 control (see #R0018)
SeeAlso: #R0015

(Table R0017)
Values for Pentium/6x86MX Event Counter event type:
 00h	data read
 01h	data write
 02h	data TLB miss
 03h	data read miss
 04h	data write miss
 05h	write hit to Modified/Exclusive cache line
 06h	data cache lines written back
 07h	external data cache snoops
 08h	external data cache snoop hits
 09h	simultaneous memory accesses in both pipes
 0Ah	data bank access conflict between U and V pipes
 0Bh	misaligned data memory or I/O references
 0Ch	code read
 0Dh	code TLB miss
 0Eh	code cache miss
 0Fh	any segment register load
 10h	(Pentium only) segment descriptor cache accessed
 11h	(Pentium only) segment descriptor cache hit
 12h	any branch
 13h	BTB hit
 14h	taken branch / BTB hit
 15h	pipeline flushes
 16h	total instructions executed
 17h	instruction executed in V pipe
 18h	bus utilization
 19h	pipeline stalled by write backups
 1Ah	pipeline stalled by data memory read
 1Bh	pipeline stalled by write to Modified/Exclusive cache line
 1Ch	locked bus cycle
 1Dh	I/O cycle
 1Eh	non-cacheable memory references
 1Fh	pipeline stalled by Address Generation Interlock
 20h	source/destination conflict
 21h	(undoc) decoding stalls (could only decode one instruction in a
	  particular clock cycle, and that instruction was potentially
	  pairable; i.e. if the following instruction could have executed in
	  the V pipe, it didn't because it wasn't decoded in time)
 22h	floating-point operations
 23h	Breakpoint 0 match
 24h	Breakpoint 1 match
 25h	Breakpoint 2 match
 26h	Breakpoint 3 match
 27h	hardware interrupt
 28h	data read or data write
 29h	data read/write miss
---Pentium---
 2Ah-3Fh reserved
---PentiumMMX---
 2Ah	bus ownership latency (counter 0, duration) or
	bus ownership transfers (counter 1)
 2Bh	MMX instructions executed in U pipe (counter 0) or V pipe (counter 1)
 2Ch	cache M-state line sharing (counter 0) or
	cache line sharing (counter 1)
 2Dh	EMMS instructions executed (counter 0) or
	transitions between MMX/FP (counter 1)
 2Eh	bus use due to processor activity (counter 0, duration) or
	writes to non-cacheable memory (counter 1)
 2Fh	saturating MMX instructions executed (counter 0) or
	saturations performed (counter 1)
 30h	number of cycles not in HLT state (counter 0) or
	number of cycles in HLT state (counter 1)
 31h	MMX instruction data reads (counter 0) or
	MMX instruction data read misses
 32h	floating-point stalls (counter 0) or taken branches (counter 1)
 33h	D1 starvation and FIFO is empty (counter 0) or
	D1 starvation and only one instruction in FIFO (counter 1)
 34h	MMX instruction data writes (counter 0) or
	MMX instruction data write misses (counter 1)
 35h	pipeline flushes due to wrong branch prediction (counter 0) or
	pl. flushes due to wrong branch pred. resolved in WB stage (counter 1)
 36h	misaligned data memory reference on MMX instruction (counter 0) or
	pipeline stalled waiting for MMX instruction data mem read (counter 1)
 37h	returns, predicted incorrectly or not at all (counter 0) or
	total returns predicted (counter 1)
 38h	clocks MMX instruction multiply unit interlock (counter 0) or
	clocks MOVD/MOVQ store stall (counter 1)
 39h	returns (counter 0 only)
 3Ah	BTB false entries (counter 0) or
	BTB prediction miss on not-taken branch (counter 1)
 3Bh	clocks MMX instruction stalled due to full write buffers (counter 0) or
	clocks stalled on MMX instruction write to E or M line (counter 1)
---6x86MX---
 2Ah	reserved
 2Bh	MMX instructions executed in X pipe (counter 0) or Y pipe (counter 1)
 2Ch	reserved
 2Dh	EMMS instructions executed (counter 0) or
	transitions between MMX/FP (counter 1)
 2Eh	reserved
 2Fh	saturating MMX instructions executed (counter 0) or
	saturations performed (counter 1)
 30h	reserved
 31h	MMX instruction data reads (counter 0 only)
 32h	taken branches (counter 1 only)
 33h-36h reserved
 37h	returns, predicted incorrectly or not at all (counter 0) or
	total returns predicted (counter 1)
 38h	clocks MMX instruction multiply unit interlock (counter 0) or
	clocks MOVD/MOVQ store stall (counter 1)
 39h	returns (counter 0) or return stack buffer overflows (counter 1)
 3Ah	BTB false entries (counter 0) or
	BTB prediction miss on not-taken branch (counter 1)
 3Bh	clocks MMX instruction stalled due to full write buffers (counter 0) or
	clocks stalled on MMX instruction write to E or M line (counter 1)
 3Ch-3Fh reserved
 40h	L2 TLB misses (code or data)
 41h	L2 TLB data miss
 42h	L2 TLB code miss
 43h	L1 TLB miss (code or data)
 44h	TLB flushes
 45h	TLB page invalidations
 46h	TLB page invalidations which hit
 47h	reserved
 48h	instructions decoded
 49h-7Fh reserved
SeeAlso: #R0015,#R0018

(Table R0018)
Values for IDT WinChip C6 event:
 00h	internal clocks
 01h	valid cycles reaching writebacks
 02h	x86 instructions
 47h	data read cache misses
 4Ah	data write cache misses
 63h	instruction fetch cache miss
SeeAlso: #R0016,#R0017
----------S00000012--------------------------
MSR 00000012h - Pentium, Cyrix 6x86MX - EVENT COUNTER #0
Size:	40 bits
Access:	Read/Write
Note:	also supported by Cyrix 6x86MX and Centaur (IDT) WinChip C6
SeeAlso: MSR 00000011h,MSR 00000013h,MSR 80000012h,MSR 000000C1h
----------S00000013--------------------------
MSR 00000013h - Pentium, Cyrix 6x86MX - EVENT COUNTER #1
Size:	40 bits
Access:	Read/Write
Note:	also supported by Cyrix 6x86MX and Centaur (IDT) WinChip C6
SeeAlso: MSR 00000011h,MSR 00000012h,MSR 80000013h,MSR 000000C2h
----------S00000014--------------------------
MSR 00000014h - Pentium P54C - bug?
Note:	returns 0 on all reads and ignores any writes for P54C processors with
	  CPUID values <= 0524h, rather than causing an exception; possibly due
	  to a microcode bug
----------S00000017--------------------------
MSR 00000017h - Pentium Pro - ???
----------S00000018--------------------------
MSR 00000018h - Pentium Pro - ???
----------S0000001B--------------------------
MSR 0000001Bh - Pentium Pro, PentiumII - APIC BASE ADDRESS
SeeAlso: MEM FEE00000h

Bitfields for Pentium Pro/PentiumII MSR 0000001Bh:
Bit(s)	Description	(Table R0019)
 63-32	reserved
 31-12	APIC base address bits 31-12
 11	APIC global enable (can not be cleared except through hard reset)
 10-9	reserved
 8	this is the BootStrap Processor
 7-0	reserved
----------S00000021--------------------------
MSR 00000021h - Pentium II - ???
----------S0000002A--------------------------
MSR 0000002Ah - Pentium Pro - "EBL_CR_POWERON"
Size:	32 bits
Access:	Read/write

Bitfields for Pentium Pro MSR 0000002Ah:
Bit(s)	Description	(Table R0020)
 31-27	reserved
 26	(read-only) Low Power enable
 25	reserved
 24-22	(read-only) clock frequency ratio (see #R0021)
 21-20	(read-only) symmetric arbitration ID
 19-18	???
 17-16	(read-only) APIC cluster ID
 15	(read-only) FRC [Funtional Redundancy Checking] mode enabled
 14	(read-only) Power-on Reset Vector at 1M instead of 4G
 13	(read-only) IN Order Queue depth is 1 instead of 8
 12	(read-only) BINIT# observation enabled
 11	???
 10	(read-only) AERR# observation enabled
 9	Execute-BIST enabled
 8	output tri-state enabled
 7	disable BINIT# drive
 6	disable BERR# for initiator internal errors
 5	reserved
 4	disable BERR# for initiator bus requests
 3	disable AERR# drive
 2	disable response error checking
 1	disable data error checking
 0	data bus uses ECC instead of parity

(Table R0021)
Values for Pentium Pro/PentiumII clock multiplier:
 0	x2
 1	x4
 2	x3
 4	x2.5
 6	x3.5
 15	x2
SeeAlso: #R0020
----------S00000032--------------------------
MSR 00000032h - Pentium Pro - ???
----------S00000033--------------------------
MSR 00000033h - Pentium Pro, PentiumII - "TEST_CTL" TEST CONTROL REGISTER
SeeAlso: 32 bits

Bitfields for Pentium Pro MSR 0033h:
Bit(s)	Description	(Table R0022)
 31	(step sB1 and later) disable LOCK# for locked transactions which
	  are split across a cache line boundary
 30	(step sB1 and later) disable Instruction Streaming buffers
	--used to work around sB1 errata 58 and 59
 29-0	reserved
----------S00000034--------------------------
MSR 00000034h - Pentium Pro - ???
----------S0000003A--------------------------
MSR 0000003Ah - Pentium Pro - ???
----------S0000003B--------------------------
MSR 0000003Bh - PentiumII - ???
----------S00000050--------------------------
MSR 00000050h - Pentium Pro - ???
----------S00000051--------------------------
MSR 00000051h - Pentium Pro - ???
----------S00000052--------------------------
MSR 00000052h - Pentium Pro - ???
----------S00000053--------------------------
MSR 00000053h - Pentium Pro - ???
----------S00000054--------------------------
MSR 00000054h - Pentium Pro - ???
----------S00000079--------------------------
MSR 00000079h - Pentium Pro, PentiumII - BIOS UPDATE TRIGGER
Size:	32 bits
Access:	Write
Desc:	writing the linear address of a microcode update block (see #00533)
	  to this MSR cause the CPU to initiate a microcode load
SeeAlso: INT 15/AX=D042h/BL=01h,MSR 0000008Bh
----------S00000082--------------------------
MSR 00000082h - AMD Am5k86 (AMD-K5) - ARRAY ACCESS REGISTER
Size:	64 bits
Note:	EDX remains unchanged after an RDMSR to simplify multiple accesses
SeeAlso: MSR 00000083h

Bitfields for AMD Am5k86 (AMD-K5) Array Access Register:
Bit(s)	Description	(Table R0023)
 63-40	pointer within array specified below
 39-32	array identifier (see #R0024)
 31-0	array data
SeeAlso: #R0036

(Table R0024)
Values for AMD Am5k86 Array Pointer:
 E0h	data cache (data)
 E1h	data cache (linear tag) (see #R0025)
 E4h	code cache (instruction) (see #R0026)
 E5h	code cache (linear tag) (see #R0027)
 E6h	code cache (valid bits) (see #R0028)
 E7h	code cache (branch-prediction bits) (see #R0029)
 E8h	4K TLB (page) (see #R0030)
 E9h	4K TLB (linear tag) (see #R0031)
 EAh	4M TLB (page) (see #R0032)
 EBh	4M TLB (linear tag) (see #R0033)
 ECh	data cache (physical tag) (see #R0034)
 EDh	code cache (physical tag) (see #R0035)
SeeAlso: #R0023

Bitfields for AMD AmK586 data cache linear tag:
Bit(s)	Description	(Table R0025)
 31-26	reserved (0)
 25	cache line is dirty
 24	user/supervisor
 23	read/write
 22	0
 21	linear address valid
 20-0	tag
SeeAlso: #R0024,#R0034

Bitfields for AMD Am5k86 code cache instruction:
Bit(s)	Description	(Table R0026)
 31-26	reserved (0)
 25	start bit 1
 24	end bit 1
 23	opcode bit 1
 22-21	map (ROPs/MROM) 1
 20-13	byte 1
 12	start bit 0
 11	end bit 0
 10	opcode bit 0
 9-8	map (ROPs/MROM) 0
 7-0	byte 0
SeeAlso: #R0024,#R0027,#R0035

Bitfields for Am5k86 code cache linear tag:
Bit(s)	Description	(Table R0027)
 31-20	reserved (0)
 19-0	bits 31-12 of linear address
SeeAlso: #R0024,#R0026,#R0028,#R0035

Bitfields for Am5k86 code cache valid bits:
Bit(s)	Description	(Table R0028)
 31-18	reserved (0)
 17	linear tag is valid
 16	user/supervisor
 15-0	bitmask of valid bytes
SeeAlso: #R0024,#R0026,#R0035

Bitfields for Am5k86 code cache branch prediction bits:
Bit(s)	Description	(Table R0029)
 31-19	reserved (0)
 18	predicted branch taken
 17-14	offset of last byte of predicted branch instruction within block
 13-12	predicted target column
 11-4	predicted target index
 3-0	target byte
SeeAlso: #R0024

Bitfields for Am5k86 4K TLB page:
Bit(s)	Description	(Table R0030)
 31-22	reserved (0)
 21	page cache disable
 20	page write-through
 19-0	page frame address
SeeAlso: #R0024,#R0031,#R0032

Bitfields for Am5k86 4K TLB linear tag:
Bit(s)	Description	(Table R0031)
 31-20	reserved (0)
 19	global valid bit
 18	TLB entry is dirty
 17	user/supervisor
 16	read/write
 15	entry is valid
 14-0	tag (bits 31-17 of address)
SeeAlso: #R0024,#R0030,#R0033

Bitfields for Am5k86 4M TLB page:
Bit(s)	Description	(Table R0032)
 31-12	reserved (0)
 11	page cache disable
 10	page write-through
 9-0	page frame address
SeeAlso: #R0024,#R0030,#R0033

Bitfields for Am5k86 4M TLB linear tag:
Bit(s)	Description	(Table R0033)
 31-15	reserved (0)
 14	global valid bit
 13	TLB entry is dirty
 12	user/supervisor
 11	read/write
 10	entry is valid
 9-0	tag (bits 31-22 of address)
SeeAlso: #R0024,#R0031,#R0032

Bitfields for Am5k86 data cache physical tag:
Bit(s)	Description	(Table R0034)
 31-23	reserved (0)
 22-21	MESI status
	00 invalid
	01 shared
	10 modified
	11 exclusive
 20-0	tag (bits 31-11 of physical address)
SeeAlso: #R0024,#R0035

Bitfields for Am5k86 code cache physical tag:
Bit(s)	Description	(Table R0035)
 31-21	reserved (0)
 20	valid
 19-0	tag (bits 31-12 of physical address)
SeeAlso: #R0024,#R0034
----------S00000083--------------------------
MSR 00000083h - AMD Am5k86 (AMD-K5) - HARDWARE CONFIGURATION REGISTER
Size:	8 bits
SeeAlso: MSR 00000082h

Bitfields for AMD Am5k86 (AMD-K5) Hardware Configuration Register:
Bit(s)	Description	(Table R0036)
 63-8	reserved
 7	disable data cache
 6	disable instruction cache
 5	disable branch prediction
 4	enable write allocation (stepping 4 and higher only)
 3-1	debug control
	000 off
	001 enable branch trace (requires bit 5 set as well)
	100 enable Probe Mode on debug trap
	other reserved
 0	disable Stopping Processor Clock in Halt and Stop Grant states
SeeAlso: #R0023
----------S00000085--------------------------
MSR 00000085h - AMD-K5 - WRITE ALLOCATE TOP-OF-MEMORY AND CONTROL REGISTER
Note:	this MSR is supported on K5 models 1/2/3 stepping 4 and higher only
SeeAlso: MSR 00000086h
!!!amd\21062e.pdf p.95
----------S00000086--------------------------
MSR 00000086h - AMD-K5 - WRITE ALLOCATE PROGRAMMABLE MEMORY RANGE REGISTER
Note:	this MSR is supported on K5 models 1/2/3 stepping 4 and higher only
SeeAlso: MSR 00000085h
----------S00000088--------------------------
MSR 00000088h - Pentium Pro, PentiumII - "BBL_CR_D0" CHUNK 0 DATA REGISTER
Note:	this register is used to read from and write to L2 cache
SeeAlso: MSR 00000089h,MSR 0000008Ah,MSR 00000116h
----------S00000089--------------------------
MSR 00000089h - Pentium Pro, PentiumII - "BBL_CR_D1" CHUNK 1 DATA REGISTER
Note:	this register is used to read from and write to L2 cache
SeeAlso: MSR 00000088h,MSR 0000008Ah,MSR 00000116h
----------S0000008A--------------------------
MSR 0000008Ah - Pentium Pro, PentiumII - "BBL_CR_D2" CHUNK 2 DATA REGISTER
Note:	this register is used to read from and write to L2 cache
SeeAlso: MSR 00000088h,MSR 00000089h,MSR 00000116h
----------S0000008B--------------------------
MSR 0000008Bh - Pentium Pro - "BIOS_SIGN" BIOS UPDATE SIGNATURE
Size:	64 bits
Access:	Read/Write
Desc:	used to determine which (if any) microcode update has been loaded into
	  the CPU
Notes:	whenever a microcode update is loaded, the PentiumPro modifies the
	  operation of the CPUID instruction to store both the standard CPUID
	  model information and a 32-bit microcode update ID into this MSR; if
	  no microcode update has been loaded, the MSR remains unchanged
	  (it is normally cleared to 0 before using CPUID to test for updates)
	the low 32 bits of this register (if modified by CPUID) contains the
	  standard model/stepping information, while the high 32 bits contain
	  the microcode update ID
SeeAlso: MSR 00000079h
----------S0000008B--------------------------
MSR 0000008Bh - PentiumII - "BBL_CR_D3" CHUNK 3 DATA REGISTER
Notes:	this register is used to read from and write to L2 cache
	whether this MSR is the BIOS update signature or L2 data depends on
	  the usage model
SeeAlso: MSR 00000088h,MSR 00000089h,MSR 00000116h
----------S000000AE--------------------------
MSR 000000AEh - Pentium Pro - ???
----------S000000C1--------------------------
MSR 000000C1h - Pentium Pro - "PERFCTR0" PERFORMANCE COUNTER REGISTER 0
Note:	the performance measure counted by this MSR is set through MSR 0186h
SeeAlso: MSR 000000C2h,MSR 00000012h,MSR 00000186h
----------S000000C2--------------------------
MSR 000000C2h - Pentium Pro - "PERFCTR1" PERFORMANCE COUNTER REGISTER 1
Note:	the performance measure counted by this MSR is set through MSR 0187h
SeeAlso: MSR 000000C1h,MSR 00000013h,MSR 00000187h
----------S000000FE--------------------------
MSR 000000FEh - Pentium Pro - "MTRRcap" MEMORY TYPE RANGE REGISTER CAPABILITIES
Desc:	determine how many and what type of Memory Type Range Registers are
	  implemented
SeeAlso: MSR 00000200h,MSR 00000250h,MSR 000002FFh

Bitfields for Pentium Pro "MTRRcap" register:
Bit(s)	Description	(Table R0037)
 63-8	???
 7-0	number of Memory Type Range Registers (at MSR 02xxh)
----------S00000107--------------------------
MSR 00000107h - Centaur (IDT) WinChip C6 - Feature Control Register #1
Size:	30 bits
SeeAlso: MSR 00000108h,MSR 00000109h

Bitfields for Centaur (IDT) WinChip C6 Feature Control Register #1:
Bit(s)	Description	(Table R0038)
 61-31	reserved
 30	enable MOV TRx instructions
 29	disable CPUID instruction
 28	don't use alternative "divide 5 by 2" EFLAGS
	0 = use Centaur (IDT) flags
	1 = use Intel flags
 27-26	reserved
 25-22	stepping ID
 21-17	reserved
 16	enable return stack (default)
 15	disable bus pipelining #NA response
 14	disable data cache
 13	disable instruction cache
 12	reserved
 11	disable page directory cache
 10	reserved
 9	enable MMX instructions (default)
 8	enable data cache updates for PDE/PTE
 7	disable check for self-modifying code
 6	enable linear burst mode
 5	disable #STPCLK support
 4	disable machine check exception
 3	disable power management
 2	enable #MC for internal errors
 1	set CPUID feature flag for CMPXCHG8 instruction
 0	reserved
SeeAlso: #R0039,#R0040
----------S00000108--------------------------
MSR 00000108h - Centaur (IDT) WinChip C6 - Feature Control Register #2
Size:	64 bits
SeeAlso: MSR 00000107h,MSR 00000109h

Bitfields for Centaur (IDT) WinChip C6 Feature Control Register #2:
Bit(s)	Description	(Table R0039)
 63-32	last four bytes of CPUID vendor ID string (see also #R0040)
 31-15	reserved
 14	use alternative CPUID vendor string
 13-12	reserved
 11-8	CPUID family
 7-4	CPUID model
 3-0	reserved
SeeAlso: #R0038,#R0039
----------S00000109--------------------------
MSR 00000109h - Centaur (IDT) WinChip C6 - Feature Control Register #3
Size:	30 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000108h

Bitfields for Centaur (IDT) WinChip C6 Feature Control Register #3:
Bit(s)	Description	(Table R0040)
 63-32	first four bytes of CPUID vendor ID string
 31-0	middle four bytes of CPUID vendor ID string
SeeAlso: #R0039
----------S00000110--------------------------
MSR 00000110h - Centaur (IDT) WinChip C6 - Memory Configuration Register #0
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000111h,MSR 00000117h"Centaur"

Bitfields for Centaur (IDT) WinChip C6 Memory Configuration Register:
Bit(s)	Description	(Table R0041)
 63-44	base address of memory region
 43-32	reserved
 31-12	memory region mask
	(region is hit if (base AND address) == (mask AND address))
 11-5	reserved
 4-3	memory write order
	00 strong ordering
	01 weak for string
	10 weak for stack
	11 weak ordering for all writes
 2	enable write merging for stack writes
 1	enable write merging for string writes
 0	enable write merging for other writes
SeeAlso: #R0045
----------S00000111--------------------------
MSR 00000111h - Centaur (IDT) WinChip C6 - Memory Configuration Register #1
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000110h,MSR 00000112h,#R0041
----------S00000112--------------------------
MSR 00000112h - Centaur (IDT) WinChip C6 - Memory Configuration Register #2
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000111h,MSR 00000113h,#R0041
----------S00000113--------------------------
MSR 00000113h - Centaur (IDT) WinChip C6 - Memory Configuration Register #3
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000112h,MSR 00000114h,#R0041
----------S00000114--------------------------
MSR 00000114h - Centaur (IDT) WinChip C6 - Memory Configuration Register #4
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000113h,MSR 00000115h,#R0041
----------S00000115--------------------------
MSR 00000115h - Centaur (IDT) WinChip C6 - Memory Configuration Register #5
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000114h,MSR 00000116h"Centaur",#R0041
----------S00000116--------------------------
MSR 00000116h - PentiumII - "BBL_CR_ADDR" - SET L2 CACHE ADDRESS
Size:	32 bits
SeeAlso: MSR 00000088h,MSR 00000118h"PentiumII"

Bitfields for PentiumII "BBL_CR_ADDR":
Bit(s)	Description	(Table R0042)
 31-3	cache address bits 31-3 (docs say 35-3!)
 2-0	reserved (0) 
----------S00000116--------------------------
MSR 00000116h - Centaur (IDT) WinChip C6 - Memory Configuration Register #6
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000115h,MSR 00000117h"Centaur",#R0041
----------S00000117--------------------------
MSR 00000117h - Centaur (IDT) WinChip C6 - Memory Configuration Register #7
Size:	64 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000110h,MSR 00000116h"Centaur",#R0041
----------S00000118--------------------------
MSR 00000118h - PentiumII - "BBL_CR_DECC" READ/WRITE L2 CACHE ECC BITS
Size:	8 bits
SeeAlso: MSR 00000088h,MSR 00000116h"PentiumII",MSR 00000119h
----------S00000119--------------------------
MSR 00000119h - PentiumII - "BBL_CR_CTL"
SeeAlso: MSR 00000118h,MSR 0000011Ah

Bitfields for PentiumII "BBL_CR_CTL":
Bit(s)	Description	(Table R0043)
 63-19	reserved
 18	use supplied ECC
 17	reserved
 16	L2 hit
 15-14	reserved
 13-12	state from L2 entry
	00 invalid
	01 shared
	10 exclusive
	11 modified
 11-10	way number from L2 cache
 9-8	way number to L2
 7	reserved
 6-5	state to L2 entry (as for bits 13-12)
 4-0	L2 command
	00010 read L2 control register
	00011 write L2 control register
	010mm tag write with data read
	01100 data read with LRU update
	01110 tag read with data read
	01111 tag inquire
	100mm tag write
	('mm' = MESI state, coded as for bits 13-12)
----------S0000011A--------------------------
MSR 0000011Ah - PentiumII - "BBL_CR_TRIG" TRIGGER CACHE CONFIGURATION CYCLE
Note:	a write (must write 00000000h!) to this MSR triggers a cache
	  configuration access cycle
SeeAlso: MSR 00000088h,MSR 00000118h,MSR 0000011Bh
----------S0000011B--------------------------
MSR 0000011Bh - PentiumII - "BBL_CR_BUSY" CHECK IF CACHE CONFIG IN PROGRESS
Size:	1 bit
Access:	Read-Only
Note:	if bit 0 is set, an L2 cache configuration access command is in
	  progress
SeeAlso: MSR 00000088h,MSR 00000118h,MSR 0000011Ah
----------S0000011E--------------------------
MSR 0000011Eh - Pentium II - "BBL_CR_CTL3" L2 CACHE CONTROL REGISTER 3
SeeAlso: MSR 00000088h,MSR 00000116h,MSR 0000011Ah,MSR 0000011Bh

Bitfields for Pentium II L2 cache control:
Bit(s)	Description	(Table R0044)
 63-26	reserved
 25	(read-only) cache bus fraction
 24	reserved
 23	(read-only) L2 hardware disable
 22-20	supported L2 physical address range
	000  512M
	001    1G
	010    2G
	011    4G
	100    8G
	101   16G
	110   32G
	111   64G
 19	reserved
 18	enable cache state error checking
 17-13	cache size per bank
	00001 256K
	00010 512K
	00100	1M
	01000	2M
	10000	4M
 12-11	(read-only) number of L2 banks
 10-9	(read-only) L2 associativity
	00 direct-mapped
	01 2-way associative
	10 4-way associative
	11 reserved
 8	L2 cache enabled
 7	CRTN parity checking enabled
 6	address parity checking enabled
 5	enable ECC testing of L2 cache memory
 4-1	L2 cache latency
 0	L2 has been configured
----------S00000120--------------------------
MSR 00000120h - Centaur (IDT) WinChip C6 - Memory Config Register Control
Size: 25 bits
Access:	Write-Only
SeeAlso: MSR 00000107h,MSR 00000110h,MSR 00000117h

Bitfields for Centaur (IDT) WinChip C6 Memory Configuration Control Register:
Bit(s)	Description	(Table R0045)
 63-25	reserved
 24-20	reserved (1)
 19-5	reserved
 4	enable weak write ordering
 3-2	write merging for string writes
	00 forward combining
	01 forward/overlapped
	10 forward/reverse
	11 forward/reverse/overlap
 1-0	write merging for non-stack/non-string writes
	00 forward combining
	01 forward/overlapped
	10 forward/reverse
	11 forward/reverse/overlap
SeeAlso: #R0041
----------S00000131--------------------------
MSR 00000131h - Pentium Pro - ???
----------S0000014E--------------------------
MSR 0000014Eh - Pentium Pro - ???
----------S0000014F--------------------------
MSR 0000014Fh - Pentium Pro - ???
----------S00000150--------------------------
MSR 00000150h - Pentium Pro - ???
----------S00000151--------------------------
MSR 00000151h - Pentium Pro - ???
----------S00000154--------------------------
MSR 00000154h - Pentium Pro - ???
----------S0000015B--------------------------
MSR 0000015Bh - Pentium Pro - ???
----------S0000015F--------------------------
MSR 0000015Fh - Pentium Pro - ???
----------S00000174--------------------------
MSR 00000174h - Pentium Pro - "SYSENTER_CS" - SYSENTER target CS
----------S00000175--------------------------
MSR 00000175h - Pentium Pro - "SYSENTER_ESP" - SYSENTER target ESP
----------S00000176--------------------------
MSR 00000176h - Pentium Pro - "SYSENTER_EIP" - SYSENTER target EIP
----------S00000179--------------------------
MSR 00000179h - Pentium Pro - "MCG_CAP"
SeeAlso: MSR 0000017Ah,MSR 0000017Bh

Bitfields for Pentium Pro "MCG_CAP" register:
Bit(s)	Description	(Table R0046)
 63-8	???
 7-0	number of MCRs
----------S0000017A--------------------------
MSR 0000017Ah - Pentium Pro - "MCG_STATUS"
SeeAlso: MSR 00000179h,MSR 0000017Bh
----------S0000017B--------------------------
MSR 0000017Bh - Pentium Pro - "MCG_CTL"
SeeAlso: MSR 00000179h,MSR 0000017Ah
----------S00000186--------------------------
MSR 00000186h - Pentium Pro - "EVNTSEL0" - PERFORM. COUNTER EVENT SELECTION 0
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 000000C1h,MSR 00000187h,MSR 00000011h,MSR 00000012h

Bitfields for Pentium Pro Event Selection MSR:
Bit(s)	Description	(Table R0047)
 31-24	CMASK (counter mask)
	compare actual count for event on this clock cycle with mask; only
	  increment counter if count >= mask (count < mask if bit 23 set)
 23	invert result of CMASK condition
 22	enable counting of events
 21	reserved
 20	signal performance counter overflows via APIC input
 19	signal performance counter overflows via BP0/BP1 pin
 18	count occurrences, not duration
 17	OS (enable counting in ring 0)
 16	USER (enable counting in rings 1,2,3)
 15-8	UMASK (Unit Mask register; set to 0 to enable all count options)
 7-0	event type (see #R0048)

(Table R0048)
Values for Pentium Pro/Pentium II performance event type:
 00h-01h	documented as unused
 02h	number of store buffer forwards
 03h	number of store buffer blocks
 04h	number of store buffer drain cycles
 05h	misaligned data memory references
 06h	segment register loads
 07h-0Fh	documented as unused
 10h	executed computational FP operations
 11h	number of microcode-handled FP exceptions
 12h	number of multiplies
 13h	number of divisions
 14h	divider busy cycles
 15h-20h	documented as unused
 21h	L2 address strobes
 22h	L2 cache data bus wait cycles
 23h	L2 cache data bus transfer cycles
 24h	allocated L2-cache lines
 25h	allocated L2 modified lines
 26h	removed L2 lines
 27h	removed modified L2 lines
 28h	instruction fetches from L2 cache
 29h	loads requested from L2 cache
 2Ah	stores into L2 cache
 2Bh-2Dh	documented as unused
 2Eh	total L2 requests
 2Fh-3Fh	documented as unused
 40h	L1 Data Cache Unit load rquests
 41h	L1 DCU store requests
 42h	L1 DCU locked requests
 43h	total memory references (all types, reads+writes+internal retries)
 44h	documented as unused
 45h	L1 allocated lines
 46h	L1 allocated M-state lines
 47h	L1 evicted M-state lines
 48h	L1 outstanding miss cycles (weighted)
 49h	L1 data TLB misses
 4Ah-51h	documented as unused
 52h	(P-II) self-modifying code occurrences
 53h-5Fh	documented as unused
 60h	outstanding bus requests
 61h	number of cycles BNR pin driven
 62h	DRDY# asserted cycles
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 63h	number of cycles with LOCK asserted
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 64h	CPU receiving data cycles
 65h	burst-read transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 66h	read for ownership transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 67h	write-back transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 68h	instruction-fetch transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 69h	invalidate transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 6Ah	partial-write transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 6Bh	partial transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 6Ch	I/O transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 6Dh	deferred transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 6Eh	burst transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 6Fh	memory transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 70h	total of all transactions
	unit mask 20h to get total counts for ALL CPUs, 00h for this CPU only
 71h-78h	documented as unused
 79h	processor not-halted cycles
 7Ah	cycles in which HIT pin is driven
 7Bh	cycles in which HITM pin is driven
 7Ch-7Dh	documented as unused
 7Eh	bus-snoop stall cycles
 7Fh	documented as unused
 80h	instruction fetches
 81h	instruction fetch misses
 82h-84h	documented as unused
 85h	L1 instruction TLB misses
 86h	instruction-fetch stall cycles
 87h	instruction-length decoder stall cycles
 88h-A1h	documented as unused
 A2h	resource-related stall cycles
 A3h-AFh	documented as unused
 B0h	(P-II) MMX instructions executed
 B1h	(P-II) saturated arithmetic instructions executed
 B2h	(P-II) MMX uOPs executed on Port #0--3
 B3h	(P-II) MMX instructions
	unit mask selects type(s): 01h packed multiply, 02h packed shift,
	  04h pack operations, 08h unpack operations, 10h packed logical,
	  20h packed arithmetic
 B4h-BFh	documented as unused
 C0h	retired instructions
 C1h	retired FLOPs
 C2h	retired uOPs
 C3h	documented as unused
 C4h	retired branch predictions
 C5h	retired mispredicted branches
 C6h	total cycles with interrupts disabled
 C7h	total cycles with interrupts disabled and interrupt(s) pending
 C8h	received hardware interrupts
 C9h	retired taken branches
 CAh	retired taken mispredicted branches
 CBh	documented as unused
 CCh	(P-II) transitions between FP and MMX states
	unit mask: 00h = from MMX to FP, 01h = from FP to MMX
 CDh	(P-II) SIMD assists (EMMS instructions executed)
 CEh	(P-II) MMX instructions retired
 CFh	(P-II) saturated arithmetic instructions retired
 D0h	decoded instructions
 D1h	documented as unused
 D2h	partial stall cycles or events
 D3h	documented as unused
 D4h	(P-II) segment rename stalls
	set unit mask to sum of: 01h for ES, 02h for DS, 04h for FS, 08h for GS
 D5h	(P-II) segment renames (unit mask as for D4h)
 D6h	(P-II) retired segment renames
 D7h-DFh	documented as unused
 E0h	decoded branch instructinos
 E1h	documented as unused
 E2h	BTB misses
 E3h	documented as unused
 E4h	bogus branches (predictions generated for non-branch instructions)
 E5h	documented as unused
 E6h	number of times BACLEAR asserted (number of static branch predictions)
 E7h-FFh	documented as unused
SeeAlso: #R0047
----------S00000187--------------------------
MSR 00000187h - Pentium Pro - "EVNTSEL1" - PERFORM. COUNTER EVENT SELECTION 1
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 000000C2h,MSR 00000186h,#R0047,MSR 00000011h,MSR 00000013h,#R0047
----------S000001D3--------------------------
MSR 000001D3h - Pentium Pro - ???
----------S000001D9--------------------------
MSR 000001D9h - Pentium Pro, PentiumII - "DEBUGCTLMSR" DEBUGGING CONTROL
Size:	16 bits

Bitfields for Pentium Pro Debugging Control MSR:
Bit(s)	Description	(Table R0049)
 63-16	reserved
 15	enable execution trace messages
 14	enable execution trace messages
 13-7	reserved
 6	enable execution trace messages
 5	performance monitor/Breakpoint pins
 4	performance monitor/Breakpoint pins
 3	performance monitor/Breakpoint pins
 2	performance monitor/Breakpoint pins
 1	Branch Trap Flag
 0	enable Last Branch records (see MSR 000001DBh,MSR 000001DCh)
----------S000001DB--------------------------
MSR 000001DBh - Pentium Pro, PentiumII - "LASTBRANCHFROMIP"
Desc:	stores the address from which a branch was last taken
SeeAlso: MSR 000001DCh,MSR 000001DDh
----------S000001DC--------------------------
MSR 000001DCh - Pentium Pro, PentiumII - "LASTBRANCHTOIP"
Desc:	stores the destination address of the last taken branch instruction
SeeAlso: MSR 000001DBh,MSR 000001DEh
----------S000001DD--------------------------
MSR 000001DDh - Pentium Pro, PentiumII - "LASTINTFROMIP"
Desc:	stores the address at which an interrupt last occurred
SeeAlso: MSR 000001DBh,MSR 000001DEh
----------S000001DE--------------------------
MSR 000001DEh - Pentium Pro, PentiumII - "LASTINTTOIP"
Desc:	stores the address to which the last interrupt caused a branch
SeeAlso: MSR 000001DCh,MSR 000001DDh
----------S000001E0--------------------------
MSR 000001E0h - Pentium Pro - "ROB_CR_BKUPTMPDR6"
Size:	>= 3 bits

Bitfields for Pentium Pro MSR 000001E0h:
Bit(s)	Description	(Table R0050)
 63-3	???
 2	Fast String Enable (default is enabled)
 1-0	reserved
Note:	if bit 2 is set, REP MOVS moves 64 bits each clock cycle if both source
	  and target are QWORD-aligned
----------S00000200--------------------------
MSR 00000200h - Pentium Pro - "MTRRphysBase0"
SeeAlso: MSR 000000FEh,MSR 00000201h,MSR 00000202h
----------S00000201--------------------------
MSR 00000201h - Pentium Pro - "MTRRphysMask0"
SeeAlso: MSR 000000FEh,MSR 00000200h,MSR 00000202h
----------S00000202--------------------------
MSR 00000202h - Pentium Pro - "MTRRphysBase1"
SeeAlso: MSR 000000FEh,MSR 00000200h,MSR 00000203h
----------S00000203--------------------------
MSR 00000203h - Pentium Pro - "MTRRphysMask1"
SeeAlso: MSR 000000FEh,MSR 00000201h,MSR 00000202h
----------S00000204--------------------------
MSR 00000204h - Pentium Pro - "MTRRphysBase2"
----------S00000205--------------------------
MSR 00000205h - Pentium Pro - "MTRRphysMask2"
----------S00000206--------------------------
MSR 00000206h - Pentium Pro - "MTRRphysBase3"
----------S00000207--------------------------
MSR 00000207h - Pentium Pro - "MTRRphysMask3"
----------S00000208--------------------------
MSR 00000208h - Pentium Pro - "MTRRphysBase4"
----------S00000209--------------------------
MSR 00000209h - Pentium Pro - "MTRRphysMask4"
----------S0000020A--------------------------
MSR 0000020Ah - Pentium Pro - "MTRRphysBase5"
----------S0000020B--------------------------
MSR 0000020Bh - Pentium Pro - "MTRRphysMask5"
----------S0000020C--------------------------
MSR 0000020Ch - Pentium Pro - "MTRRphysBase6"
----------S0000020D--------------------------
MSR 0000020Dh - Pentium Pro - "MTRRphysMask6"
----------S0000020E--------------------------
MSR 0000020Eh - Pentium Pro - "MTRRphysBase7"
----------S0000020F--------------------------
MSR 0000020Fh - Pentium Pro - "MTRRphysMask7"
----------S00000250--------------------------
MSR 00000250h - Pentium Pro - "MTRRfix64K_00000"
Desc:	control the 64K region from 00000h to 0FFFFh
SeeAlso: MSR 000000FEh,MSR 00000200h,MSR 00000258h
----------S00000258--------------------------
MSR 00000258h - Pentium Pro - "MTRRfix16K_80000"
Desc:	control the 16K region from 80000h to 83FFFh
SeeAlso: MSR 000000FEh,MSR 00000250h,MSR 00000259h
----------S00000259--------------------------
MSR 00000259h - Pentium Pro - "MTRRfix16K_A0000"
Desc:	control the 16K region from A0000h to A3FFFh
----------S00000268--------------------------
MSR 00000268h - Pentium Pro - "MTRRfix4K_C0000"
Desc:	control the 4K region from C0000h to C0FFFh
----------S00000269--------------------------
MSR 00000269h - Pentium Pro - "MTRRfix4K_C8000"
Desc:	control the 4K region from C8000h to C8FFFh
----------S0000026A--------------------------
MSR 0000026Ah - Pentium Pro - "MTRRfix4K_D0000"
Desc:	control the 4K region from D0000h to D0FFFh
----------S0000026B--------------------------
MSR 0000026Bh - Pentium Pro - "MTRRfix4K_D8000"
Desc:	control the 64K region from D8000h to D8FFFh
----------S0000026C--------------------------
MSR 0000026Ch - Pentium Pro - "MTRRfix4K_E0000"
Desc:	control the 64K region from E0000h to E0FFFh
----------S0000026D--------------------------
MSR 0000026Dh - Pentium Pro - "MTRRfix4K_E8000"
Desc:	control the 64K region from E8000h to E8FFFh
----------S0000026E--------------------------
MSR 0000026Eh - Pentium Pro - "MTRRfix4K_F0000"
Desc:	control the 64K region from F0000h to F0FFFh
----------S0000026F--------------------------
MSR 0000026Fh - Pentium Pro - "MTRRfix4K_F8000"
Desc:	control the 64K region from F8000h to F8FFFh
----------S00000277--------------------------
MSR 00000277h - Pentium Pro - Page Attribute Table
----------S00000280--------------------------
MSR 00000280h - PentiumII - ???
----------S000002FF--------------------------
MSR 000002FFh - Pentium Pro - "MTRRdefType" - DEFAULT MEMORY TYPE
Note:	this MSR sets the memory type to use for any range not claimed by one
	  of the other MTRRs
SeeAlso: MSR 000000FEh,MSR 00000200h,MSR 00000250h

Bitfields for Pentium Pro MSR 000002FFh:
Bit(s)	Description	(Table R0051)
 63-12	reserved
 11	"MTRRenable" enable Memory Type Register registers
 10	Fixed MTRR enable
 9-3	reserved
 2-0	default memory type
----------S00000400--------------------------
MSR 00000400h - Pentium Pro - "MC0_CTL" Machine Check Control 0
SeeAlso: MSR 00000401h,MSR 00000402h,MSR 00000404h,MSR 0000410h
----------S00000401--------------------------
MSR 00000401h - Pentium Pro - "MC0_STATUS" Machine Check Status 0
SeeAlso: MSR 00000400h,MSR 00000403h

Bitfields for Pentium Pro Machine Check Status:
Bit(s)	Description	(Table R0052)
 63	"MC_STATUS_V"
 62	"MC_STATUS_O"
 61	"MC_STATUS_UC"
 60	"MC_STATUS_EN"
 59	"MC_STATUS_MISCV"
 58	"MC_STATUS_ADDRV"
 57	"MC_STATUS_DAM"
 56-32	reserved
 31-16	"MC_STAT_MSCOD"
 15-0	"MC_STAT_MACCOD"
----------S00000402--------------------------
MSR 00000402h - Pentium Pro - "MC0_ADDR" Machine Check Address 0
SeeAlso: MSR 00000400h,MSR 00000403h
----------S00000403--------------------------
MSR 00000403h - Pentium Pro - "MC0_MISC"
SeeAlso: MSR 00000401h,MSR 00000402h
----------S00000404--------------------------
MSR 00000404h - Pentium Pro - "MC1_CTL" Machine Check Control 1
SeeAlso: MSR 00000400h,MSR 00000408h
----------S00000405--------------------------
MSR 00000405h - Pentium Pro - "MC1_STATUS" Machine Check Status 1
----------S00000406--------------------------
MSR 00000406h - Pentium Pro - "MC1_ADDR" Machine Check Address 1
----------S00000407--------------------------
MSR 00000407h - Pentium Pro - "MC1_MISC"
----------S00000408--------------------------
MSR 00000408h - Pentium Pro - "MC2_CTL" Machine Check Control 2
SeeAlso: MSR 00000400h,MSR 00000404h,MSR 0000040Ch
----------S00000409--------------------------
MSR 00000409h - Pentium Pro - "MC2_STATUS" Machine Check Status 2
----------S0000040A--------------------------
MSR 0000040Ah - Pentium Pro - "MC2_ADDR" Machine Check Address 2
----------S0000040B--------------------------
MSR 0000040Bh - Pentium Pro - "MC2_MISC"
----------S0000040C--------------------------
MSR 0000040Ch - Pentium II - "MC4_CTL" Machine Check Control 4
SeeAlso: MSR 000040Dh,MSR 00000400h,MSR 00000404h,MSR 00000408h
----------S0000040D--------------------------
MSR 0000040Dh - Pentium II - "MC4_STATUS" Machine Check Status 4
SeeAlso: MSR 000040Ch,MSR 000040Eh
----------S0000040E--------------------------
MSR 0000040Eh - Pentium II - "MC4_ADDR" Machine Check Address 4
SeeAlso: MSR 000040Ch,MSR 000040Dh
----------S00000410--------------------------
MSR 00000410h - Pentium Pro - "MC3_CTL" Machine Check Control 3
SeeAlso: MSR 00000400h,MSR 00000404h,MSR 0000040Ch
----------S00000411--------------------------
MSR 00000411h - Pentium Pro - "MC3_STATUS" Machine Check Status 3
----------S00000412--------------------------
MSR 00000412h - Pentium Pro - "MC3_ADDR" Machine Check Address 3
----------S00000413--------------------------
MSR 00000413h - Pentium Pro - "MC3_MISC"
----------S00001000--------------------------
MSR 00001000h - IBM 386/486 SLC - PROCESSOR OPERATION REGISTER
Size:	19 bits
Access:	Read/Write
SeeAlso: MSR 00001001h,MSR 00001002h

Bitfields for IBM 386/486 SLC Processor Operation Register:
Bit(s)	Description	(Table R0053)
 63-19	reserved
 18	(486SLC only) Low Power PLA
 17	(486SLC only) Bus Read
 16	(486SLC only) Cache Parity Generate Error
 15	enable cacheability of NPX operands
 14	enable PWI ADS
 13	enable Low Power Halt Mode (HLT instruction stops CPU clock)
 12	extended Out instruction (CPU waits for READY after any output)
 11	cache reload bit
 10	enable internal KEN# signal
 9	disable cache lock mode
 8	reserved
 7	enable cache
 6	enable DBCS
 5	enable Power Interrupt
 4	enable Flush Snooping
 3	enable Snoop Input
 2	address line A20 mask (see also #02753,#P0415)
 1	enable cache parity checking
 0	Cache Parity Error occurred
SeeAlso: #R0054,#R0055
----------S00001000--------------------------
MSR 00001000h - Pentium Pro - DEBUG REGISTER 0 
SeeAlso: MSR 00001001h"Pro",MSR 00001007h"Pro"
----------S00001001--------------------------
MSR 00001001h - IBM 386/486 SLC - CACHE REGION CONTROL REGISTER
Size:	48 bits
SeeAlso: MSR 00001000h,MSR 00001002h

Bitfields for IBM 386/486 SLC Cache Region Control Register:
Bit(s)	Description	(Table R0054)
 63-48	reserved
 47-32	extended memory cache memory limit (number of 64K blocks above 1M
	  which may be cached)
 31-16	first megabyte read-only flags (each bit represents 64K)
 15-0	first megabyte cacheable flags (each bit represents 64K)
SeeAlso: #R0053,#R0055
----------S00001001--------------------------
MSR 00001001h - Pentium Pro - DEBUG REGISTER 1
SeeAlso: MSR 00001000h"Pro",MSR 00001002h"Pro"
----------S00001002--------------------------
MSR 00001002h - IBM 386/486 SLC - PROCESSOR OPERATION REGISTER
Size:	30 bits
SeeAlso: MSR 00001000h,MSR 00001001h,MSR 00001004h

Bitfields for IBM 386/486 SLC Processor Operation Register:
Bit(s)	Description	(Table R0055)
 63-30	reserved
 29	enable External Dynamic Frequency Shift
 28	Dynamic Frequency Shift ready
 27	Dynamic Frequency Shift Mode
 26-24	clocking mode
	000 clock x1
	011 clock doubler
	100 clock tripler
 23-0	reserved
SeeAlso: #R0053,#R0054
----------S00001002--------------------------
MSR 00001002h - Pentium Pro - DEBUG REGISTER 2
SeeAlso: MSR 00001001h"Pro",MSR 00001003h"Pro"
----------S00001003--------------------------
MSR 00001003h - Pentium Pro - DEBUG REGISTER 3
SeeAlso: MSR 00001002h"Pro",MSR 00001004h"Pro"
----------S00001004--------------------------
MSR 00001004h - IBM 486BL3 - PROCESSOR CONTROL REGISTER
Size:	24 bits
SeeAlso: MSR 00001000h

Bitfields for IBM 486BL3 Processor Control Register:
Bit(s)	Description	(Table R0056)
 63-24	reserved
 23	OS/2 boot (0=DD1 hardware, 1=DD0 hardware)
 22	MOV CR0,x Decode
	0: DD0, DD1A, DD1B, DD1D hardware
	1: DD1C hardware
 21	reserved
 20	Cache Low Power (DD1 only: cache disabled when not in use)
 19	reserved
 18	NOP timing
	0: 2 cycles on DD0, 3 cycles on DD1
	1: 3 cycles on DD0, 2 cycles on DD1
 17	bus pipelining for 16-bit accesses
 16-5	reserved???
 4	MOVS split
 3	power-saving cache feature
 2	reserved
 1	enable MOV CRx decode
	(reserved on DD1B, DD1C)
 0	reserved
SeeAlso: MSR 00001000h
----------S00001004--------------------------
MSR 00001004h - Pentium Pro - DEBUG REGISTER 4 
SeeAlso: MSR 00001003h"Pro",MSR 00001005h"Pro"
----------S00001005--------------------------
MSR 00001005h - Pentium Pro - DEBUG REGISTER 5 
SeeAlso: MSR 00001004h"Pro",MSR 00001006h"Pro"
----------S00001006--------------------------
MSR 00001006h - Pentium Pro - DEBUG REGISTER 6 
SeeAlso: MSR 00001005h"Pro",MSR 00001007h"Pro"
----------S00001007--------------------------
MSR 00001007h - Pentium Pro - DEBUG REGISTER 7 
SeeAlso: MSR 00001006h"Pro",MSR 00001000h"Pro",MSR 00002000h"Pro"
----------S00002000--------------------------
MSR 00002000h - Pentium Pro - CONTROL REGISTER 0
SeeAlso: MSR 00001000h"Pro",MSR 00002002h"Pro"
----------S00002002--------------------------
MSR 00002002h - Pentium Pro - CONTROL REGISTER 2
SeeAlso: MSR 00002000h"Pro",MSR 00002003h"Pro"
----------S00002003--------------------------
MSR 00002003h - Pentium Pro - CONTROL REGISTER 3
SeeAlso: MSR 00002002h"Pro",MSR 00002004h"Pro"
----------S00002004--------------------------
MSR 00002004h - Pentium Pro - CONTROL REGISTER 4
SeeAlso: MSR 00002003h"Pro",MSR 00002000h"Pro"
----------S80000000--------------------------
MSR 80000000h - Pentium - MACHINE CHECK EXCEPTION ADDRESS
Size:	64 bits
Access:	Read
SeeAlso: MSR 00000000h,MSR 80000001h
----------S80000001--------------------------
MSR 80000001h - Pentium - MACHINE CHECK EXCEPTION TYPE
Size:	6 bits
Access:	Read
SeeAlso: MSR 00000001h,MSR 80000000h
----------S80000002--------------------------
MSR 80000002h - Pentium - (TR1) PARITY REVERSAL TEST REGISTER
Size:	14 bits
Access:	Write
SeeAlso: MSR 00000002h
----------S80000003--------------------------
MSR 80000003h - Pentium - unimplemented
SeeAlso: MSR 00000003h
----------S80000004--------------------------
MSR 80000004h - Pentium - (TR2) INSTRUCTION CACHE END BITS
Size:	4 bits
Access:	Read/Write
SeeAlso: MSR 00000004h
----------S80000005--------------------------
MSR 80000005h - Pentium - (TR3) CACHE DATA TEST REGISTER
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000005h
----------S80000006--------------------------
MSR 80000006h - Pentium - (TR4) CACHE TAG
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000006h
----------S80000007--------------------------
MSR 80000007h - Pentium - (TR5) CACHE CONTROL
Size:	15 bits
Access:	Write
SeeAlso: MSR 00000007h
----------S80000008--------------------------
MSR 80000008h - Pentium - (TR6) TLB COMMAND
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000008h
----------S80000009--------------------------
MSR 80000009h - Pentium - (TR7) TLB DATA
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 00000009h
----------S8000000A--------------------------
MSR 8000000Ah O - Pentium A-step - (TR8) 36-BIT TLB DATA TEST REGISTER
Size:	4 bits
SeeAlso: MSR 0000000Ah,#R0009
----------S8000000B--------------------------
MSR 8000000Bh - Pentium - (TR9) BRANCH TARGET BUFFER TAG
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 0000000Bh
----------S8000000C--------------------------
MSR 8000000Ch - Pentium - (TR10) BRANCH TARGET BUFFER TARGET
Size:	32 bits
Access:	Read/Write
SeeAlso: MSR 0000000Ch
----------S8000000D--------------------------
MSR 8000000Dh - Pentium - (TR11) BRANCH TARGET BUFFER CONTROL
Size:	12 bits
Access:	Write
SeeAlso: MSR 0000000Dh
----------S8000000E--------------------------
MSR 8000000Eh - Pentium - (TR12) NEW FEATURE CONTROL
Size:	10 bits
Access:	Write
SeeAlso: MSR 0000000Eh
----------S8000000F--------------------------
MSR 8000000Fh - Pentium - ???
Size:	1 bit???
Access:	Write
SeeAlso: MSR 0000000Fh
----------S80000010--------------------------
MSR 80000010h - Pentium - TIME STAMP COUNTER
Size:	64 bits
Access:	Read/Write
SeeAlso: MSR 00000010h
----------S80000011--------------------------
MSR 80000011h - Pentium - EVENT COUNTER SELECTION AND CONTROL
Size:	26 bits
Access:	Read/Write
SeeAlso: MSR 00000011h,MSR 80000012h,MSR 80000013h
----------S80000012--------------------------
MSR 80000012h - Pentium - EVENT COUNTER #0
Size:	40 bits
Access:	Read/Write
SeeAlso: MSR 00000012h,MSR 80000011h,MSR 80000013h
----------S80000013--------------------------
MSR 80000013h - Pentium - EVENT COUNTER #1
Size:	40 bits
Access:	Read/Write
SeeAlso: MSR 00000013h,MSR 80000011h,MSR 80000012h
----------S80000014--------------------------
MSR 80000014h - Pentium - ???
Access:	Read
SeeAlso: MSR 00000014h
----------S80000015--------------------------
MSR 80000015h - Pentium - unimplemented???
----------S80000016--------------------------
MSR 80000016h - Pentium - unimplemented???
----------S80000017--------------------------
MSR 80000017h - Pentium - unimplemented???
----------S80000018--------------------------
MSR 80000018h - Pentium - ??? (PAGING-RELATED)
Size:	4 bits???
Access:	Read
----------S80000019--------------------------
MSR 80000019h - Pentium - FLOATING POINT - LAST PREFETCHED OPCODE
Size:	11 bits
Access:	Read
Desc:	this register stores the opcode of the last floating-point opcode to
	  be prefetched by the CPU
SeeAlso: MSR 8000001Ah,MSR 8000001Bh

Bitfields for Pentium Floating-Point Opcode:
Bit(s)	Description	(Table R0057)
 63-11	reserved (0)
 10-8	low three bits of first byte of floating-point instruction
 7-0	second byte of floating-point instruction
Note:	both a standalone FWAIT and the instruction D8h 9Bh are represented
	  as 09Bh
----------S8000001A--------------------------
MSR 8000001Ah - Pentium - FLOATING POINT - LAST NON-CONTROL OPCODE
Size:	11 bits
Access:	Read
SeeAlso: MSR 80000019h,MSR 8000001Bh,#R0057
----------S8000001B--------------------------
MSR 8000001Bh - Pentium - FLOATING POINT - LAST EXCEPTION OPCODE
Size:	11 bits
Access:	Read/Write
SeeAlso: MSR 80000019h,MSR 8000001Ah,#R0057
----------S8000001C--------------------------
MSR 8000001Ch - Pentium - ???
Size:	4 bits???
Access:	Read
----------S8000001D--------------------------
MSR 8000001Dh - Pentium - PROBE MODE CONTROL REGISTER
Size:	32 bits
Access:	Read/Write

Bitfields for Probe Mode Control Register:
Bit(s)	Description	(Table R0058)
 31	(read-only) System Management Mode is active
 30-3	reserved (0)
 2	PB1 monitors breakpoint #1 matches instead of performance counter #1
 1	PB0 monitors breakpoint #0 matches instead of performance counter #0
 0	ICEBP enabled (every debug exception enters Probe Mode)
----------S8000001E--------------------------
MSR 8000001Eh - Pentium - ???
Size:	32 bits
Access:	Read/Write
Note:	this may be nothing more than a scratchpad register
SeeAlso: MSR 8000001Fh
----------S8000001F--------------------------
MSR 8000001Fh - Pentium - ???
Size:	32 bits
Access:	Read/Write
Note:	this may be nothing more than a scratchpad register
SeeAlso: MSR 8000001Eh
----------SC0000080--------------------------
MSR C0000080h - AMD K6 - EXTENDED FEATURE ENABLE REGISTER
Size:	1 bit
SeeAlso: MSR C0000081h,MSR C0000082h

Bitfields for AMD K6 Extended Feature Enable Register:
Bit(s)	Description	(Table R0059)
 63-1	reserved
 0	system call extension (SYSCALL/SYSRET) enabled
	when disabled, both instructions generate an Undefined Opcode
	  exception
Note:	CPUID 80000001h should be checked to determine whether the SYSCALL
	  extension is implemented by the processor
SeeAlso: #R0060
----------SC0000081--------------------------
MSR C0000081h - AMD K6 - SYSCALL TARGET ADDRESS
Size:	48 bits
Note:	if SYSCALL is supported (as indicated by CPUID; SYSCALL is not
	  yet implemented in current steppings of the K6), this MSR specifies
	  the address to which the SYSCALL instruction (opcode 0Fh 05h -- same
	  as 80286 LOADALL!) transfers control, provided it has also been
	  enabled via MSR C0000080h
SeeAlso: MSR C0000080h,MSR C0000082h

Bitfields for AMD K6 SYSCALL Target Address Register:
Bit(s)	Description	(Table R0060)
 63-48	reserved
 47-32	CS and SS selector base for SYSCALL/SYSRET
 31-0	target EIP address for SYSCALL
SeeAlso: #R0059
----------SC0000082--------------------------
MSR C0000082h - AMD K6 - WRITE-HANDLING CONTROL REGISTER
Size:	9 bits
SeeAlso: MSR C0000080h,MSR C0000081h

Bitfields for AMD K6 Write-Handling Control Register:
Bit(s)	Description	(Table R0061)
 63-9	reserved
 8	write cacheability detection enabled
 7-1	write allocate enable limit (in 4M units)
	memory above this limit will not be accessed without a write-allocate
 0	write allocate enabled for 15-16M region
Note:	the Intel Triton chipset does not support write cacheability detection,
	  so bit 8 should be kept clear
--------!---CREDITS--------------------------
Christian Ludloff's 80x86.CPU
Alex V. Potemkin's Opcodes List (OPCODES.LST)
Intel Pentium Pro Family User's Guide, Volume 3, Appendix C
--------!---Admin----------------------------
Highest Table Number = R0061
--------!---FILELIST-------------------------
Please redistribute all of the files comprising the interrupt list (listed at
the beginning of the list and in INTERRUP.1ST) unmodified as a group, in a
quartet of archives named INTER60A through INTER60D (preferably the original
authenticated PKZIP archives), and the utility and hypertext conversion
programs in three additional archives called INTER60E.ZIP to INTER60G.ZIP.

Copyright (c) 1989,1990,1991,1992,1993,1994,1995,1996,1997,1998,1999 Ralf Brown
--------!---CONTACT_INFO---------------------
Internet: ralf@pobox.com (currently forwards to ralf@telerama.lm.com)
FIDO: Ralf Brown 1:129/26.1
