MEMORY MAP			Release 60		Last change 03jan99
Copyright (c) 1989,1990,1991,1992,1993,1994,1995,1996,1997,1998,1999 Ralf Brown

--------H-M00000000--------------------------
MEM 0000h:0000h R - INTERRUPT VECTOR TABLE
Size:	1024 BYTEs
Note:	see also the main interrupt list
--------b-M0000031D--------------------------
MEM 0000h:031Dh - 1989 AMI 386sx BIOS - USER-DEFINABLE TYPE 47 HARD DISK PARMS
Size:	16 BYTEs
Note:	these fields are used if the AMI BIOS setup is set to use the top of
	  the interrupt table for the extended BIOS data area
SeeAlso: MEM 0000h:032Dh,INT 41
--------b-M0000032D--------------------------
MEM 0000h:032Dh - 1989 AMI 386sx BIOS - USER-DEFINABLE TYPE 48 HARD DISK PARMS
Size:	16 BYTEs
Note:	these fields are used if the AMI BIOS setup is set to use the top of
	  the interrupt table for the extended BIOS data area
SeeAlso: MEM 0000h:031Dh,INT 46
--------B-M00000400--------------------------
MEM 0000h:0400h - BIOS DATA AREA
Size:	256 BYTEs
Note:	see also the MEM 0040h:xxxxh entries
----------M00000500--------------------------
MEM 0000h:0500h - DATA AREA
Size:	256 BYTEs
--------D-M00000600--------------------------
MEM 0000h:0600h - MS-DOS 1.x LOAD ADDRESS
--------D-M00000700--------------------------
MEM 0000h:0700h - MS-DOS 2+ LOAD ADDRESS
--------S-M00400000--------------------------
MEM 0040h:0000h - BASE I/O ADDRESS OF FIRST SERIAL I/O PORT
Size:	WORD
Notes:	the BIOS sets this word to zero if is unable to find any serial ports
	  at the addresses it is programmed to check at boot
	DOS and BIOS serial device numbers may be redefined by re-assigning
	  these values of the base I/O addresses stored here
SeeAlso: MEM 0040h:0002h,MEM 0040h:0004h,MEM 0040h:0006h,MEM 0040h:0008h
SeeAlso: MEM 0040h:007Ch,INT 14/AH=00h,PORT 03F8h"SERIAL"
--------S-M00400002--------------------------
MEM 0040h:0002h - BASE I/O ADDRESS OF SECOND SERIAL I/O PORT
Size:	WORD
Note:	the BIOS sets this word to zero if is unable to find more than one
	  serial port at the addresses it is programmed to check at boot
SeeAlso: MEM 0040h:0000h,MEM 0040h:0004h,MEM 0040h:0006h,MEM 0040h:000Ah
SeeAlso: MEM 0040h:007Dh,INT 14/AH=00h,PORT 02F8h"SERIAL"
--------S-M00400004--------------------------
MEM 0040h:0004h - BASE I/O ADDRESS OF THIRD SERIAL I/O PORT
Size:	WORD
Note:	the BIOS sets this word to zero if is unable to find more than two
	  serial ports at the addresses it is programmed to check at boot
SeeAlso: MEM 0040h:0000h,MEM 0040h:0002h,MEM 0040h:0006h,MEM 0040h:000Ch
SeeAlso: MEM 0040h:007Eh,PORT 03E8h"SERIAL"
--------S-M00400006--------------------------
MEM 0040h:0006h - BASE I/O ADDRESS OF FOURTH SERIAL I/O PORT
Size:	WORD
Note:	the BIOS sets this word to zero if is unable to find more than three
	  serial ports at the addresses it is programmed to check at boot
SeeAlso: MEM 0040h:0000h,MEM 0040h:0002h,MEM 0040h:0004h,MEM 0040h:0008h
SeeAlso: MEM 0040h:007Fh,PORT 02E8h"SERIAL"
--------P-M00400008--------------------------
MEM 0040h:0008h - BASE I/O ADDRESS OF FIRST PARALLEL I/O PORT
Size:	WORD
Notes:	the BIOS POST routine fills in the parallel port address fields in
	  turn as it finds parallel ports.  All fields beyond the last one
	  for which a valid parallel port was found are set to zero.
	the BIOS INT 17 handler uses these fields to address the parallel
	  ports
SeeAlso: MEM 0040h:0000h,MEM 0040h:000Ah,MEM 0040h:000Ch,INT 17/AH=00h
SeeAlso: PORT 0278h"PRINTER",PORT 03BCh"PRINTER"
--------P-M0040000A--------------------------
MEM 0040h:000Ah - BASE I/O ADDRESS OF SECOND PARALLEL I/O PORT
Size:	WORD
Note:	zero if fewer than two parallel ports installed
SeeAlso: MEM 0040h:0002h,MEM 0040h:0008h,MEM 0040h:000Ch,PORT 0278h"PRINTER"
SeeAlso: PORT 0378h"PRINTER",INT 17/AH=00h
--------P-M0040000C--------------------------
MEM 0040h:000Ch - BASE I/O ADDRESS OF THIRD PARALLEL I/O PORT
Size:	WORD
Note:	zero if fewer than three parallel ports installed
SeeAlso: MEM 0040h:0004h,MEM 0040h:0008h,MEM 0040h:000Ah,MEM 0040h:000Eh
SeeAlso: PORT 0378h"PRINTER",INT 17/AH=00h
--------P-M0040000E--------------------------
MEM 0040h:000Eh - BASE I/O ADDRESS OF FOURTH PARALLEL I/O PORT (pre-PS/2)
Size:	WORD
Note:	zero if fewer than four parallel ports installed
SeeAlso: MEM 0040h:0008h,MEM 0040h:000Ah,MEM 0040h:000Eh"BIOS DATA"
SeeAlso: PORT 0378h"PRINTER",INT 17/AH=00h
--------B-M0040000E--------------------------
MEM 0040h:000Eh - SEGMENT OF EXTENDED BIOS DATA SEGMENT (PS/2, newer BIOSes)
Size:	WORD
SeeAlso: MEM 0040h:000Eh"PARALLEL",INT 15/AH=C1h

Format of Extended BIOS Data Area (IBM):
Offset	Size	Description	(Table M0001)
 00h	BYTE	length of EBDA in kilobytes
 01h 15 BYTEs	reserved
 17h	BYTE	number of entries in POST error log (0-5)
 18h  5 WORDs	POST error log (each word is a POST error number)
 22h	DWORD	Pointing Device Driver entry point
 26h	BYTE	Pointing Device Flags 1 (see #M0002)
 27h	BYTE	Pointing Device Flags 2 (see #M0003)
 28h  8 BYTEs	Pointing Device Auxiliary Device Data
 30h	DWORD	Vector for INT 07h stored here during 80387 interrupt
 34h	DWORD	Vector for INT 01h stored here during INT 07h emulation
 38h	BYTE	Scratchpad for 80287/80387 interrupt code
 39h	WORD	Timer3: Watchdog timer initial count
 3Bh	BYTE	??? seen non-zero on Model 30
 3Ch	BYTE	???
 3Dh 16 BYTEs	Fixed Disk parameter table for drive 0 (for older machines
		  which don't directly support the installed drive)
 4Dh 16 BYTEs	Fixed Disk parameter table for drive 1 (for older machines
		  which don't directly support the installed drive)
 5Dh-67h	???
 68h	BYTE	cache control
		bits 7-2 unused (0)
		bit 1: CPU cache failed test
		bit 0: CPU cache disabled
 69h-6Bh	???
 6Ch	BYTE	Fixed disk: (=FFh on ESDI systems)
		    bits 7-4: Channel number 00-0Fh
		    bits 3-0: DMA arbitration level 00-0Eh
 6Dh	BYTE	???
 6Eh	WORD	current typematic setting (see INT 16/AH=03h)
 70h	BYTE	number of attached hard drives
 71h	BYTE	hard disk 16-bit DMA channel
 72h	BYTE	interrupt status for hard disk controller (1Fh on timeout)
 73h	BYTE	hard disk operation flags
		bit 7: controller issued operation-complete INT 76h
		bit 6: controller has been reset
		bits 5-0: unused (0)
 74h	DWORD	old INT 76h vector
 78h	BYTE	hard disk DMA type
		typically 44h for reads and 4Ch for writes
 79h	BYTE	status of last hard disk operation
 7Ah	BYTE	hard disk timeout counter
 7Bh-7Dh
 7Eh  8 WORDs	storage for hard disk controller status
 8Eh-E6h
 E7h	BYTE	floppy drive type
		bit 7: drive(s) present
		bits 6-2: unused (0)
		bit 1: drive 1 is 5.25" instead of 3.5"
		bit 0: drive 0 is 5.25"
 E8h  4 BYTEs	???
 ECh	BYTE	hard disk parameters flag
		bit 7: parameters loaded into EBDA
		bits 6-0: unused (0)
 EDh	BYTE	???
 EEh	BYTE	CPU family ID (03h = 386, 04h = 486, etc.) (see INT 15/AH=C9h)
 EFh	BYTE	CPU stepping (see INT 15/AH=C9h)
 F0h 39 BYTEs	???
117h	WORD	keyboard ID (see INT 16/AH=0Ah)
		(most commonly 41ABh)
119h	BYTE	???
11Ah	BYTE	non-BIOS INT 18h flag
		bits 7-1: unused (0)
		bit 0: set by BIOS before calling user INT 18h at offset 11Dh
11Bh  2 BYTE	???
11Dh	DWORD	user INT 18h vector if BIOS has re-hooked INT 18h
121h and up:	??? seen non-zero on Model 60
3F0h	BYTE	Fixed disk buffer (???)
SeeAlso: #M0004

Bitfields for Pointing Device Flags 1:
Bit(s)	Description	(Table M0002)
 7	command in progress
 6	resend byte (FAh) received
 5	acknowledge byte (FEh) received
 4	error byte (FCh) received
 3	unexpected value received
 2-0	index count for auxiliary device data at 28h
SeeAlso: #M0001,#M0003

Bitfields for Pointing Device Flags 2:
Bit(s)	Description	(Table M0003)
 7	device driver far call flag
 6-3	reserved
 2-0	package size (number of bytes received) - 1
SeeAlso: #M0001,#M0002

Format of Extended BIOS Data Area (AMI v1.00.12.AX1T):
Offset	Size	Description	(Table M0004)
 00h	BYTE	length of XBDA in kilobytes
 01h 15 BYTEs	reserved
 17h	BYTE	number of entries in POST error log (0-10)
 18h 10 BYTEs	unused???
 22h	DWORD	Pointing Device Driver entry point
 26h	BYTE	Pointing Device Flags 1 (see #M0002)
 27h	BYTE	Pointing Device Flags 2 (see #M0003)
 28h  8 BYTEs	Pointing Device Auxiliary Device Data
 30h 13 BYTEs	???
 3Dh 16 BYTEs	Fixed Disk parameter table for drive 0
 4Dh 16 BYTEs	Fixed Disk parameter table for drive 1
 5Dh 16 BYTEs	parameter table for drive 2???
 6Dh 16 BYTEs	parameter table for drive 3???
 80h 56 BYTEs?	IDE drive 0 manufacturer/model string
 B8h 41 BYTEs	AMIBIOS copyright string
 E1h		unused???
102h	WORD	??? flags
		bit 15: ???
108h	WORD	offset of IntelIDECfgTbl (IDE configuration settings) within
		  segment F000h
10Ah  2 BYTEs	???
10Ch	DWORD	pointer to routine to call for language-specific error messages
110h	WORD	offset in segment F000h of end of currently-loaded optional
		  BIOS subsystems (language, APM, etc.)
112h	WORD	offset in segment F000h of end of area avaiable for loading
		  optional BIOS subsystems
1F0h	BYTE	APM status flags
1F1h  8 BYTEs	APM power-state data for device classes 01h-06h
		bits 0-3: current power state for devices 00h-03h in class
		bits 7-4: current engaged state for devices 00h-03h in class
1F9h  4 BYTEs	APM power-state data for device classes 01h-08h (four devices
		  per class)
1FDh  3 BYTEs	???
200h 10 WORDs	POST error log
214h	???
SeeAlso: #M0001,#M0005

Format of Extended BIOS Data Area (PhoenixBIOS 4.0):
Offset	Size	Description	(Table M0005)
 00h	BYTE	length of XBDA in kilobytes
 01h 33 BYTEs	reserved
 22h	DWORD	Pointing Device Driver entry point
 26h	BYTE	Pointing Device Flags 1 (see #M0002)
 27h	BYTE	Pointing Device Flags 2 (see #M0003)
 28h  8 BYTEs	Pointing Device Auxiliary Device Data
SeeAlso: #M0001,#M0004
--------B-M00400010--------------------------
MEM 0040h:0010h - INSTALLED HARDWARE
Size:	WORD
SeeAlso: INT 11

Bitfields for BIOS-detected installed hardware:
Bit(s)	Description	(Table M0006)
 15-14	number of parallel devices
	00 or 11 sometimes used to indicate four LPT ports
 13	(Convertible, PS/2-55LS) internal modem
 12	game port installed
 11-9	number of serial devices
	000 or 111 sometimes used to indicate eight COM ports
 8	reserved
 7-6	number of floppy disk drives (minus 1)
 5-4	initial video mode
	00 EGA,VGA,PGA, or other with on-board video BIOS
	01 40x25 CGA color
	10 80x25 CGA color
	11 80x25 mono text
 3-2	(PC only) RAM on motherboard
	00 = 16K, 01 = 32K, 10 = 48K, 11 = 64K
	(some XTs) RAM on motherboard
	00 = 64K, 01 = 128K, 10 = 192K, 11 = 256K
 2	(pre-PS/2 except PC) reserved
	(PS/2, some XT clones, newer BIOSes) pointing device installed
 1	math coprocessor installed
 0	floppy disk drives are installed
	booted from floppy
--------B-M00400012--------------------------
MEM 0040h:0012h - Convertible - POST STATUS
Size:	BYTE
--------B-M00400012--------------------------
MEM 0040h:0012h U - AT - MANUFACTURING TEST INITIALIZATION FLAGS
Size:	BYTE

Bitfields for AT manufacturing test initialization flags:
Bit(s)	Description	(Table M0007)
 0	start in manufacturing test mode rather than normal operation
 1-7	unused
--------b-M00400012--------------------------
MEM 0040h:0012h - MCA - MANUFACTURING TEST
Size:	BYTE

Bitfields for MCA manufacturing test flags :
Bit(s)	Description	(Table M0008)
 7	POST flag, ???
 6-5	unused
 4	POST flag, slot 4 has adapter identifier EDAFh
 3	POST flag, 80x25 color video
 2	POST flag, ???
 1	unused
 0	manufacturing test mode rather than normal operation
--------b-M00400012--------------------------
MEM 0040h:0012h - PS/2 Model 25 - POST SYSTEM FLAG
Size:	BYTE

Bitfields for PS/2 Model 25 POST sytem flag :
Bit(s)	Description	(Table M0009)
 0	optional memory failed; memory remapped
 1	real-time clock installed
--------B-M00400013--------------------------
MEM 0040h:0013h - BASE MEMORY SIZE IN KBYTES
Size:	WORD
SeeAlso: INT 12
--------b-M00400015--------------------------
MEM 0040h:0015h - PC, XT - ADAPTER MEMORY SIZE IN KBYTES
Size:	WORD
--------b-M00400015--------------------------
MEM 0040h:0015h U - AT - MANUFACTURING TEST SCRATCH PAD
Size:	BYTE
--------K-M00400015--------------------------
MEM 0040h:0015h - Compaq Deskpro 386 - PREVIOUS SCAN CODE
Size:	BYTE
--------b-M00400016--------------------------
MEM 0040h:0016h U - AT - MANUFACTURING TEST SCRATCH PAD
Size:	BYTE
--------b-M00400016--------------------------
MEM 0040h:0016h U - PS/2 Model 30 - BIOS CONTROL FLAGS
Size:	BYTE
--------K-M00400016--------------------------
MEM 0040h:0016h - Compaq Deskpro 386 - KEYCLICK VOLUME
Size:	BYTE
Range:	00h-7Fh
--------K-M00400017--------------------------
MEM 0040h:0017h - KEYBOARD - STATUS FLAGS 1
Size:	BYTE
SeeAlso: MEM 0040h:0018h,INT 16/AH=02h,MEM 0040h:0096h

Bitfields for keyboard status flags 1:
Bit(s)	Description	(Table M0010)
 7	INSert active
 6	Caps Lock active
 5	Num Lock active
 4	Scroll Lock active
 3	either Alt pressed
 2	either Ctrl pressed
 1	Left Shift pressed
 0	Right Shift pressed
SeeAlso: #M0011,#00587
--------K-M00400018--------------------------
MEM 0040h:0018h - KEYBOARD - STATUS FLAGS 2
Size:	BYTE
SeeAlso: MEM 0040h:0017h,INT 16/AH=12h

Bitfields for keyboard status flags 2 :
Bit(s)	Description	(Table M0011)
 7	INSert pressed
 6	Caps Lock pressed
 5	Num Lock pressed
 4	Scroll Lock pressed
 3	Pause state active
 2	Sys Req pressed
 1	Left Alt pressed
 0	Left Ctrl pressed
SeeAlso: #M0010,#00588
--------K-M00400019--------------------------
MEM 0040h:0019h - KEYBOARD - ALT-nnn KEYPAD WORKSPACE
Size:	BYTE
Desc:	holds the current value of an Alt-NNN keypad sequence; when Alt is
	  released and this byte is non-zero, the appropriate character is
	  placed in the keyboard buffer
SeeAlso: INT 16/AH=00h,MEM 0040h:001Ah
--------K-M0040001A--------------------------
MEM 0040h:001Ah - KEYBOARD - POINTER TO NEXT CHARACTER IN KEYBOARD BUFFER
Size:	WORD
SeeAlso: MEM 0040h:001Ch,MEM 0040h:0080h,MEM 0040h:0082h,INT 16/AH=00h
--------K-M0040001C--------------------------
MEM 0040h:001Ch - KEYBOARD - POINTER TO FIRST FREE SLOT IN KEYBOARD BUFFER
Size:	WORD
SeeAlso: MEM 0040h:001Ah,MEM 0040h:001Eh,MEM 0040h:0080h,MEM 0040h:0082h
SeeAlso: INT 16/AH=00h
--------K-M0040001E--------------------------
MEM 0040h:001Eh - KEYBOARD - DEFAULT KEYBOARD CIRCULAR BUFFER
Size:	16 WORDs
SeeAlso: MEM 0040h:001Ah,MEM 0040h:001Ch,MEM 0040h:0080h,MEM 0040h:0082h
SeeAlso: INT 16/AH=00h,INT 16/AH=05h
--------B-M0040003E--------------------------
MEM 0040h:003Eh - DISKETTE - RECALIBRATE STATUS
Size:	BYTE
SeeAlso: MEM 0040h:003Fh,MEM 0040h:0040h,INT 13/AH=00h,INT 13/AH=11h

Bitfields for diskette recalibrate status:
Bit(s)	Description	(Table M0012)
 7	diskette hardware interrupt occurred
 6-4	reserved
 3	recalibrate diskette 3 (PC,XT only)
 2	recalibrate diskette 2 (PC,XT only)
 1	recalibrate diskette 1
 0	recalibrate diskette 0
--------B-M0040003F--------------------------
MEM 0040h:003Fh - DISKETTE - MOTOR STATUS
Size:	BYTE
SeeAlso: MEM 0040h:003Eh,MEM 0040h:0040h

Bitfields for diskette motor status:
Bit(s)	Description	(Table M0013)
 7	current operation is write or format, rather than read or verify
 6	reserved (DMA enabled on 82077)
 5-4	diskette drive number selected (0-3)
 3	diskette 3 motor on (PC,XT only)
 2	diskette 2 motor on (PC,XT only)
 1	diskette 1 motor on
 0	diskette 0 motor on
--------B-M00400040--------------------------
MEM 0040h:0040h - DISKETTE - MOTOR TURN-OFF TIMEOUT COUNT
Size:	BYTE
Desc:	number of clock ticks until diskette motor is turned off
Note:	the typical implementation of the timeout is to have the INT 08 
	  handler decrement this byte on every clock tick, and force the
	  diskette motor off if the result is equal to zero
SeeAlso: MEM 0040h:003Eh,MEM 0040h:003Fh,MEM 0040h:0041h,INT 08"IRQ0"
--------B-M00400041--------------------------
MEM 0040h:0041h - DISKETTE - LAST OPERATION STATUS
Size:	BYTE
SeeAlso: MEM 0040h:003Eh,MEM 0040h:0042h,INT 13/AH=01h

Bitfields for diskette last operation status:
Bit(s)	Description	(Table M0014)
 7	drive not ready
 6	seek error
 5	general controller failure
 4-0	error reason
	00h no error
	01h invalid request/parameter
	02h address mark not found
	03h write-protect error
	04h sector not found
	06h diskette change line active
	08h DMA overrun
	09h DMA across 64k boundary
	0Ch media type unknown
	10h CRC error on read
Note:	the following values for this byte differ somewhat from the
	  bitfield definition above:
	    30h drive does not support media sense
	    31h no media in drive
	    32h drive does not support media type
	    AAh diskette drive not ready
--------B-M00400042--------------------------
MEM 0040h:0042h - DISK - FLOPPY/HARD DRIVE STATUS/COMMAND BYTES
Size:	7 BYTEs
SeeAlso: MEM 0040h:0041h

    42h BYTE	XT: command byte to hard disk controller
		AT: write precompensation cylinder number / 4
    43h	BYTE	XT: bit 5 = drive number, bits 3-0=head number
		AT: sector count
    44h BYTE	XT: bits 6,7 = high bits of track, bits 5-0 = start sector-1
		AT: starting sector
    45h BYTE	low byte of track number
    46h BYTE	XT: sector count
		AT: high bits of track number
    47h BYTE	XT: controlbyte from HD parameters (step rate,...)
		AT: 101DHHHH, D=drive number, HHHH=head number
    48h BYTE	XT: INT 13h subfunction number
		AT: comand byte to hard disk controller
--------B-M00400042--------------------------
MEM 0040h:0042h - DISK CONTROLLER STATUS REGISTER 0
Size:	BYTE
SeeAlso: MEM 0040h:0043h

Bitfields for diskette controller status register 0:
Bit(s)	Description	(Table M0015)
 7-6	interrupt code
	00 normal completion
	01 abnormal termination during execution
	10 invalid command
	11 abnormal termination: ready line on/diskette change
 5	requested seek complete
 4	drive fault
 3	drive not ready
 2	head state at time of interrupt
 1-0	selected drive (drives 2&3 on PC,XT only)
SeeAlso: #M0016
--------B-M00400043--------------------------
MEM 0040h:0043h - DISK CONTROLLER STATUS REGISTER 1
Size:	BYTE
SeeAlso: MEM 0040h:0042h,MEM 0040h:0044h

Bitfields for diskette controller status register 0:
Bit(s)	Description	(Table M0016)
 7	attempted access beyon last cylinder
 6	unused
 5	CRC error on read
 4	DMA overrun
 3	unused
 2	data error
 1	disk write protected
 0	missing address mark
SeeAlso: #M0015,#M0017
--------B-M00400044--------------------------
MEM 0040h:0044h - DISK CONTROLLER STATUS REGISTER 2
Size:	BYTE
SeeAlso: MEM 0040h:0043h

Bitfields for diskette controller status register 0:
Bit(s)	Description	(Table M0017)
 7	unused
 6	found deleted data address mark
 5	CRC error in data field
 4	wrong cylinder number read
 3	verify equal
 2	can't find sector matching verify condition
 1	bad cylinder
 0	unable to find address mark
SeeAlso: #M0016
--------V-M00400049--------------------------
MEM 0040h:0049h - VIDEO - CURRENT VIDEO MODE
Size:	BYTE
SeeAlso: MEM 0040h:004Ah,INT 10/AH=00h
--------V-M0040004A--------------------------
MEM 0040h:004Ah - VIDEO - COLUMNS ON SCREEN
Size:	WORD
SeeAlso: MEM 0040h:0049h,MEM 0040h:004Ch,MEM 0040h:004Eh,INT 10/AH=0Fh
--------V-M0040004C--------------------------
MEM 0040h:004Ch - VIDEO - PAGE (REGEN BUFFER) SIZE IN BYTES
Size:	WORD
SeeAlso: MEM 0040h:004Ah,MEM 0040h:004Eh,MEM 0040h:0050h
--------V-M0040004E--------------------------
MEM 0040h:004Eh - VIDEO - CURRENT PAGE START ADDRESS IN REGEN BUFFER
Size:	WORD
SeeAlso: MEM 0040h:004Ch,MEM 0040h:0050h,MEM 0040h:0062h,INT 10/AH=05h
--------V-M00400050--------------------------
MEM 0040h:0050h - VIDEO - CURSOR POSITIONS
Size:	8 WORDs
Desc:	contains row and column position for the cursors on each of eight
	  video pages
SeeAlso: MEM 0040h:004Eh,MEM 0040h:0060h,INT 10/AH=02h
--------V-M00400060--------------------------
MEM 0040h:0060h - VIDEO - CURSOR TYPE
Size:	WORD	(big-endian)
Desc:	contains cursor start scan line and cursor end scan line
SeeAlso: MEM 0040h:0050h,MEM 0040h:0062h,INT 10/AH=03h
--------V-M00400062--------------------------
MEM 0040h:0062h - VIDEO - CURRENT PAGE NUMBER
Size:	BYTE
SeeAlso: MEM 0040h:004Eh,MEM 0040h:0063h,INT 10/AH=05h
--------V-M00400063--------------------------
MEM 0040h:0063h - VIDEO - CRT CONTROLLER BASE I/O PORT ADDRESS
Size:	WORD
Note:	normally 03B4h for mono and 03D4h for color video boards
SeeAlso: MEM 0040h:0065h,MEM 0040h:0066h
--------V-M00400065--------------------------
MEM 0040h:0065h - VIDEO - CURRENT MODE SELECT REGISTER
Size:	BYTE
Desc:	contains last value written to I/O port 03B8h / 03D8h
SeeAlso: MEM 0040h:0063h,MEM 0040h:0066h

Bitfields for current video mode select register:
Bit(s)	Description	(Table M0018)
 7-6	unused
 5	attribute bit 7 controls blinking instead of background
 4	mode 6 graphics in monochrome
 3	video signal enabled
 2	monochrome
 1	graphics
 0	80x25 text
--------V-M00400066--------------------------
MEM 0040h:0066h - VIDEO - CURRENT SETTING OF CGA PALETTE REGISTER
Size:	BYTE
Desc:	contains the last value written to I/O port 03D9h
SeeAlso: MEM 0040h:0063h,MEM 0040h:0065h,INT 10h/AH=0Bh/BH=01h

Bitfields for CGA palette register:
Bit(s)	Description	(Table M0019)
 7-6	unused
 5	palette (0/1)
 4	intense background colors in text mode
 3	intense border color (40x25) / background color (mode 5)
 2	red
 1	green
 0	blue
----------M00400067--------------------------
MEM 0040h:0067h - PC only - CASSETTE TIME COUNT
Size:	WORD
SeeAlso: INT 15/AH=00h
----------M00400067--------------------------
MEM 0040h:0067h - RESET RESTART ADDRESS
Size:	DWORD
Desc:	this address stores the address at which to resume execution after a
	  CPU reset (or jump to F000h:FFF0h) when certain magic values are
	  stored at 0040h:0072h or in CMOS RAM location 0Fh
SeeAlso: MEM 0040h:0072h,MEM F000h:FFF0h,CMOS 0Fh,INT 19
----------M00400069--------------------------
MEM 0040h:0069h	- CASSETTE (PC only) - CASSETTE CRC REGISTER
Size:	WORD
SeeAlso: MEM 0040h:006Bh"CASSETTE",INT 15/AH=02h
----------M00400069--------------------------
MEM 0040h:0069h - V20-XT-BIOS - KEY REPEAT
Size:	BYTE

Bitfields for V20-XT-BIOS key repeat flags:
Bit(s)	Description	(Table M0020)
 7	key repeat disabled
 6	Ctrl-Alt pressed instead of just Alt
----------M0040006B--------------------------
MEM 0040h:006Bh - CASSETTE (PC only) - LAST VALUE READ FROM CASSETTE
Size:	BYTE
SeeAlso: MEM 0040h:0069h"CASSETTE",INT 15/AH=02h
----------M0040006B--------------------------
MEM 0040h:006Bh - POST LAST UNEXPECTED INTERRUPT (XT and later)
Size:	BYTE
Desc:	this is a bitmask of IRQs which have occurred while the corresponding
	  interrupt vector points at the default system BIOS handler
	  (bit 0 = IRQ0 to bit 7 = IRQ7; bit 2 = IRQ8-15 on AT and later)
SeeAlso: INT 0F"IRQ7",INT 70"IRQ8",INT 77"IRQ15"
----------M0040006C--------------------------
MEM 0040h:006Ch - TIMER TICKS SINCE MIDNIGHT
Size:	DWORD
Desc:	updated approximately every 55 milliseconds by the BIOS INT 08 handler
SeeAlso: MEM 0040h:0070h,INT 08"IRQ0",INT 1A/AH=00h
----------M00400070--------------------------
MEM 0040h:0070h - TIMER OVERFLOW
Size:	BYTE
Desc:	non-zero if timer has counted past midnight since last call to
	  INT 1A/AH=00h
Note:	the original IBM BIOS, and thus most other BIOSes, sets this byte to
	  01h at midnight; a few (such as the Eagle PC-2) increment it each
	  time midnight is passed.  The former behavior results in lost days
	  if multiple midnights pass between "get-time" calls while the machine
	  is powered up.
SeeAlso: MEM 0040h:006Ch,INT 1A/AH=00h
--------K-M00400071--------------------------
MEM 0040h:0071h - Ctrl-Break FLAG
Size:	BYTE
Desc:	bit 7 is set when Ctrl-Break has been pressed
SeeAlso: INT 1B
----------M00400072--------------------------
MEM 0040h:0072h - POST RESET FLAG
Size:	WORD
Desc:	specify the action the BIOS should take at the beginning of the
	  power-on self-test when the machine is reset
SeeAlso: INT 19,MEM F000h:FFF0h

(Table M0021)
Values for POST reset flag:
 0000h	cold boot
 0064h	Burn-in mode
 1234h	to bypass memory test (warm boot)
 4321h	[PS/2 except Mod 25,30] to preserve memory
 5678h	[Conv] system suspended
 9ABCh	[Conv] manufacturing test mode
 ABCDh	[Conv] POST loop mode
--------B-M00400074--------------------------
MEM 0040h:0074h - FIXED DISK LAST OPERATION STATUS (except ESDI drives)
Size:	BYTE
SeeAlso: INT 13/AH=01h,INT 13h/AH=0Ah,MEM 0040h:0041h

(Table M0022)
Values for fixed disk last operation status:
 00h	no error
 01h	invalid function request
 02h	address mark not found
 03h	write protect error
 04h	sector not found
 05h	reset failed
 06h	diskette removed
 07h	drive parameter activity failed
 08h	DMA overrun
 09h	DMA data boundary error
 0Ah	bad sector flag detected
 0Bh	bad track detected
 0Ch	requested diskette media type not found
	(PS/2 or extended BIOS only) unsupported track
 0Dh	invalid number of sectors for Format
 0Eh	control data address mark detected
 0Fh	DMA arbitration level out of range
 10h	uncorrectable ECC or CRC error
 11h	ECC corrected data error
 20h	general controller failed
 40h	seek failed
 80h	time out
 AAh	drive not ready
 B0h	volume not locked in drive (INT 13 extensions)
 B1h	volume locked in drive (INT 13 extensions)
 B2h	volume not removable (INT 13 extensions)
 B3h	volume in use (INT 13 extensions)
 B4h	lock count exceeded (INT 13 extensions)
 B5h	valid eject request failed (INT 13 extensions)
 BBh	undefined error
 CCh	write fault on selected drive
 E0h	status error/error register is zero
 FFh	sense failed
SeeAlso: #00234
--------d-M00400074--------------------------
MEM 0040h:0074h - WD1002-27X SuperBIOS - TOTAL DRIVES, FIRST CONTROLLER ONLY
Size:	BYTE
SeeAlso: MEM 0040h:0075h"SuperBIOS",MEM 0040h:0076h"SuperBIOS"
--------B-M00400075--------------------------
MEM 0040h:0075h - FIXED DISK - NUMBER OF FIXED DISK DRIVES
Size:	BYTE
SeeAlso: MEM 0040h:0076h"FIXED DISK",MEM 0040h:0077h"FIXED DISK"
--------d-M00400075--------------------------
MEM 0040h:0075h - WD1002-27X SuperBIOS - TOTAL FIXED DRIVES, BOTH CONTROLLERS
Size:	BYTE
SeeAlso: MEM 0040h:0074h"SuperBIOS",MEM 0040h:0076h"SuperBIOS"
--------B-M00400076--------------------------
MEM 0040h:0076h - FIXED DISK - CONTROL BYTE    {IBM documented only for XT}
Size:	BYTE
Desc:	loaded from the disk parameter table control byte (offset 8) during
	  various hard disk operations
SeeAlso: MEM 0040h:0075h"FIXED DISK",MEM 0040h:0077h"FIXED DISK"
--------d-M00400076--------------------------
MEM 0040h:0076h - XT: hard disk controller's I/O address (Western Digital)
Size:	BYTE
--------d-M00400076--------------------------
MEM 0040h:0076h - WD1002-27X SuperBIOS - USED IN TRACK RECALCULATION
Size:	BYTE
SeeAlso: MEM 0040h:0074h"SuperBIOS",MEM 0040h:0075h"SuperBIOS"
SeeAlso: MEM 0040h:0077h"SuperBIOS"
--------B-M00400077--------------------------
MEM 0040h:0077h	- FIXED DISK - I/O port offset {IBM documented only for XT}
Size:	BYTE
SeeAlso: MEM 0040h:0075h"FIXED DISK",MEM 0040h:0076h"FIXED DISK"
--------d-M00400077--------------------------
MEM 0040h:0077h - WD1002-27X SuperBIOS - USED IN TRACK RECALCULATION
Size:	BYTE
SeeAlso: MEM 0040h:0076h"SuperBIOS"
--------B-M00400078--------------------------
MEM 0040h:0078h - PARALLEL DEVICE 1 TIME-OUT COUNTER
Size:	BYTE
SeeAlso: MEM 0040h:0079h,MEM 0040h:007Ah,INT 17/AH=00h
--------B-M00400079--------------------------
MEM 0040h:0079h - PARALLEL DEVICE 2 TIME-OUT COUNTER
Size:	BYTE
SeeAlso: MEM 0040h:0078h,MEM 0040h:007Ah,INT 17/AH=00h
--------B-M0040007A--------------------------
MEM 0040h:007Ah - PARALLEL DEVICE 3 TIME-OUT COUNTER
Size:	BYTE
SeeAlso: MEM 0040h:0078h,MEM 0040h:0079h,MEM 0040h:007Bh"PARALLEL"
--------B-M0040007B--------------------------
MEM 0040h:007Bh - PARALLEL DEVICE 4 TIME-OUT COUNTER (pre-PS, PS Models 25,30)
Size:	BYTE
SeeAlso: MEM 0040h:0078h,MEM 0040h:007Ah,MEM 0040h:007Bh"INT 4Bh"
--------m-M0040007B--------------------------
MEM 0040h:007Bh - INT 4Bh FLAGS (PS2 and newer)
Size:	BYTE
SeeAlso: INT 4B/AX=8102h

Bitfields for INT 4Bh flags:
Bit(s)	Description	(Table M0023)
 7-6	reserved
 5	set if Virtual DMA Spec supported [PS] (see INT 4B)
 4	reserved
 3	set if INT 4Bh intercepted and must be chained
 2	reserved
 1	set if Generic SCSI CBIOS services available on INT 4Bh
 0	reserved
--------B-M0040007C--------------------------
MEM 0040h:007Ch - SERIAL DEVICE 1 TIMEOUT COUNTER
Size:	BYTE
SeeAlso: MEM 0040h:0000h,MEM 0040h:007Dh,MEM 0040h:007Eh,MEM 0040h:007Fh
SeeAlso: INT 14/AH=01h
--------B-M0040007D--------------------------
MEM 0040h:007Dh - SERIAL DEVICE 2 TIMEOUT COUNTER
Size:	BYTE
SeeAlso: MEM 0040h:0002h,MEM 0040h:007Ch,MEM 0040h:007Eh,MEM 0040h:007Fh
SeeAlso: INT 14/AH=01h
--------B-M0040007E--------------------------
MEM 0040h:007Eh - SERIAL DEVICE 3 TIMEOUT COUNTER
Size:	BYTE
SeeAlso: MEM 0040h:0004h,MEM 0040h:007Ch,MEM 0040h:007Dh,MEM 0040h:007Fh
SeeAlso: INT 14/AH=01h
--------B-M0040007F--------------------------
MEM 0040h:007Fh - SERIAL DEVICE 4 TIMEOUT COUNTER
Size:	BYTE
SeeAlso: MEM 0040h:0006h,MEM 0040h:007Ch,MEM 0040h:007Dh,MEM 0040h:007Eh
SeeAlso: INT 14/AH=01h
--------K-M00400080--------------------------
MEM 0040h:0080h - KEYBOARD BUFFER START OFFSET FROM SEGMENT 40h (normally 1Eh)
Size:	WORD
SeeAlso: MEM 0040h:001Ah,MEM 0040h:001Eh,MEM 0040h:0082h,INT 16/AH=05h
--------K-M00400082--------------------------
MEM 0040h:0082h - KEYBOARD BUFFER END+1 OFFSET FROM SEGMENT 40h (normally 3Eh)
Size:	WORD
Note:	XT BIOS dated 11/08/82 ends here
SeeAlso: MEM 0040h:001Ch,MEM 0040h:003Eh,MEM 0040h:0080h,INT 16/AH=05h
--------V-M00400084--------------------------
MEM 0040h:0084h - VIDEO (EGA/MCGA/VGA) - ROWS ON SCREEN MINUS ONE
Size:	BYTE
SeeAlso: MEM 0040h:0085h,INT 10/AX=1100h
--------V-M00400085--------------------------
MEM 0040h:0085h - VIDEO (EGA/MCGA/VGA) - CHARACTER HEIGHT IN SCAN-LINES
Size:	WORD
SeeAlso: MEM 0040h:0084h
--------V-M00400087--------------------------
MEM 0040h:0087h - VIDEO (EGA/VGA) CONTROL: [MCGA: =00h]
Size:	BYTE
SeeAlso: MEM 0040h:0084h,MEM 0040h:0085h,MEM 0040h:0088h

Bitfields for EGA/VGA Video control flags:
Bit(s)	Description	(Table M0024)
 7	do not to clear RAM on mode set (see INT 10h, AH=00h)
 6-5	RAM on adapter = (this field + 1) * 64K
 4	reserved
 3	EGA/VGA video system INactive
 2	wait for display enable
 1	mono monitor
 0	alphanumeric cursor emulation DISabled
	When enabled, text mode cursor size (INT 10,AH=01h) settings looking
	 like CGA ones are translated to equivalent EGA/VGA ones.
--------V-M00400088--------------------------
MEM 0040h:0088h - VIDEO (EGA/VGA) SWITCHES: [MCGA: reserved]
Size:	BYTE
SeeAlso: MEM 0040h:0087h,MEM 0040h:0089h

Bitfields for EGA/VGA Video switches:
Bit(s)	Description	(Table M0025)
 7-4	power-on state of feature connector bits 3-0
 3-0	configuration switches 4-1 (=0 on, =1 off) (see #M0026)
Note:	when bit 4 of 0040h:0089h is 0, VGA emulates 350-line EGA if this
	  byte is x3h or x9h, otherwise emulates 200-line CGA in 400-line
	  double scan. VGA resets this byte to x9h after the mode set.
	See also note for 0040h:0089h.

(Table M0026)
Values for EGA/VGA configuration switches:
 00h Pri MDA,				Sec EGA+old color display 40 x 25
 01h Pri MDA,				Sec EGA+old color display 80 x 25
 02h Pri MDA,				Sec EGA+ECD normal mode (CGA emul)
 03h Pri MDA,				Sec EGA+ECD enhanced mode
 04h Pri CGA 40 x 25,			Sec EGA mono display
 05h Pri CGA 80 x 25,			Sec EGA mono display
 06h Pri EGA+old color display 40 x 25, Sec MDA
 07h Pri EGA+old color display 80 x 25, Sec MDA
 08h Pri EGA+ECD normal mode (CGA emul), Sec MDA
 09h Pri EGA+ECD enhanced mode,		Sec MDA
 0Ah Pri EGA mono display,		Sec CGA 40 x 25
 0Bh Pri EGA mono display,		Sec CGA 80 x 25
SeeAlso: #M0025
--------V-M00400089--------------------------
MEM 0040h:0089h U - VIDEO (MCGA/VGA) - MODE-SET OPTION CONTROL
Size:	BYTE
SeeAlso: MEM 0040h:0087h,MEM 0040h:0088h

Bitfields for Video mode-set option control:
Bit(s)	Description	(Table M0027)
 7,4	requested scan lines
	0 0  350-line mode requested
	0 1  400-line mode at next mode set
	1 0  200-line mode requested
	1 1  reserved
	Note:	Apparently VGA BIOS mode set disregards bit 7 and uses
		  byte 40h:88h to determine 200/350 selection when bit 4
		  is zero. Presumably bit 7 is a convenience for other
		  purposes. Bit 7 is reset to zero after the mode set.
 6	display switching enabled
 5	reserved
 4	if set:	  use 400-line mode at next mode set
	if clear: [VGA] emulate EGA at next mode set
		[MCGA] emulate CGA, digital monitor, 200 lines, 8x8 text
	Note: this bit is set by the video mode set on VGA, unchanged on MCGA
 3	default palette loading DISabled at mode set
 2	mono display
 1	gray scale summing enabled
 0	[VGA] =1 if VGA active, =0 if not
	[MCGA] reserved, zero
Note:	the Tseng ET4000 BIOS v3.00 uses bits 6-4 of 88h and bits 6-5 of 89h
	  to specify graphics-mode refresh rates as follows
		88h/6		640x480:  1 for 72Hz,0 for 60Hz
		88h/5+89h/6	800x600:  00  60Hz
					  01  56Hz
					  11  72Hz
		88h/4+89h/5	1024x768: 00  interlaced
					  01  60Hz
					  10  72Hz???
					  11  70Hz
--------V-M0040008A--------------------------
MEM 0040h:008Ah U - VIDEO (MCGA/VGA) - INDEX INTO DISPLAY COMBINATION CODE TBL
Size:	BYTE
SeeAlso: INT 10/AX=1A00h,#M0039
--------*-M0040008B--------------------------
MEM 0040h:008Bh - PC, PCjr, PC/XT 11/8/82, Convertible - RESERVED
Size:	11 BYTEs
--------B-M0040008B--------------------------
MEM 0040h:008Bh - DISKETTE MEDIA CONTROL
Size:	BYTE

Bitfields for diskette media control:
Bit(s)	Description	(Table M0028)
 7-6	last data rate set by controller
	00=500kbps, 01=300kbps, 10=250kbps, 11=1Mbps
 5-4	last diskette drive step rate selected
	00=0Ch, 01=0Dh, 10=0Eh, 11=0Ah
 3-2	{data rate at start of operation}
 1-0	reserved
Note:	EHD BIOS sets this byte to 01h and never reads it back
--------B-M0040008C--------------------------
MEM 0040h:008Ch - FIXED DISK - CONTROLLER STATUS [not XT]
Size:	BYTE
SeeAlso: MEM 0040h:008Dh,MEM 0040h:008Eh
--------B-M0040008D--------------------------
MEM 0040h:008Dh - FIXED DISK - CONTROLLER ERROR STATUS [not XT]
Size:	BYTE
SeeAlso: MEM 0040h:008Ch,MEM 0040h:008Eh
--------B-M0040008E--------------------------
MEM 0040h:008Eh - FIXED DISK - INTERRUPT CONTROL [not XT]
Size:	BYTE
Note:	cleared to 00h at start of disk operation, set to FFh by IRQ14
	  handler when hard disk controller completes command
SeeAlso: MEM 0040h:008Ch,MEM 0040h:008Dh,MEM 0040h:008Fh
--------B-M0040008F--------------------------
MEM 0040h:008Fh U - DISKETTE CONTROLLER INFORMATION [not XT]
Size:	BYTE
SeeAlso: MEM 0040h:008Ch,MEM 0040h:008Dh,MEM 0040h:008Eh

Bitfields for diskette controller information:
Bit(s)	Description	(Table M0029)
 7	reserved
 6	=1 drive 1 determined
 5	=1 drive 1 is multi-rate, valid if drive determined
 4	=1 drive 1 supports 80 tracks, always valid
 3	reserved
 2	=1 drive 0 determined
 1	=1 drive 0 is multi-rate, valid if drive determined
 0	=1 drive 0 supports 80 tracks, always valid
Note:	EHD BIOS sets this byte to 01h and never alters it again
--------B-M00400090--------------------------
MEM 0040h:0090h - DISKETTE DRIVE 0 MEDIA STATE
Size:	BYTE
SeeAlso: MEM 0040h:0091h

Bitfields for diskette drive media state:
Bit(s)	Description	(Table M0030)
 7-6	data rate
	00=500kbps, 01=300kbps, 10=250kbps, 11=1Mbps
 5	double stepping required (e.g. 360kB in 1.2MB)
 4	media type established
 3	drive capable of supporting 4MB media
 2-0	on exit from BIOS, contains
	000 trying 360kB in 360kB
	001 trying 360kB in 1.2MB
	010 trying 1.2MB in 1.2MB
	011 360kB in 360kB established
	100 360kB in 1.2MB established
	101 1.2MB in 1.2MB established
	110 reserved
	111 all other formats/drives
SeeAlso: #M0031,#M0032
--------B-M00400091--------------------------
MEM 0040h:0091h - DISKETTE DRIVE 1 MEDIA STATE
Size:	BYTE
SeeAlso: MEM 0040h:0090h,#M0030
--------B-M00400092--------------------------
MEM 0040h:0092h U - DISKETTE DRIVE 0 MEDIA STATE AT START OF OPERATION
Size:	BYTE
Note:	officially "Drive 2 media state"
SeeAlso: MEM 0040h:0093h"DRIVE 1"

Bitfields for diskette drive 0 media state at start of operation:
Bit(s)	Description	(Table M0031)
 7-3 (see #M0030)
 2	multiple data rate capability determined
 1	multiple data rate capability
 0	=1 if drive has 80 tracks, =0 if 40 tracks
SeeAlso: #M0030,#M0032
--------d-M00400092--------------------------
MEM 0040h:0092h - Olivetti Quaderno - HARD DISK POWERDOWN COUNTDOWN CLOCK TICKS
Size:	BYTE
Note:	hard disk is turned off when counter reaches zero
--------B-M00400093--------------------------
MEM 0040h:0093h U - DISKETTE DRIVE 1 MEDIA STATE AT START OF OPERATION
Size:	BYTE
Note:	officially "Drive 3 media state"
SeeAlso: MEM 0040h:0092h"DRIVE 0"

Bitfields for diskette drive 1 media state at start of operation:
Bit(s)	Description	(Table M0032)
 7-3	(see #M0030)
 2	multiple data rate capability determined
 1	multiple data rate capability
 0	=1 if drive has 80 tracks, =0 if 40 tracks
--HP 100LX/200LX--
	display control status
 0	=1 if DISPCTL -K
 1	=1 if DISPCTL -C
--------B-M00400094--------------------------
MEM 0040h:0094h - DISKETTE DRIVE 0 CURRENT TRACK NUMBER
Size:	BYTE
SeeAlso: MEM 0040h:0095h
--------B-M00400095--------------------------
MEM 0040h:0095h - DISKETTE DRIVE 1 CURRENT TRACK NUMBER
Size:	BYTE
SeeAlso: MEM 0040h:0094h
--------K-M00400096--------------------------
MEM 0040h:0096h - KEYBOARD STATUS BYTE 1
Size:	BYTE
SeeAlso: MEM 0040h:0097h,INT 16/AH=11h

Bitfields for keyboard status byte 1:
Bit(s)	Description	(Table M0033)
 7	=1 read-ID in progress
 6	=1 last code read was first of two ID codes
 5	=1 force Num Lock if read-ID and enhanced keyboard
 4	=1 enhanced keyboard installed
 3	=1 Right Alt pressed
 2	=1 Right Ctrl pressed
 1	=1 last code read was E0h
 0	=1 last code read was E1h
SeeAlso: #M0034,#M0010
--------K-M00400097--------------------------
MEM 0040h:0097h - KEYBOARD STATUS BYTE 2
Size:	BYTE
SeeAlso: MEM 0040h:0096h,INT 16/AH=11h

Bitfields for keyboard status byte 2:
Bit(s)	Description	(Table M0034)
 7	=1 keyboard transmit error flag
 6	=1 LED update in progress
 5	=1 RESEND received from keyboard
 4	=1 ACK received from keyboard
 3	reserved, must be zero
 2	Caps Lock LED
 1	Num Lock LED
 0	Scroll Lock LED
SeeAlso: #M0033,#M0010
--------B-M00400098--------------------------
MEM 0040h:0098h - TIMER2 (AT, PS exc Mod 30) - PTR TO USER WAIT-COMPLETE FLAG
Size:	DWORD
Note:	(see INT 15/AX=8300h)
SeeAlso: MEM 0040h:009Ch,INT 15/AH=83h,INT 15/AH=86h
--------B-M0040009C--------------------------
MEM 0040h:009Ch - TIMER2 (AT, PS exc Mod 30) - USER WAIT COUNT IN MICROSECONDS
Size:	DWORD
SeeAlso: MEM 0040h:0098h,MEM 0040h:00A0h,INT 15/AH=83h,INT 15/AH=86h
--------V-M0040009F--------------------------
MEM 0040h:009Fh - HP 100LX/200LX - VIDEO ZOOM MODE
Size:	BYTE

(Table M0035)
Values for HP 100LX/200LX video zoom mode:
 02h	80x25 mono
 03h	80x25 color
 80h	64x18 mono
 81h	64x18 color
 82h	40x25 mono
 83h	40x25 color
 84h	40x16 mono
 85h	40x16 color
SeeAlso: INT 10/AH=D0h
--------B-M004000A0--------------------------
MEM 0040h:00A0h - TIMER2 (AT, PS exc Mod 30) - WAIT ACTIVE FLAG
Size:	BYTE
SeeAlso: MEM 0040h:009Ch,INT 15/AH=83h,INT 15/AH=86h

Bitfields for Timer2 wait active flag:
Bit(s)	Description	(Table M0036)
 7	wait time elapsed
 6-1	reserved
 0	INT 15/AH=86h has occurred
--------N-M004000A1--------------------------
MEM 0040h:00A1h - BIT 5 SET IF LAN SUPPORT PROGRAM INTERRUPT ARBITRATOR PRESENT
Size:	BYTE
Note:	DEVICE=DXMA0MOD.SYS
--------N-M004000A2--------------------------
MEM 0040h:00A2h - RESERVED FOR NETWORK ADAPTERS
Size:	6 BYTEs
--------d-M004000A4--------------------------
MEM 0040h:00A4h - PS/2 Mod 30 - SAVED FIXED DISK INTERRUPT VECTOR 
Size:	DWORD
--------V-M004000A8--------------------------
MEM 0040h:00A8h - VIDEO (EGA/MCGA/VGA) - POINTER TO VIDEO SAVE POINTER TABLE
Size:	DWORD
SeeAlso: INT 10/AH=1Ch

Format of Video Save Pointer Table [EGA/VGA/MCGA only]:
Offset	Size	Description	(Table M0037)
 00h	DWORD	ptr to Video Parameter Table
 04h	DWORD	ptr to Parameter Dynamic Save Area, else 0 [EGA/VGA only]
 08h	DWORD	ptr to Alphanumeric Character Set Override, else 0
 0Ch	DWORD	ptr to Graphics Character Set Override, else 0
 10h	DWORD	[VGA only] ptr to Secondary Save Pointer Table, must be valid
 14h	DWORD	reserved, zero
 18h	DWORD	reserved, zero
Note: table initially in ROM, copy to RAM to alter, then update 40h:A8h.
 
Format of Secondary Video Save Pointer Table [VGA only]:
Offset	Size	Description	(Table M0038)
 00h	WORD	Length of this table in bytes, including this word (1Ah)
 02h	DWORD	ptr to Display Combination Code Table, must be valid
 06h	DWORD	ptr to second Alphanumeric Character Set Override, else 0
 0Ah	DWORD	ptr to User Palette Profile Table, else 0
 0Eh	DWORD	reserved, zero
 12h	DWORD	reserved, zero
 16h	DWORD	reserved, zero
Note: table initially in ROM, copy to RAM to alter, then alter Save Ptr Table.
 
Format of Display Combination Code Table [VGA only]:
Offset	Size	Description	(Table M0039)
 00h	BYTE	Number of entries in the DCC table at offset 04h
 01h	BYTE	Version number
 02h	BYTE	Maximum display type code that can appear in DCC table
 03h	BYTE	reserved
 04h 2N BYTEs	Each pair of bytes gives a valid display combination, one
		  display type per byte (see #M0040)

(Table M0040)
Values for Display Combination display type:
 00h	 no display
 01h	 MDA with mono display
 02h	 CGA with color display
 03h	 reserved
 04h	 EGA with color display
 05h	 EGA with mono display
 06h	 Professional Graphics Controller
 07h	 VGA with mono display
 08h	 VGA with color display
 09h	 reserved
 0Ah	 MCGA with digital color display
 0Bh	 MCGA with analog mono display
 0Ch	 MCGA with analog color display
 FFh	 unrecognised video system
SeeAlso: #M0039
 
Format of Video Parameter Table [EGA, VGA only]:
Offset	Size	Description	(Table M0041)
 00h-03h	Modes 00h-03h in 200-line CGA emulation mode
 04h-0Eh	Modes 04h-0Eh
 0Fh-10h	Modes 0Fh-10h when only 64kB RAM on adapter
 11h-12h	Modes 0Fh-10h when >64kB RAM on adapter
 13h-16h	Modes 00h-03h in 350-line mode
 17h		VGA Modes 00h or 01h in 400-line mode
 18h		VGA Modes 02h or 03h in 400-line mode
 19h		VGA Mode  07h in 400-line mode
 1Ah-1Ch	VGA Modes 11h-13h
Note:	An array of 23 [EGA] or 29 [VGA] elements, each element being 64
	  bytes long.  Elements appear in the above order.
 
Format of Video Parameter Table element [EGA, VGA only]:
Offset	Size	Description	(Table M0042)
 00h	BYTE	Columns on screen		  (see 40h:4Ah)
 01h	BYTE	Rows on screen minus one	  (see 40h:84h)
 02h	BYTE	Height of character in scan lines (see 40h:85h)
 03h	WORD	Size of video buffer		  (see 40h:4Ch)
 05h  4 BYTEs	Values for Sequencer Registers 1-4
 09h	BYTE	Value for Miscellaneous Output Register
 0Ah 25 BYTEs	Values for CRTC Registers 00h-18h
 23h 20 BYTEs	Values for Attribute Controller Registers 00h-13h
 37h  9 BYTEs	Values for Graphics Controller Registers 00h-08h
 
Format of Video Parameter Table [MCGA only] {guesswork from inspection}:
Offset	Size	Description	(Table M0043)
    - 16 triplet BYTEs of R,G,B DAC info for 16 colors;
    - An array of 11 elements, each element being 32 bytes long.
	  Elements appear in the order:
		Modes 00h,01h in 200-line mode for digital displays
		Modes 00h,01h in 400-line mode for analog displays
		Modes 02h,03h in 200-line mode for digital displays
		Modes 02h,03h in 400-line mode for analog displays
		Modes 04h,05h in 200-line mode for digital displays
		Modes 04h,05h in 400-line mode for analog displays
		Mode  06h in 200-line mode for digital displays
		Mode  06h in 400-line mode for analog displays
		Mode  11h
		Mode  13h in 200-line mode for digital displays
		Mode  13h in 400-line mode for analog displays
 
Format of Video Parameter Table element [MCGA only]:
Offset	Size	Description	(Table M0044)
 00h	BYTE	Columns on screen		  (see 40h:4Ah)
 01h	BYTE	Rows on screen minus one	  (see 40h:84h)
 02h	BYTE	Height of character in scan lines (see 40h:85h)
 03h	WORD	Size of video buffer		  (see 40h:4Ch)
 05h	WORD	??? always zero
 07h 21 BYTEs	Video data registers 00h-14h to port 3D5h indexed by 3D4h
 1Ch	BYTE	PEL Mask to port 3C6h
 1Dh	BYTE	CGA Mode Control to port 3D8h
 1Eh	BYTE	CGA Border Control to port 3D9h
 1Fh	BYTE	Extended Mode Control to port 3DDh
 
Format of Video Parameter Dynamic Save Area [EGA, VGA only]:
Offset	Size	Description	(Table M0045)
 00h 16 BYTEs	Last data written to Attribute Contr. Palette Registers 0-15
 10h	BYTE	Last data written to Attribute Controller Overscan Register
 11h-FFh	Reserved
		Note: Need for table was that EGA registers were write-only.
		Note: If default values (from the Video Parameter Table) are
		      over-ridden at a mode set by the VGA User Palette Profile
		      Table, then the Dynamic Save Area is updated with the
		      default values, not the User Profile ones.
 
Format of Alphanumeric Character Set Override:
Offset	Size	Description	(Table M0046)
 00h	BYTE	Length in bytes of each character in font table
 01h	BYTE	Character generator RAM bank to load, 0=normal
 02h	WORD	Number of characters in font table, normally 256
 04h	WORD	Code of first character in font table, normally 0
 06h	DWORD	ptr to font table
 0Ah	BYTE	Displayable rows (FFh=use maximum calculated value)
 0Bh	BYTEs	Array of mode values to which this font is to pertain
	BYTE	FFh end of array
 
Format of Second Alphanumeric Character Set Override:
Offset	Size	Description	(Table M0047)
 00h	BYTE	Length in bytes of each character in font table
 01h	BYTE	Character generator RAM bank to load, normally non-zero
 02h	BYTE	reserved
 03h	DWORD	ptr to font table
 07h	BYTEs	Array of mode values to which this font is to pertain
	BYTE	FFh end of array
Note:	Authorities differ, some say same as first override above, but IBM
	  says it is as shown above
 
Format of Graphics Character Set Override:
Offset	Size	Description	(Table M0048)
 00h	BYTE	Number of displayable character rows
 01h	WORD	Length in bytes of each character in font table
 03h	DWORD	ptr to font table
 07h	BYTEs	Array of mode values to which this font is to pertain
	BYTE	FFh end of array
 
Format of User Palette Profile Table [VGA only]:
Offset	Size	Description	(Table M0049)
 00h	BYTE	Underlining: 01h=enable in all alphanumeric modes
			     00h=enable in monochrome alphanumeric modes only
			     FFh=disable in all alphanumeric modes
 01h	BYTE	reserved
 02h	WORD	reserved
 04h	WORD	Number (0-17) of Attribute Controller registers in table
 06h	WORD	Index (0-16) of first Attribute Controller register in table
 08h	DWORD	ptr to table of Attribute Controller registers to override
			Table is an array of BYTEs.
 0Ch	WORD	Number (0-256) of video DAC Color registers in table
 0Eh	WORD	Index (0-255) of first video DAC Color register in table
 10h	DWORD	ptr to table of video DAC Color registers to override
			Table is ??? triplets ??? of BYTEs???
 14h	BYTEs	array of mode values to which this profile is to pertain
	BYTE	FFh end of array
--------*-M004000AC--------------------------
MEM 0040h:00ACh - RESERVED
Size:	4 BYTEs
--------b-M004000B0--------------------------
MEM 0040h:00B0h - Phoenix 386 BIOS 1.10 10a - LOOP COUNT FOR HARD DISK TIMEOUT
Size:	BYTE
Desc:	number of times a tight software delay loop should be executed to
	  generate the sub-55ms delays used internally by the BIOS
Note:	also used for delaying when beeping due to full keyboard buffer
SeeAlso: MEM 0040h:00ECh"Dell",INT 15/AH=BCh
--------d-M004000B0--------------------------
MEM 0040h:00B0h - PTR TO 3363 OPTICAL DISK DRIVER OR BIOS ENTRY POINT
Size:	DWORD
Notes:	When 3363 BIOS present, the ASCIZ signature "OPTIC "occurs 3 bytes
	  beyond this entry point
	When 3363 BIOS and 3363 File System Driver present, the ASCIZ signature
	  "FILE SYSTEM DRIVER" occurs 3 bytes beyond this entry point
--------b-M004000B0--------------------------
MEM 0040h:00B0h	- 1988 Phoenix 386 BIOS 1.10 03 - PARAMS FOR TYPE 48 HARD DISK
Size:	16 BYTEs
SeeAlso: INT 41,INT 46,MEM 0040h:00C0h"HARD DISK"
--------*-M004000B4--------------------------
MEM 0040h:00B4h	- RESERVED
Size:	WORD
--------b-M004000B5--------------------------
MEM 0040h:00B5h	- Dell 4xxDE
Size:	BYTE

Bitfields for Dell 4xxDE flags:
Bit(s)	Description	(Table M0050)
 2	??? (related to disk drives)
 5	page tables set to allow Weitek addressing in real mode
 6	Weitek math coprocessor present
----------M004000B6--------------------------
MEM 0040h:00B6h	- RESERVED FOR POST???
Size:	3 BYTEs
----------M004000B9--------------------------
MEM 0040h:00B9h - ???
Size:	7 BYTEs
--------b-M004000BC--------------------------
MEM 0040h:00BCh - 1993 Phoenix 486 BIOS 1.03 PCI - CPU TYPE/MASK REVISION
Size:	WORD
Desc:	the high byte contains the CPU type, the low byte the mask revision
	  (stepping level), as reported to the BIOS in DX by the CPU at startup
SeeAlso: INT 15/AH=C9h
--------b-M004000C0--------------------------
MEM 0040h:00C0h	- 1988 Phoenix 386 BIOS 1.10 03 - PARAMS FOR TYPE 49 HARD DISK
Size:	16 BYTEs
SeeAlso: INT 41,INT 46,MEM 0040h:00B0h"HARD DISK"
--------*-M004000C0--------------------------
MEM 0040h:00C0h	- RESERVED
Size:	14 BYTEs
--------K-M004000C2--------------------------
MEM 0040h:00C2h - AMI BIOS 1.00.12.AX1T - KEYBOARD TYPE
Size:	WORD
Desc:	this word contains an indication of the type of keyboard
	  (controller???) attached to the system
Note:	AMI's APM code checks for 4147h vs. other value (5047h seen on Intel
	  "Plato" motherboard)
SeeAlso: #00586,INT 16/AH=F2h
--------b-M004000CE--------------------------
MEM 0040h:00CEh	- COUNT OF DAYS SINCE LAST BOOT
Size:	WORD
--------*-M004000D0--------------------------
MEM 0040h:00D0h - RESERVED
Size:	32 BYTEs
--------S-M004000D0--------------------------
MEM 0040h:00D0h	- Digiboard MV/4 - LENGTH OF DATA TABLE
Size:	BYTE
--------d-M004000D0--------------------------
MEM 0040h:00D0h	EHD floppy - INSTALLATION FLAGS
Size:	BYTE

Bitfields for EHD floppy installation flags:
Bit(s)	Description	(Table M0051)
 4	installation completed
 3-0	drives 0-3
--------b-M004000D0--------------------------
MEM 0040h:00D0h	- AMI BIOS v1.00.12.AX1T - EPP - SCRATCH SPACE
Size:	WORD
Desc:	this word holds the value of BX during an EPP BIOS call
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00D5h"AMI",MEM 0040h:00D6h"AMI"
SeeAlso: MEM 0040h:00DDh"AMI"
--------S-M004000D1--------------------------
MEM 0040h:00D1h	- Digiboard MV/4 - PRODUCT ID
Size:	BYTE
--------S-M004000D2--------------------------
MEM 0040h:00D2h	- Digiboard MV/4 - BASE ADDRESS FOUND
Size:	WORD
--------b-M004000D2--------------------------
MEM 0040h:00D2h	- AMI BIOS v1.00.12.AX1T - EPP BASE I/O PORT
Size:	WORD
--------S-M004000D4--------------------------
MEM 0040h:00D4h	- Digiboard MV/4 - PORTS
Size:	BYTE
--------S-M004000D5--------------------------
MEM 0040h:00D5h	- Digiboard MV/4 - IRQ
Size:	BYTE
--------d-M004000D5--------------------------
MEM 0040h:00D5h	- EHD floppy - NUMBER OF FLOPPY DISK CONTROLLERS IN SYSTEM
Size:	BYTE
--------b-M004000D5--------------------------
MEM 0040h:00D5h	- AMI BIOS v1.00.12.AX1T - EPP - PARALLEL PORT 0 CAPABILITIES
Size:	BYTE
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00D6h"AMI",MEM 0040h:00D7h"AMI"
SeeAlso: MEM 0040h:00DCh"AMI"
--------d-M004000D6--------------------------
MEM 0040h:00D6h	- EHD floppy - AND-BITS TO ADJUST PORT ADDRESS
Size:	BYTE
Note:	this byte contains FFh if controller at 03Fxh and 7Fh if at 037xh; the
	  value is ANDed with DL prior to using IN A?,DX or OUT DX,A?
	  instructions
--------K-M004000D6--------------------------
MEM 0040h:00D6h - Digiboard MV/4 - NUMBER OF KEYBOARDS FOUND
Size:	WORD
SeeAlso: MEM 0040h:00D8h"Digiboard"
--------b-M004000D6--------------------------
MEM 0040h:00D6h	- AMI BIOS v1.00.12.AX1T - EPP - PARALLEL PORT 0 IRQ
Size:	BYTE
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00D5h"AMI",MEM 0040h:00D8h"AMI"
SeeAlso: MEM 0040h:00DDh"AMI"
--------d-M004000D7--------------------------
MEM 0040h:00D7h - EHD floppy - DRIVE 0 DISKETTE MEDIA STATE
Size:	BYTE
Note:	the value in this byte is copied into 0040h:0090h (diskette 0 status)
SeeAlso: MEM 0040h:00D8h"EHD",MEM 0040h:00D9h"EHD",MEM 0040h:00DAh"EHD"

Bitfields for EHD diskette media state:
Bit(s)	Description	(Table M0052)
 7-6	data rate: 00=500kbps,01=300kbps,10=250k,11=1M/S
 5	double stepping required (e.g. 360kB in 1.2MB)
 4	media type established
 3	reserved
 2-0	on exit from BIOS, contains:
	000 trying 360kB in 360kB
	001 trying 360kB in 1.2MB
	010 trying 1.2MB in 1.2MB
	011 360kB in 360kB established
	100 360kB in 1.2MB established
	101 1.2MB in 1.2MB established
	110 reserved (2M8?)
	111 all other formats/drives
--------b-M004000D7--------------------------
MEM 0040h:00D7h	- AMI BIOS v1.00.12.AX1T - EPP - PARALLEL PORT 1 CAPABILITIES
Size:	BYTE
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00D5h"AMI",MEM 0040h:00D6h"AMI"
SeeAlso: MEM 0040h:00DDh"AMI"
--------M-M004000D8--------------------------
MEM 0040h:00D8h - Digiboard MV/4 - NUMBER OF MICE FOUND
Size:	WORD
SeeAlso: MEM 0040h:00D6h"Digiboard",MEM 0040h:00DAh"Digiboard"
--------d-M004000D8--------------------------
MEM 0040h:00D8h - EHD floppy - DRIVE 1 DISKETTE MEDIA STATE
Size:	BYTE
SeeAlso: MEM 0040h:00D7h"EHD",MEM 0040h:00D9h"EHD",MEM 0040h:00DAh"EHD"
--------b-M004000D8--------------------------
MEM 0040h:00D8h - AMI BIOS v1.00.12.AX1T - EPP - PARALLEL PORT 1 IRQ
Size:	BYTE
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00D6h"AMI",MEM 0040h:00D7h"AMI"
SeeAlso: MEM 0040h:00DDh"AMI"
--------b-M004000D8--------------------------
MEM 0040h:00D8h U - Phoenix BIOS 4.0 Rel 6.0 - POWER MANAGEMENT FLAGS
Size:	BYTE
SeeAlso: INT 15/AX=5300h
--------d-M004000D9--------------------------
MEM 0040h:00D9h - EHD floppy - DRIVE 2 DISKETTE MEDIA STATE
Size:	BYTE
SeeAlso: MEM 0040h:00D7h"EHD",MEM 0040h:00D8h"EHD",MEM 0040h:00DAh"EHD"
--------S-M004000DA--------------------------
MEM 0040h:00DAh - Digiboard MV/4 - CURRENT PORT (used by VGA initializatn only)
Size:	BYTE
SeeAlso: MEM 0040h:00D8h"Digiboard"
--------d-M004000DA--------------------------
MEM 0040h:00DAh - EHD floppy - DRIVE 3 DISKETTE MEDIA STATE
Size:	BYTE
SeeAlso: MEM 0040h:00D7h"EHD",MEM 0040h:00D8h"EHD",MEM 0040h:00D9h"EHD"
--------S-M004000DB--------------------------
MEM 0040h:00DBh - Digiboard MV/4 - MASTER 8259 MASK (used by VGA init only)
Size:	BYTE
SeeAlso: MEM 0040h:00DCh"Digiboard"
--------d-M004000DB--------------------------
MEM 0040h:00DBh - EHD floppy - DRIVE 0 NEEDS RECALIBARATION
Size:	BYTE
SeeAlso: MEM 0040h:00DCh"EHD",MEM 0040h:00DDh"EHD",MEM 0040h:00DEh"EHD"
--------S-M004000DC--------------------------
MEM 0040h:00DCh - Digiboard MV/4 - SLAVE 8259 MASK (used by VGA init only)
Size:	BYTE
SeeAlso: MEM 0040h:00DBh"Digiboard"
--------b-M004000DC--------------------------
MEM 0040h:00DCh	- AMI BIOS v1.00.12.AX1T - EPP - PARALLEL PORT 0 MODE
Size:	BYTE
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00D5h"AMI",MEM 0040h:00DDh"AMI"
SeeAlso: INT 17/AX=0200h/BX=5050h

(Table M0053)
Values for AMI Enhanced Parallel Port mode:
 01h	compatibility mode
 02h	bi-directional mode
 04h	EPP mode
SeeAlso: #00637
--------d-M004000DC--------------------------
MEM 0040h:00DCh - EHD floppy - DRIVE 1 NEEDS RECALIBARATION
Size:	BYTE
SeeAlso: MEM 0040h:00DBh"EHD",MEM 0040h:00DDh"EHD",MEM 0040h:00DEh"EHD"
--------b-M004000DC--------------------------
MEM 0040h:00DCh	- AMI BIOS v1.00.12.AX1T - EPP - PARALLEL PORT 1 MODE
Size:	BYTE
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00DCh"AMI",#M0053
--------d-M004000DD--------------------------
MEM 0040h:00DDh - EHD floppy - DRIVE 2 NEEDS RECALIBARATION
Size:	BYTE
SeeAlso: MEM 0040h:00DBh"EHD",MEM 0040h:00DCh"EHD",MEM 0040h:00DEh"EHD"
--------d-M004000DE--------------------------
MEM 0040h:00DEh - EHD floppy - DRIVE 3 NEEDS RECALIBARATION
Size:	BYTE
SeeAlso: MEM 0040h:00DBh"EHD",MEM 0040h:00DCh"EHD",MEM 0040h:00DDh"EHD"
--------b-M004000DF--------------------------
MEM 0040h:00DFh	- AMI BIOS v1.00.12.AX1T - EPP - PARALLEL PORT LOCK STATE
Size:	BYTE
Note:	set to 01h if last request was to lock a port, 00h if last request was
	  to unlock a port
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00DCh"AMI"
--------b-M004000E0--------------------------
MEM 0040h:00E0h	- AMI BIOS v1.00.12.AX1T - EPP - REAL-TIME DEVICE COUNT
Size:	BYTE
Desc:	contains the number of advertised real-time devices as set by EPP
	  function 12h (see #00632)
SeeAlso: MEM 0040h:00D2h"AMI",MEM 0040h:00DFh"AMI"
--------b-M004000E0--------------------------
MEM 0040h:00E0h - Phoenix 386 BIOS - DRIVE PARAMETER TABLE FOR FIRST HARD DISK
Size:	16 BYTEs
Note:	this area is used to store the driver parameter table for the first
	  hard disk if it has been setup as the user-configurable "type 47"
--------d-M004000E3--------------------------
MEM 0040h:00E3h - EHD floppy - DRIVE 0 DISKETTE TYPE (from jumpers)
Size:	BYTE
SeeAlso: MEM 0040h:00E4h,MEM 0040h:00E5h"EHD",MEM 0040h:00E6h"EHD"

(Table M0054)
Values for EHD floppy diskette type:
 01h	undefined by diskette change (360K)
 02h	1.2M
 03h	720K
 04h	1.44M
 05h	2.88M
--------d-M004000E4--------------------------
MEM 0040h:00E4h - EHD floppy - DRIVE 1 DISKETTE TYPE (from jumpers)
Size:	BYTE
SeeAlso: MEM 0040h:00E3h,MEM 0040h:00E5h"EHD",MEM 0040h:00E6h"EHD"
--------d-M004000E5--------------------------
MEM 0040h:00E5h - EHD floppy - DRIVE 2 DISKETTE TYPE (from jumpers)
Size:	BYTE
SeeAlso: MEM 0040h:00E3h,MEM 0040h:00E4h"EHD",MEM 0040h:00E6h"EHD"
--------d-M004000E6--------------------------
MEM 0040h:00E6h - EHD floppy - DRIVE 3 DISKETTE TYPE (from jumpers)
Size:	BYTE
SeeAlso: MEM 0040h:00E3h,MEM 0040h:00E4h"EHD",MEM 0040h:00E5h"EHD"
--------d-M004000EA--------------------------
MEM 0040h:00EAh - Omti controller - SEGMENT OF EXTENDED BIOS DATA AREA???
Size:	WORD
Note:	drive parameter tables stored in specified segment
--------b-M004000EC--------------------------
MEM 0040h:00ECh - Dell 4xxDE BIOS A11 - LOOP COUNT FOR DELAYS
Size:	WORD
----------M004000F0--------------------------
MEM 0040h:00F0h - INTRA-APPLICATION COMMUNICATION AREA
Size:	16 BYTEs
--------B-M00500000--------------------------
MEM 0050h:0000h - PRINT-SCREEN STATUS
Size:	BYTE
--------J-M00500001--------------------------
MEM 0050h:0001h - NEC PC-9800 series - SCREEN MODE
Size:	BYTE
Note:	if bit 3 set, the screen is in high-resolution mode (start memory at
	  segment E000h instead of A000h)
--------D-M00500004--------------------------
MEM 0050h:0004h - MS-DOS - LOGICAL DRIVE FOR SINGLE-FLOPPY SYSTEM (A: / B:)
Size:	BYTE
--------A-M0050000E--------------------------
MEM 0050h:000Eh - STATE OF BREAK CHECKING AT START OF BASICA.COM EXECUTION
Size:	BYTE
--------A-M0050000F--------------------------
MEM 0050h:000Fh - BASICA VERSION FLAG
Size:	BYTE
Note:	this byte contains the value 02h if BASICA v2.10 is running
--------A-M00500010--------------------------
MEM 0050h:0010h - POINTER TO BASIC DATA SEGMENT
Size:	WORD
--------A-M00500012--------------------------
MEM 0050h:0012h - INT 08 VECTOR AT START OF BASICA.COM EXECUTION
Size:	DWORD
--------A-M00500016--------------------------
MEM 0050h:0016h - INT 1B VECTOR AT START OF BASICA.COM EXECUTION
Size:	DWORD
--------A-M0050001A--------------------------
MEM 0050h:001Ah - INT 24 VECTOR AT START OF BASICA.COM EXECUTION
Size:	DWORD
--------D-M00600000--------------------------
MEM 0060h:0000h - DOS 2+ SCRATCH SPACE
Size:	256 BYTEs
Note:	used during DOS 2+ boot process			   
--------D-M00600000--------------------------
MEM 0060h:0000h - DOS 1.x IO.SYS LOAD ADDRESS
--------D-M00700000--------------------------
MEM 0070h:0000h - DOS 2+ IO.SYS LOAD ADDRESS
--------D-M00700100--------------------------
MEM 0070h:0100h - DOS 5+ - ORIGINAL INTERRUPT VECTORS 10h,13h,15h,19h,1Bh
Size:	25 BYTEs
Note:	each value is stored as a BYTE for the interrupt number followed by
	  a DWORD for the vector
	these values are restored on INT 19 by recent versions of
	  DR/Novell/PC/MS-DOS (MS-DOS 3.x used this area to support HIMEM.SYS)
	not supported by OS/2 MDOS
SeeAlso: MEM 0080h:0000h,INT 2F/AH=13
--------H-M00800000--------------------------
MEM 0080h:0000h - 80286 CPU - LOADALL WORKSPACE
Size:	102 BYTEs
Desc:	on the 80286 (unlike 80386), the state buffer from which the LOADALL
	  instruction loads all internal registers is hardwired to physical
	  address 000800h
Note:	several versions 3.x of MS-DOS leave an empty space at offset 100h in
	  IO.SYS (which is loaded at 0070h:0000h) so that HIMEM.SYS can use
	  LOADALL on 80286 machines without having to save/restore the area
	  of memory that LOADALL uses
SeeAlso: MEM 0070h:0100h
--------m-m80C00000--------------------------
MEM 80C00000h - Compaq Deskpro 386 system memory board register
Size:	BYTE

80C00000  R   Diagnostics register (see #M0055)
80C00000   W  RAM relocation register (see #M0056)

Bitfields for Compaq Deskpro 386 diagnostics register:
Bit(s)	Description	(Table M0055)
 7	=0 memory expansion board is installed
 6	=0 second 1 MB of system memory board is installed
 5-4	base memory
	00 set to 640 KB
	01 invalid
	10 set to 512 KB
	11 set to 256 KB
 3	parity correct in byte 3
 2	parity correct in byte 2
 1	parity correct in byte 1
 0	parity correct in byte 0 (in 32-bit double word)
SeeAlso: #M0056

Bitfields for Compaq Deskpro 386 RAM relocation register:
Bit(s)	Description	(Table M0056)
 7-2	reserved, always write 1's.
 1	=0  Write-protect 128-Kbyte RAM at FE0000.
	=1  Do not write-protect RAM at FE0000.
 0	=0  Relocate 128-Kbyte block at FE0000 to address 0E0000
	=1  128-Kbyte RAM is addressed only at FE0000.
SeeAlso: #M0055
--------V-MA0000000--------------------------
MEM A000h:0000h - EGA+ GRAPHICS BUFFER
Size:	65536 BYTEs
--------V-MA0000000--------------------------
MEM A000h:0000h - S3 - MEMORY-MAPPED GRAPHICS PROCESSOR REGISTERS
Size:	65536 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
--------V-MA0001234--------------------------
MEM A000h:1234h - S3 - MEMORY-MAPPED ???
Size:	WORD???
Note:	the Win95 driver for the Stealth64 tests various bits in this word,
	  sometimes looping until a particular bit is set or cleared
--------V-MA0008000--------------------------
MEM A000h:8000h - S3 - MEMORY-MAPPED PCI CONFIGURATION REGISTERS
Size:	256 BYTEs
Notes:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
	additional setup may be required to access these registers via memory
	the DWORDs at 8080h,8088h,808Ch,8090h,8094h,8098h,809Ch are used by
	  STLTH64.DRV
	the DWORDs at 18080h,18088h,18090h,18094h,18098h,1809Ch are written
	  by S3_32.DLL
--------V-MA0008100--------------------------
MEM A000h:8100h - S3 - MEMORY-MAPPED PACKED REGISTERS
Size:	80 BYTEs
Access:	Write-Only
Desc:	these registers pack two 16-bit I/O registers into a single DWORD
	  for faster writes
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
SeeAlso: MEM A000h:8180h

Format of S3 Trio32/Trio64 packed memory-mapped registers:
Offset	Size	Description	(Table M0057)
8100h	DWORD	drawing control: row (low word), column (high word)
		"CUR_X" and "CUR_Y" (see PORT 82E8h,PORT 86E8h)
8104h	DWORD	(Trio64) drawing control: row 2 (low word), column 2 (high word)
8108h	DWORD	drawing control: destination Y and axial step constant (low
		  word), destination X and axial step constant (high word)
		(see PORT 8AE8h,PORT 8EE8h)
810Ch	DWORD	(Trio64 only) destination Y 2 and axial step constant 2 (low
		  word), destination X 2 and axial step constant 2 (high word)
		(see PORT 8AEAh,PORT 8EEAh)
8110h	WORD	error term (see PORT 92E8h)
8112h	WORD	(Trio64) error term 2 (see PORT 92EAh)
8114h	DWORD	unused??? (would correspond to PORT 96E8h)
8118h	WORD	drawing control: command register (see PORT 9AE8h)
811Ah	WORD	(Trio64) command register 2 (see PORT 9AEAh)
811Ch	DWORD	short stroke (see PORT 9EE8h)
8120h	DWORD	background color (see PORT A2E8h)
8124h	DWORD	foreground color (see PORT A6E8h)
8128h	DWORD	write mask (see PORT AAE8h)
812Ch	DWORD	read mask (see PORT AEE8h)
8130h	DWORD	color compare (see PORT B2E8h)
8134h	DWORD	background mix (low word) and foreground mix (high word)
		(see PORT B6E8h,PORT BAE8h)
8138h	DWORD	top scissors (low word) and left scissors (high word)
		(see PORT BEE8h,#P1047)
813Ch	DWORD	bottom scissors (low word) and right scissors (high word)
		(see PORT BEE8h,#P1047)
8140h	DWORD	data manipulation control (low word) and miscellaneous 2 (high
		  word) (see PORT BEE8h,#P1047)
8144h	DWORD	miscellaneous (low word) and read register select (high word)
		(see PORT BEE8h,#P1047)
8148h	DWORD	minor axis pixel count (low word) and major axis pixel count
		  (high word) (see PORT BEE8h,#P1047,PORT 96E8h)
814Ch	WORD	(Trio64) major axis pixel count 2 (see PORT 96EAh)
8150h	DWORD	pixel data transfer (see PORT E2E8h,PORT E2EAh)
8154h 4 DWORDs	???
8164h	DWORD	??? (written by STLTH64.DRV for Win95)
8168h	DWORD	(Trio64 only) Pattern Y (low word), Pattern X (high word)
		(see PORT EAE8h,PORT EAEAh)
816Ch	DWORD	??? (written by STLTH64.DRV for Win95)
Note:	setting 8138h to 0 and 813Ch to 12345678h may be a magic value to unlock
	  some S3 features
SeeAlso: #M0073,#M0070
--------V-MA0008180--------------------------
MEM A000h:8180h - S3 - STREAMS PROCESSOR
Size:	128 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
SeeAlso: MEM A000h:8100h,MEM A000h:FF00h

Format of S3 Streams Processor memory-mapped registers:
Offset	Size	Description	(Table M0058)
8180h	DWORD	primary stream control (see #M0059)
8184h	DWORD	chroma key control (see #M0063)
8188h	DWORD	unused??? (high word seems to echo 8184h, low word 8180h)
818Ch	DWORD	unused??? (high word seems to echo 8184h, low word 8180h)
8190h	DWORD	secondary stream control (see #M0061)
8194h	DWORD	chroma key upper bound (bits 23-0) (see also #M0063)
8198h	DWORD	secondary stream stretch (see #M0062)
819Ch	DWORD	??? (set by S3_32.DLL)
		bits 30-16: ???
		bits 14-0: ???
81A0h	DWORD	blend control (see #M0064)
81A4h 3 DWORDs	unused??? (reads as FFFFFFFFh)
81B0h 4 DWORDs	??? (appear to be read-only)
81C0h	DWORD	primary frame buffer address 0 (bits 21-0, multiple of 8)
81C4h	DWORD	primary frame buffer address 1 (bits 21-0, multiple of 8)
81C8h	DWORD	primary stream stride (bits 11-0 only)
81CCh	DWORD	double buffer/LPB control (see #M0065)
81D0h	DWORD	secondary frame buffer address 0 (bits 21-0, multiple of 8)
81D4h	DWORD	secondary frame buffer address 1 (bits 21-0, multiple of 8)
81D8h	DWORD	secondary stream stride (bits 11-0 only)
81DCh	DWORD	opaque overlay control (see #M0066)
81E0h	DWORD	K1 -- vertical stretch (lines in) (bits 10-0 only)
		set to one less than # lines in
81E4h	DWORD	K2 -- vertical stretch (stretch factor) (bits 10-0 only)
		set to -(#lines_in - #lines_out)
81E8h	DWORD	DDA vertical accumulator (bits 11-0 only) (lines out)
		set to (#lines_out) - 1
81ECh	DWORD	streams FIFO and RAS control (see #M0067)
81F0h	DWORD	primary start coordinate (see #M0068)
81F4h	DWORD	primary window size (see #M0069)
81F8h	DWORD	secondary start coordinate (see #M0068)
81FCh	DWORD	secondary window size (see #M0069)
Note:	changes to registers 81E0h-81E8h do not take effect until the next
	  VSYNC
SeeAlso: #M0073,#M0057,#M0070

Bitfields for S3 Streams Processor primary stream control:
Bit(s)	Description	(Table M0059)
 31	reserved
 30-28	filter characteristics
	000 unchanged primary stream
	001 2X stretch by replicating pixels
	010 2X stretch by interpolating horizontally (replicating vertically)
	else reserved
 27	reserved
 26-24	color mode (see #M0060)
 23-0	officially reserved, but writing nonzero values can hang display
Notes:	the primary stream is the output from the display RAM
	bits 26-24 correspond to CR67 color mode field (see #P0688)
SeeAlso: #M0058,#M0061

(Table M0060)
Values for S3 Streams Processor color mode:
 000b	eight bits per pixel
 001b	YCrCb 4:2:2 unsigned, range 10h-F0h (secondary stream only)
 010b	YUV 4:2:2, range 00h-FFh  (secondary stream only)
 011b	keyed high-color (1-5-5-5)
 100b	YUV 2:1:1 two's complement (secondary stream only)
 101b	high-color (5-6-5)
 110b	reserved
 111b	true-color (32bpp, high byte ignored)
SeeAlso: #M0059,#M0061

Bitfields for S3 Streams Processor secondary stream control:
Bit(s)	Description	(Table M0061)
 31	reserved
 30-28	filter characteristics
	000 unchanged secondary stream
	001 linear 0-2-4-2-0 for 1x-2x stretch
	010 bi-linear for 2x-4x stretch
	011 linear 1-2-2-2-1 for 4x+ stretch
	else reserved
 28	enable smoothing between horizontally adjacent bits (trial-and-error)
 27	reserved
 26-24	color mode (see #M0060,#M0074)
 23-12	reserved
 11-0	initial value of DDA horizontal accumulator
	set to 2*(inwidth-1)-(outwidth-1)
Notes:	the secondary stream is typically live video, but can be pointed at
	  any part of video memory
	changes to this register do not take effect until the next VSYNC
SeeAlso: #M0058,#M0059,#M0062

Bitfields for S3 Streams Processor stretch/filter constants:
Bit(s)	Description	(Table M0062)
 31-27	reserved
 26-16	K2 horizontal scaling factor (input width - output width)
 15-11	reserved
 10-0	K1 horizontal scaling factor (input width - 1)
Note:	changes to this register do not take effect until the next VSYNC
SeeAlso: #M0061

Bitfields for S3 Streams Processor chroma-key control:
Bit(s)	Description	(Table M0063)
 31-29	reserved
 28	key control
	=1 normal color-key or chroma-key
	=0 (keyed RGB 1-5-5-5 mode only) extract key from high bit of input
	  stream; if key bit is clear, show pixel from other stream
 27	reserved
 26-24	color comparison precision
	000 compare bit 7 of R,G, and B values only
	001 compare bits 7-6
	...
	111 compare bits 7-0
 23-0	chroma-key color value
	23-16 = red or Y
	15-8 = green or U/Cb
	7-0 = blue or V/Cr
Note:	if the keyed stream is YUV or YCrCb, then this register contains the
	  lower bound and 8194h contains the upper bound of the chromakey
	  value
SeeAlso: #M0058

Bitfields for S3 Streams Processor blend control:
Bit(s)	Description	(Table M0064)
 31-27	reserved (unused)
 26-24	blend type
	000 show secondary stream (video) overlaying primary stream
	001 show primary stream overlaying secondary stream
	010 blend pri/sec. streams (dissolve, secondary intensity = full-prim.)
	011 blend pri/sec. streams
	100 reserved (blank display)
	101 show secondary stream only where chroma-key color present
	110 show secondary stream (video) unconditionally
	111 reserved (blank display)
 23-14	reserved
 13	??? (officially reserved, but set by S3_32.DLL)
 12-8	primary stream intensity (00h-1Ch, must be multiple of 4)
 4-0	secondary stream intensity (00h-1Ch, must be multiple of 4)
	(ignored for blend type 010)
Notes:	for blend type 011, the primary and secondary stream intensities should
	  not total more than 20h to avoid wraparounds which appear as
	  incorrect colors; for blend type 010, the secondary stream intensity
	  is automatically computed as 20h - bits12-8
	changes to this register do not take effect until the next VSYNC
SeeAlso: #M0058

Bitfields for S3 Streams Processor double-buffer/LPB control:
Bit(s)	Description	(Table M0065)
 31-7	reserved (unused; all but bit 7 appear to be read-only, as well)
 6	LPB frame buffer auto-toggle
	if set, End-of-Frame toggles bit 4
 5	delay loading LPB input buffer select until next End-of-Frame
 4	LPB input buffer select (see #M0073)
	0 use LPB frame buffer address 0 (FF0Ch) for incoming video data
	1 use LPB frame buffer address 1 (FF10h)
 3	reserved
 2-1	secondary stream buffer select
	00 use frame buffer address 0 (81D0h)
	01 use frame buffer address 1 (81D4h)
	1x use frame buffer 0/1 (81D0h/81D4h) selected by bit 4 for secondary
	   stream and selected LPB frame buffer for LPB input
 0	primary stream buffer select
	=0 use frame buffer address 0 (81C0h)
	=1 use frame buffer address 1 (81C4h)
SeeAlso: #M0058,#M0073

Bitfields for S3 Streams Processor opaque overlay control:
Bit(s)	Description	(Table M0066)
 31	enable opaque overlay control
 30	select top stream (0 = secondary on top, 1 = primary)
 29	reserved
 28-19	pixel resume fetch
	number of quadwords from background's left edge to position at which
	  to start fetching pixels again
 18-13	reserved
 12-3	pixel stop fetch
	number of quadwords from background's left edge to position at which
	  to stop fetching pixels
 2-0	reserved
SeeAlso: #M0058

Bitfields for S3 Streams Processor streams FIFO and RAS control register:
Bit(s)	Description	(Table M0067)
 31-22	reserved (0)
 21	skip 0.5 MCLK delay of PD[63:0] output (default = 0)
 20	skip memory arbitration for ROM cycles (default = 0)
 19	do not tristate PD[63:16] during ROM cycles (default = 0)
	(set by Win95 driver when using ISA bus)
 18	EDO wait state control (LPB memory cycles only)
	=0 two-cycle accesses
	=1 one-cycle EDO accesses
 17	reserved
 16	RAS# pre-charge control
	=0 use CR68(bit3) setting (2.5/3.5 MCLKs)
	=1 1.5 MCLKs
 15	RAS# low control
	=0 use CR68(bit2) setting (3.5/4.5 MCLKs)
	=1 2.5 MCLKs
 14-10	primary stream FIFO threshold
	number of filled quadword slots at which to request refilling
 9-5	secondary stream FIFO threshold
	number of filled quadword slots at which to request refilling
 4-0	FIFO allocation, in quadword slots
	00000 primary stream = 24, secondary = 0
	01000 primary stream = 16, secondary = 8
	01100 primary stream = 12, secondary = 12
	10000 primary stream = 8, secondary = 16
	11000 primary stream = 0, secondary = 24
	else reserved
SeeAlso: #M0058

Bitfields for S3 Streams Processor start coordinate:
Bit(s)	Description	(Table M0068)
 31-27	reserved (read-only)
 26-16	X coordinate (column) of upper left corner, plus 1
 15-11	reserved (read-only)
 10-0	Y coordinate (row) of upper left corner, plus 1
SeeAlso: #M0058,#M0069

Bitfields for S3 Streams Processor window size:
Bit(s)	Description	(Table M0069)
 31-27	reserved (read-only)
 26-16	width in pixels - 1
 15-11	reserved (read-only)
 10-0	height in scan lines
SeeAlso: #M0058,#M0068
--------V-MA0008200--------------------------
MEM A000h:8200h - S3 ViRGE - MEMORY-MAPPED MEMORY-PORT CONTROL REGISTERS
Size:	40 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer

Format of S3 memory-maped port control registers:
Offset	Size	Description	(Table M0070)
8200h	DWORD	FIFO control
8204h	DWORD	MIU control
8208h	DWORD	streams timeout
820Ch	DWORD	miscellaneous timeout
8210h 4 DWORDs	???
8220h	DWORD	DMA read base address
8224h	DWORD	DMA read stride width
SeeAlso: #M0057
--------V-MA00082E8--------------------------
MEM A000h:82E8h - S3 - MEMORY-MAPPED CURRENT Y POSITION REGISTER
Size:	WORD
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
SeeAlso: PORT 82E8h
--------V-MA00083B0--------------------------
MEM A000h:83B0h - S3 - MEMORY-MAPPED VGA REGISTERS
Size:	48 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
SeeAlso: PORT 03B0h,PORT 03C0h,PORT 03D0h
--------V-MA0008504--------------------------
MEM A000h:8504h - S3 ViRGE - MEMORY-MAPPED SUBSYSTEM REGISTERS
Size:	12 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer

Format of S3 memory-mapped subsystem registers:
Offset	Size	Description	(Table M0071)
8504h	DWORD	subsystem Control/Status Register (see PORT 42E8h,PORT 9AE8h)
		on read:
		    bit 13 indicates whether graphics processor is busy
		    bits 12-8 indicate number of free FIFO slots
8508h	DWORD	???
850Ch	DWORD	advanced function control (see PORT 4AE8h)
SeeAlso: #M0073,#M0057,#M0072
--------V-MA0008580--------------------------
MEM A000h:8580h - S3 - MEMORY-MAPPED DMA REGISTERS
Size:	32 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer

Format of S3 memory-mapped DMA registers:
Offset	Size	Description	(Table M0072)
8580h	DWORD	start address in system memory
8584h	DWORD	transfer length
8588h	DWORD	transfer enable
858Ch	DWORD	???
8590h	DWORD	DMA base address
8594h	DWORD	DMA write pointer
8598h	DWORD	DMA read pointer
859Ch	DWORD	DMA enable
SeeAlso: #M0057,#M0073
--------V-MA00086E8--------------------------
MEM A000h:86E8h - S3 - MEMORY-MAPPED ENHANCED REGISTERS
Size:	? BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
--------V-MA000A000--------------------------
MEM A000h:A000h - S3 - MEMORY-MAPPED COLOR PALETTE REGISTERS
Size:	448 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
--------V-MA000A4D4--------------------------
MEM A000h:A4D4h - S3 - MEMORY-MAPPED BLT-FILL REGISTERS
Size:	60 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer

A4D4h	DWORD	???
A4D8h	DWORD	???
A4DCh	DWORD	??? (set to 07FFh by S3_32.DLL)
A4E0h	DWORD	??? (set to 07FFh by S3_32.DLL)
A4E4h	DWORD	???
A4E8h	DWORD	???
A4ECh	DWORD	???
A4F0h
A4F4h	DWORD	???
A4F8h
A4FCh	DWORD	???
A500h	DWORD	???
A504h	DWORD	???
A508h	DWORD	???
A50Ch	DWORD	???
--------V-MA000A8D4--------------------------
MEM A000h:A8D4h - S3 - MEMORY-MAPPED LINE REGISTERS
Size:	172 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
--------V-MA000ACD4--------------------------
MEM A000h:ACD4h - S3 - MEMORY-MAPPED POLYGON-FILL REGISTERS
Size:	172 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
--------V-MA000B0D4--------------------------
MEM A000h:B0D4h - S3 - MEMORY-MAPPED 3D-LINE REGISTERS
Size:	172 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
--------V-MA000B4D4--------------------------
MEM A000h:B4D4h - S3 - MEMORY-MAPPED 3D-TRIANGLE REGISTERS
Size:	172 BYTEs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
--------V-MA000FF00--------------------------
MEM A000h:FF00h - S3 - MEM-MAPPED "SCENIC HIGHWAY" (Local Periph. Bus) ACCESS
Size:	64 DWORDs
Note:	the S3 graphics processor registers can be mapped at either
	  linear 000A0000h or at offset 16M from the start of the linear
	  frame buffer
SeeAlso: MEM A000h:8180h

Format of S3 Local Peripheral Bus memory-mapped registers:
Offset	Size	Description	(Table M0073)
FF00h	DWORD	LPB mode (see #M0074)
FF04h	DWORD	LPB FIFO status (see #M0075)
FF08h	DWORD	interrupt status (see #M0076)
FF0Ch	DWORD	frame buffer address 0 (bits 21-0, multiple of 8)
		offset within frame buffer at which to store incoming data from
		  LPB when Streams Processor double-buffer control (see #M0065)
		  bit 4 clear
FF10h	DWORD	frame buffer address 1 (bits 21-0, multiple of 8)
		offset within frame buffer at which to store incoming data from
		  LPB when Streams Processor double-buffer control (see #M0065)
		  bit 4 is set
FF14h	DWORD	"direct address" = index for FF18h (see #M0077)
FF18h	DWORD	"direct data" (see #M0077)
		Note: the direct address/direct data registers presumably rely
		  on the attached device inserting data into the digital video
		  stream, as on a Diamond Stealth64 Video, the "direct data"
		  appears to reflect the video stream data (i.e. it varies, but
		  with a pattern that depends on the video image, and stops
		  varying when video is frozen)
FF1Ch	DWORD	general purpose I/O (see #M0078)
FF20h	DWORD	LPB serial port -- I2C/DDC access (see #M0079)
FF24h	DWORD	input window size (high word = rows, low word = columns)
FF28h	DWORD	data offsets
		(video alignment; high word = rows ; low word = columns)
FF2Ch	DWORD	horizontal decimation
		bits 0-31 set indicate that bytes 0-31 (mod 32)
		  of each line should be dropped (in Video16 mode, each bit
		  controls a WORD); decimation is aligned with the start of
		  line as specified by the data offsets at FF28h
FF30h	DWORD	vertical decimation
		bits 0-31 set indicate that lines 0-31 (mod 32) should be
		  dropped, i.e. setting this DWORD to 55555555h will drop
		  every other line; decimation starts with VSYNC regardless
		  of the data offsets specified at FF28h
FF34h	DWORD	line stride (number of bytes between starts of successive lines
		  of video data)
		must be multiple of 4 -- lowest two bits forced to 0
FF38h	3 DWORDs unused??? (seem to echo FF34h)
FF40h 8 DWORDs	LPB output FIFO - data transfer
		writing to ANY of these DWORDs transfers a value to the FIFO;
		  this organization allows use of a REP MOVSD instruction to
		  fill the FIFO
		on ISA bus, there must be a delay between successive writes
SeeAlso: #M0058

Bitfields for S3 Local Peripheral Bus LPB Mode register:
Bit(s)	Description	(Table M0074)
 0	enable LPB
 3-1	LPB operational mode
	000 Scenic/MX2
	001 Video 16 (PCI only)
	010 Video 8 In
		used by Philips SAA7110/SAA7111 and Diamond's DTV1100
	011 Video 8 In/Out
		used by CL-480
	100 Pass-Through
		send FIFO data written by CPU through the decimation logic
	else reserved (Trio64V+)
 4	LBP Reset
	pulse this bit before changing operational mode
 5	skip every other frame
	=0 write all received frames to memory
 6	disable byte-swapping
	=0 incoming 8-bit video is in order U, Y0, V, Y1 (CL-480)
	=1 incoming 8-bit video is in order Y0, U, Y1, V (SAA711x)
	(refer to bit 26 below)
 8-7	officially reserved
 7	??? messes up video image when set
 9	LPB vertical sync input polarity
	=0 active low
	=1 active high
 10	LPB horizontal sync input polarity
	=0 active low
	=1 active high
 11	(write-only) CPU VSYNC
	writing a 1 makes Trio act as if LPB VSYNC had been received
 12	(write-only) CPU HSYNC
	writing a 1 makes Trio act as if LPB HSYNC had been received
 13	(write-only) load base address
	writing a 1 causes an immediate load of the currently active base
	  address
 15-14	reserved
 17-16	maximum compressed data burst, LPB to Scenic/MX2
	00 one DWORD
	01 two DWORDs
	10 three DWORDs
	11 burst until empty (must ensure that MX2's 8-entry FIFO is not
	  overrun)
 20-18	reserved
 22-21	video FIFO threshold
	number of filled slots at which to request that Trio's memory manager
	  begin to empty the FIFO (00 = one slot, 01 = two slots, 10 = four
	  slots, 11 = six slots)
 23	reserved (read-only)
 24	LPB clock source
	=0 driven by SCLK (Pin194) (for Trio64-compatibility mode)
	=1 driven by LCLK (Pin148) (default)
 25	don't add line stride after first HSYNC within VSYNC
	must be set if first HSYNC occurs before VSYNC goes active
 26	invert LCLK (only has effect if bit 24 set)
 27	reserved
 28	(not yet on Trio64V+) current odd/even video field status
 29	(not yet on Trio64V+) field inversion - when set, the LPB's FIELD pin
	  state is inverted before being reported in bit 28
 30	reserved
 31	(read-only) current state of CFLEVEL input (Pin182) in Video In/Out
	  mode (refer to bits 3-1)
SeeAlso: #M0073

Bitfields for S3 Local Peripheral Bus LPB FIFO status:
Bit(s)	Description	(Table M0075)
 31	video FIFO 1 is almost empty (has exactly one full slot)
 30	video FIFO 1 is empty
 29	video FIFO 1 is full
 28-23	reserved
 22	video FIFO 0 is almost empty (has exactly one full slot)
 21	video FIFO 0 is empty
 20	video FIFO 0 is full
 19-14	reserved
 13	output FIFO is almost empty (has exactly one full slot)
 12	output FIFO is empty
 11	output FIFO is full
 10-4	reserved
 3-0	number of free four-byte slots in FIFO (there are 8 slots)
SeeAlso: #M0073,#M0076

Bitfields for S3 Local Peripheral Bus interrupt status:
Bit(s)	Description	(Table M0076)
 31-25	reserved
 24	drive serial port clock line low on receipt of start condition
	(causes I2C wait states until interrupt handler responds to start cond)
 23-20	reserved
 19	enable interrupt on I2C start condition detection
 18	enable interrupt on end of frame (VSYNC received)
 17	enable interrupt on end of line (HSYNC received)
 16	enable interrupt on LPB output FIFO empty
 15-4	reserved
 3	serial port detected I2C start condition
 2	VSYNC received (end of frame)
 1	HSYNC received (end of line)
 0	LPB output FIFO emptied
Note:	bits 3-0 are write-clear: writing a 1 to a bit resets it
SeeAlso: #M0073,#P0721

(Table M0077)
Values for S3 Local Peripheral Bus "direct address" index:
 0000h CP3 installation (FF18h reads 00C3h if installed)
 0001h ?
 0002h ?
 0003h ?
	bit 7: ???
	bits 6-0: ???
 0004h ?
 0005h ?
	bits 7-0: ???
 0020h ? (set to 107D4h, 1xxD4h by CP3.DLL))
 0028h ?
 0034h ? (set to 10000h by CP3.DLL)
 0414h ? (set by CP3.DLL)
 0500h ?
 0504h ?
 0508h ?
 050Ch ?
 0510h ?
SeeAlso: #M0073

Bitfields for S3 Local Peripheral Bus General-Purpose I/O:
Bit(s)	Description	(Table M0078)
 3-0	values to drive onto LPB GP output lines whenever CR5C is written
 7-4	values of GP input lines (read-only), latched whenever CR5C is read
 31-8	unused (read-only 0)
SeeAlso: #M0073

Bitfields for S3 Local Peripheral Bus serial-port register:
Bit(s)	Description	(Table M0079)
 0	I2C clock line [SCL] (write)
	=1 tri-state SCL, allowing other devices to pull it low
 1	I2C data line [SDA] (write)
	=1 tri-state SDA, allowing other devices to pull it low
 2	I2C clock line (read)
	this bit reflect the actual state of the SCL line
 3	I2C data line (read)
	this bit reflect the actual state of the SDA line
 4	enable I2C interface
	=0 disable bits 0/1, forcing both SCL and SDA to be tri-stated
 15-5	reserved (unused)
 20-16	mirrors of bits 4-0
	(these bits are on the data bus' byte lane 2 to make them accessible
	  via I/O port 00E2h)
Notes:	see file I2C.LST for details of the I2C device registers accessible
	  through this interface (VPX3220A for Stealth64 Video 2001TV)
	when the feature connector is disabled on the Stealth64 Video, these
	  bits are connected to the monitor's DDC data and clock lines
	the official documentation erroneously lists the mirrors in bits 12-8
	  instead of 20-16
SeeAlso: #M0073,PORT 00E2h,#P0677
--------V-MB0000000--------------------------
MEM B000h:0000h - MDA TEXT BUFFER
Size:	4096 BYTEs
--------V-MB0000000--------------------------
MEM B000h:0000h - HGC+ RAMFont-MODE TEXT BUFFER
Size:	16384 BYTEs
Note:	in RAMFont Mode 1, the memory is filled with the usual
	  character/attribute pairs; in RAMFont Mode 2, four bits of each
	  'attribute' byte is used to provide 12 bits for specifying the
	  character
--------V-MB0000000--------------------------
MEM B000h:0000h - HGC GRAPHICS BUFFER (PAGE 0)
Size:	32768 BYTEs
--------V-MB4000000--------------------------
MEM B400h:0000h - HGC+ RAMFont BUFFER
Size:	4096 BYTEs
Notes:	apparently write-only
	RAMFont Mode 1: 256 characters (8 bits each for char and attribute)
	RAMFont Mode 2: 3072 characters (12 bits for char, 4 bits for attrib)
	each character definition is 8 pixels wide (with 9th-column duplication
	  if appropriate) by 8-16 pixels high
--------V-MB8000000--------------------------
MEM B800h:0000h - CGA TEXT/GRAPHICS BUFFER
Size:	16384 BYTEs
--------V-MB8000000--------------------------
MEM B800h:0000h - EGA/VGA+ TEXT BUFFER
Size:	32768 BYTEs
--------V-MB8000000--------------------------
MEM B800h:0000h - HGC GRAPHICS BUFFER (PAGE 1)
Size:	32768 BYTEs
--------V-MBFF00000--------------------------
MEM BFF0h:0000h - ET4000/W32 ACL accelerator
Size:	169 BYTES

Format of ET4000/W32 memory-mapped registers:
Offset	Size	Description	(Table M0080)
 00h	DWORD	MMU Registers: memory base pointer register 0 (see #M0081)
 04h	DWORD	MMU Registers: memory base pointer register 1 (see #M0081)
 08h	DWORD	MMU Registers: memory base pointer register 2 (see #M0081)
 0Ch  7 BYTEs	???
 13h	BYTE	MMU Registers: MMU control register (see #M0082)
 14h 28 BYTEs	???
 30h	BYTE	Non-Queued Registers: suspend/terminate
 31h	BYTE	Non-Queued Registers: operation state (see #M0083) (write-only)
 32h	BYTE	Non-Queued Registers: sync enable
 33h	BYTE	???
 34h	BYTE	Non-Queued Registers: interrupt mask
 35h	BYTE	Non-Queued Registers: interrupt status
 36h	BYTE	Non-Queued Registers: ACL status (read-only)
		bit 1: read status (RDST) 1=ACL active, queue not empty
		bit 0: write status (WRST) 1=queue full
 37h 73 BYTEs	???
 80h	DWORD	Queued Registers: pattern address (see #M0084)
 84h	DWORD	Queued Registers: source address (see #M0084)
 88h	WORD	Queued Registers: pattern Y offset (see #M0085)
 8Ah	WORD	Queued Registers: source Y offset (see #M0085)
 8Ch	WORD	Queued Registers: destination y offset (see #M0085)
 8Eh	BYTE	Queued Registers: virtual bus size
 8Fh	BYTE	Queued Registers: X/Y direction (see #M0086)
 90h	BYTE	Queued Registers: pattern wrap (see #M0087)
 91h	BYTE	???
 92h	BYTE	Queued Registers: source wrap (see #M0087)
 93h	BYTE	???
 94h	WORD	Queued Registers: X position
 96h	WORD	Queued Registers: Y position
 98h	WORD	Queued Registers: X count (see #M0088)
 9Ah	WORD	Queued Registers: Y count (see #M0088)
 9Ch	BYTE	Queued Registers: routine control (see #M0089)
 9Dh	BYTE	Queued Registers: reload control
 9Eh	BYTE	Queued Registers: background ROP for mixing
 9Fh	BYTE	Queued Registers: foreground ROP for mixing
 A0h	DWORD	Queued Registers: destination address
 A4h	DWORD	Queued Registers: internal pattern address
 A8h	DWORD	Queued Registers: internal source address

Bitfields for ET4000/W32 memory base pointer register:
Bit(s)	Description	(Table M0081)
 31-22	reserved
 21-0	memory base pointer
SeeAlso: #M0080

Bitfields for ET4000/W32 MMU control register:
Bit(s)	Description	(Table M0082)
 7	reserved
 6-4	linear address control (LAC)
	  bit 6: MMU aperture 2
	  bit 5: MMU aperture 1
	  bit 4: MMU aperture 0
 3	reserved
 t2-0	aperture type (APT)
	  bit 2: MMU aperture 2
	  bit 1: MMU aperture 1
	  bit 0: MMU aperture 0
SeeAlso: #M0080 

Bitfields for ET4000/W32 operation state register:
Bit(s)	Description	(Table M0083)
 7-4	reserved
 3	restart operation after ACL-interruption
 2-1	reserved
 0	restore status before ACL-interruption
SeeAlso: #M0080

Bitfields for ET4000/W32 memory address register:
Bit(s)	Description	(Table M0084)
 31-22	reserved
 21-0	memory base pointer
SeeAlso: #M0080

Bitfields for ET4000/W32 offset register:
Bit(s)	Description	(Table M0085)
 15-12	reserved
 11-0	Y offset
SeeAlso: #M0080

Bitfields for ET4000/W32 X/Y direction register:
Bit(s)	Description	(Table M0086)
 7-2	reserved
 1	X direction
 0	Y direction
SeeAlso: #M0080

Bitfields for ET4000/W32 wrap register:
Bit(s)	Description	(Table M0087)
 7	reserved
 6-4	pattern Y wrap
	000 = 1 line	
	001 = 2 lines	
	010 = 4 lines	
	011 = 8 lines	
	100 = reserved
	101 = reserved
	110 = reserved
	111 = no wrap 
 3	reserved
 2-0	pattern X wrap
	000 = reserved	
	001 = reserved	
	010 = 4 byte	
	011 = 8 byte	
	100 = 16 byte	
	101 = 32 byte	
	110 = 64 byte	
	111 = no wrap	
SeeAlso: #M0080

Bitfields for ET4000/W32 count register:
Bit(s)	Description	(Table M0088)
 15-12	reserved
 11-0	pixel count
SeeAlso: #M0080

Bitfields for ET4000/W32 routine control register:
Bit(s)	Description	(Table M0089)
 7-6	reserved			   
 5-4	routing of CPU address (ADRO)	   
	00 don't use CPU address	   
	01 CPU address is destination	
	10 reserved			   
	11 reserved			   
 3	reserved			   
 2-0	routing of CPU data (DARQ)	   
	000 don't use CPU data	   
	001 CPU data is source data	   
	010 CPU data is mixed data	   
	011 reserved			   
	100 CPU data is x-count	   
	101 CPU data is y-count	   
	10x reserved			
SeeAlso: #M0080 
--------V-MC0000000--------------------------
MEM C000h:0000h - VIDEO BIOS (EGA and newer)
Size:	varies (usually 16K-24K for EGA, 24K-32K for VGA)
--------h-mC0000000--------------------------
MEM C0000000h -	Weitek "Abacus" math coprocessor
Size:	4096 BYTEs
--------B-MC8000000--------------------------
MEM C800h:0000h - HARD DISK BIOS
Size:	varies (usually 8K or 16K)
--------V-MC8001C00--------------------------
MEM C800h:1C00h - IBM XGA, XGA/A - MEMORY-MAPPED REGISTERS
Range:	any 8K boundary within segments C000h to DFFFh
Notes:	The XGA memory mapped registers can be assigned to the last 1K block in
	  in each 8K block in the range of C0000h-DFFFFh; the base offset of
	  the 128 memory mapped lcoation for a particular XGA instance is
	  Segment:(1C00h+instance*80h) for each XGA installed in a system
	  (default instance is 6).  The instance number may be read from the
	  XGA's Programmable Option Select registers
	The XGA/A (PS/2 adapter) uses the 7KB area below the memory-mapped
	  register area for ROM data; the XGA (PS/2 onboard) has included
	  this area in it's video BIOS ROM.
	Most of the memory mapped registers are from the graphics coprocessor,
	  while the I/O-registers are for the display controller.
--------V-MC0007FF8--------------------------
MEM C000h:7FF8h - Matrox MGA Video Adapters - CARD VENDOR ID
Size:	WORD
Desc:	contains the PCI vendor ID for the card vendor; this is written into
	  the video controllers PCI subsystem-vendor-ID field
SeeAlso: MEM C000h:7FFAh,MEM C000h:7FFCh
--------V-MC0007FFA--------------------------
MEM C000h:7FFAh - Matrox MGA Video Adapters - HARDWARE REVISION ID
Size:	BYTE
SeeAlso: MEM C000h:7FF8h,MEM C000h:7FFCh
--------V-MC0007FFC--------------------------
MEM C000h:7FFCh - Matrox MGA Video Adapters - OFFSET OF PINS DATA STRUCTURE
Size:	WORD
SeeAlso: INT 10/AX=4F14h"Matrox",#00126,MEM C000h:7FF8h
--------A-MF0006000--------------------------
MEM F000h:6000h - IBM PC ROM BASIC
Size:	32768 BYTEs
--------B-MF000E000--------------------------
MEM F000h:E000h - ORIGINAL IBM PC ROM BIOS
Size:	8192 BYTEs
--------H-MF000FFF0--------------------------
MEM F000h:FFF0h - RESET JUMP
Size:	5 BYTEs
--------B-MF000FFF5--------------------------
MEM F000h:FFF5h - ASCII BIOS DATE
Size:	8 BYTEs
--------B-MF000FFFD--------------------------
MEM F000h:FFFDh - OFTEN USED TO ENSURE CORRECT BIOS CHECKSUM
Size:	BYTE
--------B-MF000FFFE--------------------------
MEM F000h:FFFEh - MACHINE TYPE CODE
Size:	BYTE
SeeAlso: INT 15/AH=C0h
--------X-MF000xxx0--------------------------
MEM F000h:xxx0h - PCI IRQ Routing Table Specification v1.0
Size:	N paragraphs (N >= 2)
InstallCheck: scan for the signature string "$PIR" followed by a valid
	  PCI IRQ Routing Table
Range:	any paragraph boundary within the range F0000h to FFFFFh

Format of PCI IRQ Routing Table v1.0:
Offset	Size	Description	(Table M0090)
 00h  4 BYTEs	signature "$PIR"
 04h	WORD	version (0100h for v1.0)
 06h	WORD	table size in bytes
 08h	BYTE	bus number for PCI Interrupt Router
 09h	BYTE	device/function number for PCI Interrupt Router
 0Ah	WORD	bitmap of PCI-exclusive IRQs (bit 0 = IRQ0, etc.)
 0Ch	WORD	PCI vendor ID for compatible PCI Interrupt Router
 0Eh	WORD	PCI device ID for compatible PCI Interrupt Router
 10h	DWORD	Miniport data
 14h 11 BYTEs	reserved (0)
 1Fh	BYTE	checksum (set to make 8-bit sum of bytes in entire structure
		  equal 00h)
--- optional data ---
 20h 16 BYTEs	first slot entry (see #M0091)
	...
     16 BYTEs	Nth slot entry

Format of PCI IRQ Routing Table slot entry:
Offset	Size	Description	(Table M0091)
 00h	BYTE	PCI bus number
 01h	BYTE	PCI device number (bits 7-3)
 02h	BYTE	link value for INTA#
 03h	WORD	IRQ bitmap for INTA#
 05h	BYTE	link value for INTB#
 06h	WORD	IRQ bitmap for INTB#
 08h	BYTE	link value for INTC#
 09h	WORD	IRQ bitmap for INTC#
 0Bh	BYTE	link value for INTD#
 0Ch	WORD	IRQ bitmap for INTD#
 0Eh	BYTE	slot number (00h = motherboard, other = vendor-specific)
 0Fh	BYTE	reserved
SeeAlso: #M0090,#01260 at INT 1A/AX=B406h
--------B-MF000xxxx--------------------------
MEM F000h:xxxxh - AWARD Flash Hook

Format of AWARD Flash BIOS interface:
Offset	Size	Description	(Table M0092)
 00h  8 BYTEs	signature "AWDFLASH"
 08h	WORD	offset in F000h of FAR function: Get ???
		Return: BL = ??? (00h)
 0Ah	WORD	offset in F000h of FAR function: ???
 0Ch	WORD	offset in F000h of FAR function: ???
 0Eh	WORD	offset in F000h of FAR function: ???
 10h	WORD	offset in F000h of FAR function: ???
 12h	WORD	offset in F000h of FAR function: Disable Shadowing
 14h	WORD	offset in F000h of FAR function: Enable Shadowing
 16h	WORD	offset in F000h of FAR function: Get ???
		Return: DS:SI -> ??? (30 bytes?)
 18h	WORD	offset in F000h of FAR function: Set ???
		DS:SI -> ??? (appears to be same as previous function)
Note:	the AWDFLASH utility copies the ROM from F000h and uses the copy
	  instead of the original F000h:xxxxh addresses
--------B-MF000xxxx--------------------------
MEM F000h:xxxxh - Asustek Flash Hook

Format of Asustek Flash interface:
Offset	Size	Description	(Table M0093)
 00h 10 BYTEs	signature "ASUS_FLASH"
 0Ah  6 BYTEs	blanks (padding)
 10h	WORD	interface version??? (current PFLASH.EXE requires 0101h)
 12h	DWORD	-> position-independent code to enable shadowing
 16h	WORD	size of code pointed at by previous field (<= 0400h)
 18h	DWORD	-> position-independent code to disable shadowing
 1Ch	WORD	size of code pointed at by previous field (<= 0400h)
--------p-Mxxxxxxx0--------------------------
MEM xxxxh:xxx0h - Advanced Configuration and Power Interface Spec (ACPI) v0.9+
Range: any paragraph boundary in the first kilobyte of the XBDA, the last
	kilobyte of conventional memory, or from E000h:0000h to F000h:FFE0h
Note:	scan paragraph boundaries for the signature string "RSD PTR ", followed
	  by a valid Root System Description Pointer structure (see #M0094)
SeeAlso: INT 15/AX=E820h
!!!acpi\acpi10.pdf p.194

Format of ACPI Root System Description Pointer structure:
Offset	Size	Description	(Table M0094)
 00h  8 BYTEs	signature "RSD PTR "
 08h	BYTE	checksum (entire structure, including this byte, must
		  add up to zero)
 09h  6 BYTEs	OEM identifier
 0Fh	BYTE	reserved (0)
 10h	DWORD	physical address of Root System Description Table (see #M0096)
SeeAlso: #M0096

Format of ACPI System Description Table header:
Offset	Size	Description	(Table M0095)
 00h  4 BYTEs	signature
 04h	DWORD	length of table in bytes, including this header
 08h	BYTE	revision of specification corresponding to signature
		01h for both v0.9 and v1.0
 09h	BYTE	checksum (set such that entire table sums to 00h)
 0Ah  6 BYTEs	OEM identification
 10h  8 BYTEs	OEM table identifier
 18h  4 BYTEs	OEM revision number
---ACPI v1.0---
 1Ch  4 BYTEs	vendor ID for table-creation utility used
 20h  4 BYTEs	revision of table-creation utility
SeeAlso: #M0094,#M0096,#M0099,#M0097,#M0100,#M0105,#M0108,#M0110

Format of ACPI Root System Description Table:
Offset	Size	Description	(Table M0096)
 00h 36 BYTEs	System Description Table Header (see #M0095)
		signature "RSDT"
 24h  N DWORDs	physical addresses of other description tables
		(see #M0099,#M0097,#M0100,#M0105,#M0108,#M0109)
Notes:	the number of table pointers is implied by the table length
	  field in the header (at offset 04h)
	for ACPI v0.9, the header is eight bytes smaller and thus all
	  following offsets are 8 less
SeeAlso: #M0094

Format of ACPI Fixed ACPI Description Table:
Offset	Size	Description	(Table M0097)
 00h 36 BYTEs	System Description Table Header (see #M0095)
		signature "FACP"
 24h	DWORD	physical address of the Firmware ACPI Control Structure
		  (see #M0105)
 28h	DWORD	physical address of the Differentiated System Description Table
		  (see #M0099)
 2Ch	BYTE	interrupt mode
		00h dual PIC (industry-standard AT-type)
		01h multiple APIC (see #M0100)
		else reserved
 2Dh	BYTE	reserved
 2Eh	WORD	system vector of SCI interrupt
 30h	DWORD	I/O port address of SMI command port
 34h	BYTE	value to write to SMI comamnd port to disable SMI ownership
		  of ACPI hardware registers
 35h	BYTE	value to write to SMI comamnd port to re-enable SMI ownership
		  of ACPI hardware registers
 36h	BYTE	(v1.0) value to write to SMI command port to enter S4BIOS state
		00h if not supported
 37h	BYTE	reserved
 38h	DWORD	I/O port address of Power Management 1a Event Register Block
 3Ch	DWORD	I/O port address of Power Management 1b Event Register Block
		(optional, 00000000h if not supported)
 40h	DWORD	I/O port address of Power Management 1a Control Register Block
 44h	DWORD	I/O port address of Power Management 1b Control Register Block
		(optional, 00000000h if not supported)
 48h	DWORD	I/O port address of Power Management 2 Control Register Block
		(optional, 00000000h if not supported)
 4Ch	DWORD	I/O port address of Power Management Timer Control Reg. Block
 50h	DWORD	I/O port address of Generic Purpose Event 0 Register Block
		(optional, 00000000h if not supported)
 54h	DWORD	I/O port address of Generic Purpose Event 1 Register Block
		(optional, 00000000h if not supported)
 58h	BYTE	size of Power Management 1a/1b Event Register Block (>= 4)
 59h	BYTE	size of Power Management 1a/1b Control Register Block (>= 1)
 5Ah	BYTE	size of Power Management 2 Control Register Block (>= 1)
 5Bh	BYTE	size of Power Management Timer Control Register Block (>= 4)
 5Ch	BYTE	size of Generic Purpose Event 0 Register Block (multiple of 2)
 5Dh	BYTE	size of Generic Purpose Event 1 Register Block (multiple of 2)
 5Eh	BYTE	offset within General Purpose Event model for GPE1-based events
 5Fh	BYTE	reserved
 60h	WORD	worst-case hardware latency (microseconds) for entering/leaving
		  state C2; >100 if C2 not supported
 62h	WORD	worst-case hardware latency (microseconds) for entering/leaving
		  state C3; >1000 if C3 not supported
 64h	WORD	size of contiguous cacheable memory which must be read to flush
		  all dirty lines from a processor's memory cache; use if
		  fixed feature flag WBINVD (see #M0098) is clear
		0000h if flushing not supported
 66h	WORD	memory stride size (in bytes) to flush processor's memory cache
 68h	BYTE	bit index of processor's duty cycle setting within the
		  processor's P_CNT register
 69h	BYTE	size of processor's duty cycle setting in bits
 6Ah	BYTE	index within RTC CMOS RAM of the day-of-month alarm value
		00h = not supported
 6Bh	BYTE	index within RTC CMOS RAM of the month-of-year alarm value
		00h = not supported
 6Ch	BYTE	index within RTC CMOS RAM of the century alarm value
		00h = not supported
 6Dh	BYTE	reserved
 6Eh	DWORD	fixed feature flags (see #M0098)
SeeAlso: #M0094,CMOS 7Dh,CMOS 7Eh,CMOS 7Fh

Bitfields for ACPI Fixed Feature Flags:
Bit(s)	Description	(Table M0098)
 0	WBINVD instruction is correctly supported by processor
 1	WBINVD instruction flushes all caches and maintains coherency, but
	  does not guarantee invalidation of all caches
 2	all processors support C1 sleep state
 3	C2 sleep state is configured to work on multiprocessor system
---v0.9---
 4	power button is handled as a generic feature
 5	RTC wake-up state is not supported in fixed register space
 6	TMR_VAL size
	=0 24 bits
	=1 32 bits
 7-31	reserved
---v1.0---
 4	power button is handled as a control method device
 5	=0 sleep button is handled as a fixed feature programming mode
	=1 control method device, or no sleep button
 6	RTC wake-up state is not supported in fixed register space
 7	RTc alarm can wake system from S4 state
 8	TMR_VAL size
	=0 24 bits
	=1 32 bits
 9-31	reserved
SeeAlso: #M0097

Format of ACPI Differentiated System Description Table:
Offset	Size	Description	(Table M0099)
 00h 36 BYTEs	System Description Table Header (see #M0095)
		signature "DSDT"
 24h		complex byte stream; refer to ACPI document and software
SeeAlso: #M0094

Format of ACPI Multiple APIC Description Table:
Offset	Size	Description	(Table M0100)
 00h 36 BYTEs	System Description Table Header (see #M0095)
		signature "APIC"
 24h	DWORD	physical address of the local APIC in each processor's address
		  space
 28h	DWORD	multiple-APIC flags (see #M0101)
 2Ch 12N BYTEs	APIC structures (see #M0102,#M0104)
		first byte of each is type, second is length; types other than
		  00h and 01h are currently reserved and should be skipped
SeeAlso: #M0094

Bitfields for ACPI Multiple APIC Description Table flags:
Bit(s)	Description	(Table M0101)
 0	system contains AT-compatible dual 8259 interrupt controllers in
	  addition to APICs
 1-31	reserved (0)
SeeAlso: #M0100

Format of ACPI Local APIC Structure:
Offset	Size	Description	(Table M0102)
 00h	BYTE	structure type (00h = Processor Local APIC)
 01h	BYTE	length of this structure (0Ch for v0.9, 08h for v1.0)
 02h	BYTE	processor ID
 03h	BYTE	processor's local APIC ID
---v0.9---
 04h	DWORD	physical address of APIC
 08h	DWORD	flags (TBD)
--v1.0---
 04h	DWORD	flags (see #M0103)
SeeAlso: #M0100,#M0104

Bitfields for ACPI Local APIC flags:
Bit(s)	Description	(Table M0103)
 0	APIC enabled
 1-31	reserved (0)
SeeAlso: #M0102

Format of ACPI I/O APIC Structure:
Offset	Size	Description	(Table M0104)
 00h	BYTE	structure type (00h = Processor Local APIC)
 01h	BYTE	0Ch (length of this structure)
 02h	BYTE	I/O APIC's ID
 03h	BYTE	reserved (0)
 04h	DWORD	physical address of the APIC
 08h	DWORD	number of first system interrupt vector for APIC
SeeAlso: #M0100,#M0102

Format of ACPI Firmware ACPI Control Structure:
Offset	Size	Description	(Table M0105)
 00h  4 BYTEs	signature "FACS"
 04h	DWORD	length of entire structure in bytes (>= 40h)
 08h	DWORD	value of system's hardware signature at last boot
 0Ch	DWORD	real-mode ACPI OS waking vector
		if nonzero, control is transferred to this address on next BIOS
		  POST
 10h	DWORD	global lock (see #M0107)
 14h	DWORD	(v1.0) firmware control structure flags (see #M0106)
 18h 44 BYTEs	reserved (0)
Notes:	this structure is located on a 64-byte boundary anywhere in the
	  first 4GB of memory
	the BIOS is required to omit the address space containing this
	  structure from system memory in the system's memory map
SeeAlso: #M0094,INT 15/AX=E820h

Bitfields for ACPI Firmware Control Structure Feature flags:
Bit(s)	Description	(Table M0106)
 0	system supports S4BIOS_REQ
	=0 operating system must save/restore memory state in order to go to S4
 1-31	reserved (0)
SeeAlso: #M0105

Bitfields for ACPI Embedded Controller Arbitration Structure:
Bit(s)	Description	(Table M0107)
 0	request for Global Lock ownership is pending
 1	Global Lock is currently owned
 2-31	reserved
SeeAlso: #M0105

Format of ACPI Persistent System Description Table:
Offset	Size	Description	(Table M0108)
 00h 36 BYTEs	System Description Table Header (see #M0095)
		signature "PSDT"
 24h		complex byte stream; refer to ACPI document and software
SeeAlso: #M0094

Format of ACPI Secondary System Description Table:
Offset	Size	Description	(Table M0109)
 00h 36 BYTEs	System Description Table Header (see #M0095)
		signature "SSDT"
 24h		complex byte stream; refer to ACPI document and software
SeeAlso: #M0094

Format of ACPI Smart Battery Description Table:
Offset	Size	Description	(Table M0110)
 00h 36 BYTEs	System Description Table Header (see #M0095)
		signature "SBST"
 24h	DWORD	energy level in mWh at which system should warn user
 28h	DWORD	energy level in mWh at which system should automatically enter
		  sleep state
 2Ch	DWORD	energy level in mWh at which system should perform an emergency
		  shutdown
SeeAlso: #M0094
----------Mxxxxxxx0---------------------------
MEM xxxxh:xxx0h - BIOS32 Service Directory
InstallCheck:	scan paragraph boundaries E000h to FFFFh for signature string
	"_32_", followed by a valid header structure (see #F0021)
SeeAlso: CALL xxxxh:xxxxh"BIOS32"
----------Mxxxxxxx0---------------------------
MEM xxxxh:xxx0h - Desktop Management Interface / System Management BIOS
InstallCheck:	scan paragraph boundaries F000h to FFFFh for signature string
	   "_DMI_", followed by a valid header structure (see #M0111,#M0112)

Format of Desktop Management Interface entry-point structure:
Offset	Size	Description	(Table M0111)
 00h  5 BYTEs	signature "_DMI_"
 05h	BYTE	checksum of this structure (forces 8-bit sum of bytes to 00h)
 06h	WORD	total length of SMBIOS structure table, in bytes
 08h	DWORD	32-bit physical address of read-only SMBIOS structure table
		(see #F0059)
 0Ch	WORD	number of SMBIOS structures
 0Eh	BYTE	BCD SMBIOS revision (high nybble = major, low = minor)
!!!ftp://download.intel.com/ial/wfm/smbios.pdf
SeeAlso: #M0112

Format of System Management BIOS entry-point structure:
Offset	Size	Description	(Table M0112)
 00h  4 BYTEs	signature "_SM_"
 04h	BYTE	checksum of this structure (forces 8-bit sum of bytes to 00h)
 05h	BYTE	length of structure in bytes (1Fh for v2.1+)
 06h	BYTE	major version of specification
 07h	BYTE	minor version of specification (01h = vX.1, 16h = vX.22)
 08h	WORD	size of largest SMBIOS structure (see also #F0046)
 0Ah	BYTE	revision of this data structure
		00h SMBIOS v2.1-2.3
		01h-FFh reserved for future versions
 0Bh  5 BYTEs	revision-specific data (currently unused)
 10h  5 BYTEs	intermediate anchor string "_DMI_"
 15h	BYTE	checksum of intermediate entry-point structure
		(forces 8-bit sum of bytes 10h-1Eh to 00h)
 16h	WORD	total length of SMBIOS structure table, in bytes
 18h	DWORD	32-bit physical address of read-only SMBIOS structure table
		(see #F0059)
 1Ch	WORD	number of SMBIOS structures
 1Eh	BYTE	BCD SMBIOS revision (high nybble = major, low = minor)
		00h if specification version only given in bytes 06h/07h
BUG:	due to an error in the v2.1 specification, some implementations might
	  indicate a length of 1Eh bytes instead of 1Fh
SeeAlso: #M0111
----------Mxxxxxxx0--------------------------
MEM xxxxh:xxx0h - Multiprocessor Specification - FLOATING POINTER STRUCTURE
InstallCheck: scan paragraph boundaries for the signature string "_MP_",
	  followed by a valid floating pointer structure (see #M0113)
Range: any paragraph boundary in the first kilobyte of the XBDA, the last
	kilobyte of conventional memory, or from F000h:0000h to F000h:FFE0h
SeeAlso: MEM FEE00000h

Format of Multiprocessor Specification Floating Pointer structure:
Offset	Size	Description	(Table M0113)
 00h  4 BYTEs	signature "_MP_"
 04h	DWORD	physical address of MP configuration table (see #M0114)
		00000000h if no configuration table
 08h	BYTE	length of this structure in paragraphs (currently 01h)
 09h	BYTE	revision of MP specification supported
		01h = v1.1
		04h = v1.4
 0Ah	BYTE	checksum (8-bit sum of entire structure, including this
		  byte, must equal 00h)
 0Bh	BYTE	MP feature byte 1: system configuration type
		00h: MP configuration table present
		nonzero: default configuration implemented by system
 0Ch	BYTE	MP feature byte 2
		bit 7: IMCR present
		bits 6-0: reserved (0)
 0Dh  3	BYTEs	MP feature bytes 3-5 (reserved, must be 00h)

Format of Multiprocessor Specification configuration table header:
Offset	Size	Description	(Table M0114)
 00h  4 BYTEs	signature "PCMP"
 04h	WORD	length of base configuration table in bytes, including
		  this header
 06h	BYTE	revision of MP specification supported
		01h = v1.1
		04h = v1.4
 07h	BYTE	checksum of entire base configuration table
 08h  8 BYTEs	OEM identifier
 10h 12 BYTEs	product ID
 1Ch	DWORD	physical address to OEM-defined configuration table
		00000000h if not present
 20h	WORD	size of base OEM table in bytes (0000h if not present)
 22h	WORD	number of entries in variable portion of base table
 24h	DWORD	address of local APIC (see also MEM FEE0h:0020h)
 28h	WORD	length of extended entries following end of base table
		  (in bytes)
 2Ah	BYTE	checksum for extended table entries (includes only
		  extended entries following base table)
 2Ch	var	configuration table entries (see #M0115)
SeeAlso: #M0113

Format of Multiprocessor Specification configuration table entries:
Offset	Size	Description	(Table M0115)
 00h	BYTE	entry type code
		00h processor
		01h bus
		02h I/O APIC
		03h I/IO interrupt assignment
		04h local interrupt assignment
		80h system address space mapping
		81h bus hierarchy descriptor
		82h compatibility bus address space modifier
---processor---
 01h	BYTE	local APIC identifier
 02h	BYTE	local APIC version
 03h	BYTE	CPU flags
		bit 0: processor usable
		bit 1: bootstrap processor
 04h	WORD	CPU type
		bits 11-8: CPU family
		bits 7-4: CPU model
		bits 3-0: stepping
		(bits 11-0 all set indicate non-Intel-compatible CPU)
 06h  2 BYTEs	unused
 08h	DWORD	feature flags (as returned by Pentium CPUID instruction)
 0Ch  8 BYTEs	reserved
---bus---
 01h	BYTE	bus ID (assigned sequentially from 00h by BIOS)
 02h  6 BYTEs	bus type (blank-padded ASCII string) (see #M0116)
---I/O APIC---
 01h	BYTE	APIC identifier
 02h	BYTE	APIC version
 03h	BYTE	I/O APIC flags
		bit 0: enabled
		bits 7-1: reserved
 04h	DWORD	base address for APIC
---I/O,local interrupt assignment---
 01h	BYTE	interrupt type
		00h vectored interrupt (from APIC)
		01h NMI
		02h system management interrupt
		03h vectored interrupt (from external PIC)
 02h	BYTE	APIC control (see #M0117)
 03h	BYTE	unused
 04h	BYTE	source bus identifier
 05h	BYTE	source bus IRQ
 06h	BYTE	destination I/O APIC identifier
 07h	BYTE	destination I/O APIC interrupt pin number
---system address space mapping---
 01h	BYTE	entry length (14h)
 02h	BYTE	bus ID
 03h	BYTE	address type (00h I/O, 01h memory, 02h prefetch)
 04h	QWORD	starting address of region visible to bus
 0Ch	QWORD	length of region visible to bus
---bus hierarchy descriptor---
 01h	BYTE	entry length (08h)
 02h	BYTE	bus ID
 03h	BYTE	bus information
		bit 0: subtractive decoding
 04h	BYTE	ID of parent bus
 05h  3 BYTEs	reserved
---compatibility bus address space modifier---
 01h	BYTE	entry length (08h)
 02h	BYTE	bus ID
 03h	BYTE	address modifier
		bit 0: remove address ranges in predefined range list from
			  bus's address space
 04h	DWORD	number indicating predefined address space range to be removed
		00h ISA-compatible I/O range (x100h-x3FFh and aliases)
		01h VGA-compatible I/O range (x3B0h-x3BBh,x3C0h-x3DFh,aliases)
SeeAlso: #M0114

(Table M0116)
Values for Multiprocessor Specification bus name:
 "CBUS"		Corollary CBus
 "CBUSII"	Corollary CBus II
 "EISA"
 "FUTURE"	IEEE FutureBus
 "INTERN"	internal bus
 "ISA"
 "MBI"		Multibus I
 "MBII"		Multibus II
 "MCA"		Microchannel
 "MPI"
 "MPSA"
 "NUBUS"	Apple Macintosh NuBus
 "PCI"
 "PCMCIA"
 "TC"		DEC TurboChannel
 "VL"		VESA Local Bus
 "VME"		VMEbus
 "XPRESS"	Express System Bus
SeeAlso: #M0115

Bitfields for Multiprocessor Specification APIC control:
Bit(s)	Description	(Table M0117)
 1-0	input signal polarity
	00 conforms to bus specification
	01 active high
	10 reserved
	11 active low
 3-2	trigger mode
	00 conforms to bus specification
	01 edge-triggered
	10 reserved
	11 level-triggered
SeeAlso: #M0115
--------H-mFEC00000--------------------------
MEM FEC00000h - Pentium - 82379AB I/O APIC - I/O REGISTER SELECT
Size:	DWORD
Desc:	bits 7-0 of the I/O Register Select memory location specify which
	  of the APIC's registers appears in the I/O Window at FExxx010h
Range:	the Multiprocessor Specification calls for I/O APICs to be memory-
	  mapped on 4K boundaries between FEC00000h and FEDFC000h; the Intel
	  82379AB I/O APIC can be memory-mapped on any 1K boundary within
	  FEC0000h-FEC0F800h
Note:	this memory-mapped register is also supported by the Intel 82093AA
	  I/O APIC
SeeAlso: MEM FEC00010h,MEM FEE00000h,MEM xxxxh:xxx0h"Multiprocessor"
--------H-mFEC00010--------------------------
MEM FEC00010h - Pentium - 82379AB I/O APIC - I/O WINDOW
Size:	DWORD
Range:	the Multiprocessor Specification calls for I/O APICs to be memory-
	  mapped on 4K boundaries between FEC00000h and FEDFC000h
Note:	this memory-mapped register is also supported by the Intel 82093AA
	  I/O APIC
SeeAlso: MEM FEC00010h

(Table M0118)
Values for Intel 82379AB/82093AA I/O APIC registers:
 00h	APIC ID
 01h	APIC version (read-only)
	bits 31-24: reserved
	bits 23-16: maximum redirection entry
	bits 15-8: reserved
	bits 7-0: APIC version (11h for 82093AA)
 02h	APIC arbitration ID (read-only)
	bits 31-28: reserved
	bits 27-24: arbitration ID
	bits 23-0: reserved
 10h-11h	redirection table entry 0 (10h=low DWORD, 11h=high DWORD)
 12h-13h	redirection table entry 1 (see !!!)
 ...
 2Eh-2Fh	redirection table entry 15
---82093AA only---
 30h-31h	redirection table entry 16
 ...
 3Eh-3Fh	redirection table entry 23

Bitfields for APIC redirection table entry:
Bit(s)	Description	(Table M0119)
 63-56	destination
!!!29056601.pdf pg. 10
 55-17	reserved
 16	interrupt mask
 15	trigger mode
 14	remote IRR (read-only)
 13	interrupt input pin polarity
 12	delivery status (read-only)
 11	destination mode
 10-8	delivery mode
 7-0	interrupt vector (10h-FEh)
--------H-mFEE00000--------------------------
MEM FEE00000h - Pentium - LOCAL APIC
Size:	4096 BYTEs
Notes:	the Advanced Programmable Interrupt Controller built into
	  multiprocessor-capable Pentiums (P54C, etc. -- basically 75MHz and
	  faster Pentiums) maps its registers into the top of the physical
	  address space on data reads and writes, but not on code reads;
	  data accesses to the APIC registers do not cause external bus
	  cycles
	the APIC's registers are only visible when the APIC is enabled (which
	  occurs at CPU reset when external data lines contain proper signals);
	  all accesses to APIC registers should use 32-bit reads or writes, as
	  8-bit and 16-bit accesses may produce unpredictable results
	the PentiumPro (P6) permits the address at which the local APIC
	  appears to be changed with Model-Specific Register 0000001Bh
SeeAlso: MEM FEC00000h,MEM FEE00020h,MEM xxxxh:xxx0h"Multiprocessor"
SeeAlso: MSR 0000001Bh
--------H-mFEE00020--------------------------
MEM FEE00020h - Pentium - LOCAL APIC - LOCAL APIC ID REGISTER
Size:	DWORD
SeeAlso: MEM FEE00030h
--------H-mFEE00030--------------------------
MEM FEE00030h - Pentium - LOCAL APIC - LOCAL APIC VERSION REGISTER
Size:	DWORD
Note:	read-only
SeeAlso: MEM FEE00020h
--------H-mFEE00040--------------------------
MEM FEE00040h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE00050--------------------------
MEM FEE00050h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE00060--------------------------
MEM FEE00060h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE00070--------------------------
MEM FEE00070h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE00080--------------------------
MEM FEE00080h - Pentium - LOCAL APIC - TASK PRIORITY REGISTER (TPR)
Size:	DWORD
--------H-mFEE00090--------------------------
MEM FEE00090h - Pentium - LOCAL APIC - ARBITRATION PRIORITY REGISTER (APR)
Size:	DWORD
Note:	read-only
--------H-mFEE000A0--------------------------
MEM FEE000A0h - Pentium - LOCAL APIC - END OF INTERRUPT REGISTER (EOI)
Size:	DWORD
Note:	write-only
--------H-mFEE000A0--------------------------
MEM FEE000A0h - Pentium - LOCAL APIC - PROCESSOR PRIORITY REGISTER (PPR)
Size:	DWORD
Note:	read-only
SeeAlso: MEM FEE00000h
--------H-mFEE000B0--------------------------
MEM FEE000B0h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE000C0--------------------------
MEM FEE000C0h - Pentium - LOCAL APIC - REMOTE READ REGISTER
Size:	DWORD
Note:	read-only
--------H-mFEE000D0--------------------------
MEM FEE000D0h - Pentium - LOCAL APIC - LOGICAL DURATION REGISTER (LDR)
Size:	DWORD
SeeAlso: MEM FEE00000h
--------H-mFEE000E0--------------------------
MEM FEE000E0h - Pentium - LOCAL APIC - DESTINATION FORMAT REGISTER (DFR)
Size:	DWORD
	bits 27-0: read-only
	bits 31-28: read-write
--------H-mFEE000F0--------------------------
MEM FEE000F0h - Pentium - LOCAL APIC - SPURIOUS INTERRUPT VECTOR REGISTER
Size:	DWORD
	bits 3-0, read-only
	bits 9-4, read/write
--------H-mFEE00100--------------------------
MEM FEE00100h - Pentium - LOCAL APIC - IN-SERVICE REGISTER (ISR)
Size:	128 BYTEs
Note:	read-only
SeeAlso: MEM FEE00200h
--------H-mFEE00180--------------------------
MEM FEE00180h - Pentium - LOCAL APIC - TRIGGER MODE REGISTER (TMR)
Size:	128 BYTEs
Note:	read-only
SeeAlso: MEM FEE00000h
--------H-mFEE00200--------------------------
MEM FEE00200h - Pentium - LOCAL APIC - INTERRUPT REQUEST REGISTER (IRR)
Size:	128 BYTEs
Note:	read-only
SeeAlso: MEM FEE00100h
--------H-mFEE00280--------------------------
MEM FEE00280h - Pentium - LOCAL APIC - ERROR STATUS REGISTER
Size:	DWORD
Note:	read-only

Bitfields for Pentium APIC error status register:
Bit(s)	Description	(Table M0120)
 0	send checksum error
 1	receive checksum error
 2	send accept error
 3	receive accept error
 4	reserved
 5	send illegal vector
 6	receive illegal vector
 7	illegal register address
 31-8	reserved
--------H-mFEE00300--------------------------
MEM FEE00300h - Pentium - LOCAL APIC - INTERRUPT COMMAND REGISTER (ICR)
Size:	DWORD
Note:	this is the low half of the 64-bit ICR
SeeAlso: MEM FEE00310h,#M0121

Bitfields for Pentium APIC Interrupt Command Register:
Bit(s)	Description	(Table M0121)
 7-0	interrupt vector number
 10-8	delivery mode (see #M0122)
 11	destination mode
 12	delivery status (read-only)
	1 = transfer pending
 13	reserved
 14	level (0 = INIT Level Deassert message, 1 = anything else)
 15	trigger mode (1)
 17-16	remote read status (read-only)
 19-18	destination shorthand
	00 as specified by destination field
	01 self
	10 all including self
	11 all except self
 55-20	reserved
 63-56	destination for interrupt request or message
SeeAlso: #M0124

(Table M0122)
Values for Pentium APIC delivery mode:
 000b	fixed
 001b	lowest-priority
 010b	SMI
 011b	remote read
 100b	NMI
 101b	INIT
 110b	start up
 111b	reserved
SeeAlso: #M0121
--------H-mFEE00310--------------------------
MEM FEE00310h - Pentium - LOCAL APIC - INTERRUPT COMMAND REGISTER (ICR)
Size:	DWORD
Note:	this is the high half of the 64-bit ICR
SeeAlso: MEM FEE00300h,#M0121
--------H-mFEE00320--------------------------
MEM FEE00320h - Pentium - LOCAL APIC - LOCAL VECTOR TABLE ENTRY 0 (TIMER)
Size:	DWORD
SeeAlso: MEM FEE00350h,MEM FEE00370h,MEM FEE003E0h,INT 70h

Bitfields for Pentium APIC timer local vector entry:
Bit(s)	Description	(Table M0123)
 7-0	interrupt vector number
 11-8	reserved
 12	delivery status (read-only)
	1 = interrupt being sent to APIC
 15-13	reserved
 16	interrupt delivery disabled
 17	timer mode (0=one-shot, 1=periodic)
 31-18	reserved
SeeAlso: #M0125,#M0124
--------H-mFEE00330--------------------------
MEM FEE00330h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE00340--------------------------
MEM FEE00340h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE00350--------------------------
MEM FEE00350h - Pentium - LOCAL APIC - LOCAL VECTOR TABLE ENTRY 1 (LINT0)
Size:	DWORD
SeeAlso: MEM FEE00320h,MEM FEE00360h

Bitfields for Pentium APIC LINTx local vector entry:
Bit(s)	Description	(Table M0124)
 7-0	interrupt vector number
 10-8	delivery mode
	000 fixed
	100 NMI
	111 external interrupt (8259A-compatibility)
 11	reserved
 12	delivery status (read-only)
	1 = interrupt being sent to APIC
 13	interrupt pin is active low
 14	remote IRR
 15	trigger mode
	0 edge-sensitive
	1 level-sensitive
 16	interrupt delivery disabled
 31-17	reserved
SeeAlso: #M0123
--------H-mFEE00360--------------------------
MEM FEE00360h - Pentium - LOCAL APIC - LOCAL VECTOR TABLE ENTRY 2 (LINT1)
Size:	DWORD
SeeAlso: MEM FEE00350h,MEM FEE00370h,#M0124
--------H-mFEE00370--------------------------
MEM FEE00370h - Pentium - LOCAL APIC - LOCAL VECTOR TABLE ENTRY 3 (Error)
Size:	DWORD
SeeAlso: MEM FEE00320h,MEM FEE00370h
--------H-mFEE00380--------------------------
MEM FEE00380h - Pentium - LOCAL APIC - INITIAL COUNT REGISTER (ICR) TIMER
Size:	DWORD
Desc:	timer start value, which together with the Divide Configuration
	  Register also determines its period when periodic mode has been
	  selected
SeeAlso: MEM FEE00000h,MEM FEE00390h
--------H-mFEE00390--------------------------
MEM FEE00390h - Pentium - LOCAL APIC - CURRENT COUNT REGISTER (CCR) TIMER
Size:	DWORD
Desc:	current timer count; when this value reaches zero, an interrupt is
	  generated
Note:	read-only
SeeAlso: MEM FEE00380h
--------H-mFEE003A0--------------------------
MEM FEE003A0h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE003B0--------------------------
MEM FEE003B0h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE003C0--------------------------
MEM FEE003C0h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE003D0--------------------------
MEM FEE003D0h - Pentium - LOCAL APIC - RESERVED
SeeAlso: MEM FEE00000h
--------H-mFEE003E0--------------------------
MEM FEE003E0h - Pentium - LOCAL APIC - TIMER DIVIDE CONFIGURATION REGISTER
Size:	DWORD
SeeAlso: MEM FEE00000h,MEM FEE00320h

Bitfields for Pentium APIC timer divide configuration:
Bit(s)	Description	(Table M0125)
 3,1,0	divisor
	000 divide by 2
	001 by 4
	010 by 8
	...
	110 by 128
	111 by 1
 2	zero (0)
 31-4	reserved
Note:	the divisor determines the timer's time base relative to the processor
	  clock
SeeAlso: #M0123
----------MFFFF0010--------------------------
MEM FFFFh:0010h - HIGH MEMORY AREA (HMA)
Size:	65520 BYTEs
--------!---CONTRIBUTORS---------------------
Robin Walker	<rdhw@cus.cam.ac.uk> ORIGINAL FILE
Wim Osterholt	<wim@djo.wtm.tudelft.nl> or Wim Osterholt 2:512/56
	EHD floppy = 'KEGAN 4.0M Floppy Drive Controller.',
		     'ACME FX4-K7tb2 v:2.5 11/5/91'
Stanley Appel	<appel@stack.urc.tue.nl>
Matthias Paul	<mpaul@ibh.rwth-aachen.de>
--------!---Admin----------------------------
Highest Table Number = M0125
--------!---FILELIST-------------------------
Please redistribute all of the files comprising the interrupt list (listed at
the beginning of the list and in INTERRUP.1ST) unmodified as a group, in a
quartet of archives named INTER60A through INTER60D (preferably the original
authenticated PKZIP archives), and the utility and hypertext programs in
three additional archives called INTER60E.ZIP to INTER60G.ZIP.

Copyright (c) 1989,1990,1991,1992,1993,1994,1995,1996,1997,1998,1999 Ralf Brown
--------!---CONTACT_INFO---------------------
Internet: ralf@pobox.com (currently forwards to ralf@telerama.lm.com)
FIDO: Ralf Brown 1:129/26.1
